

**ADDENDA NUMBER (1)**

**April 19, 2017**

**ITB # 2017-04-005**

**DESIGN/BUILD WATER STORAGE TANK**

**Pre-Con Questions and Answers April 18, 2017**

**This amendment is issued as a result of questions and answers which were received in response to the above referenced ITB Pre-Proposal Conference held on 4/18/2017.**

**Notice of change in web site: Sierra County recently update their hosting domain for RFPs ITBs and RFQs to** [**http://www.sierraco.org**](http://www.sierraco.org) **– Vendor Registry Link.**

**CLARIFICATIONS:**

* Hydrant will require a 6 inch tie pipe to water tank
* Hydrant is to be a minimum of 50 to a maximum of 75 Feet from water tank.
* Hydrant Steamer (4 ½) should be facing the building
* Water for tank is from a domestic well located behind the building
* Preferred staging area is marked with stakes
* Well should be able to be filled from a bottom connector with a minimum 2’ Inch Stub Out
* If dirt work is required for the slab it may have to be hauled in- Note: some dirt work may be required to deter potential water build up for slab
* When tank is complete Fire Department will provide water for testing
* Geo Tech Report will be provided- density test will be required
* **END**