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SIERRA COUNTY
STATE OF NEW MEXICO


INVITATION TO BID

AUTOMOTIVE AMBULANCE
FOR EMS SERVICES
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ITB # 2016-11-004

SIERRA COUNTY PROCUREMENT
		855 VAN PATTEN
TRUTH OR CONSEQUENCES, NM  87901

 				Issue Date:  November 16, 2016
	               Question Deadline: November 29, 2016 @ 2:00 PM MDT
                                   Due Date:  December 8, 2016 @ 2:00 PM MDT
PUBLIC OPENING 




OTHER INFORMATION: 
COMMODITY CODE REF: 07003- Ambulance
Freight Terms: FOB Destination 
Payment Terms: NET 30

INVITATION:
Sierra County (hereinafter called County) invites you to submit a Bid for the material(s) and/or services identified and described within this Invitation To Bid (ITB).  Please read carefully all instructions, specifications, and requirements, scope of work, terms and conditions. Failure to comply with the instructions, terms and conditions and specifications of this Bid may result in your Bid being classified as unresponsive and disqualified. Bids must be submitted to the delivery location and mailing address indicated below no later than the time and date specified above. New Mexico criminal law prohibits bribes, gratuities and kickbacks. 

BID SUBMITTAL: 
All information must be entered in ink or typed and corrections must be initialed. Bidders are required to submit four (4) printed and one (1) electronic copies of their Bid.   Bids are to be submitted in a sealed envelope or package, clearly marked with the Invitation To Bid Number and Opening Date (see Bid Due By date above) in the lower left hand Corner.  Failure to mark your sealed Bid Submission Envelope or package may result in your Bid being opened early or your Bid not being included in the Invitation To Bid Opening.  

SUBMITTAL LOCATION:
Delivery Location address:
Sierra County
Attn: Jocelyn Holguin, Chief Procurement Officer
855 Van Patten
Truth or Consequences, NM  87901

Mailing Address:
Sierra County
Attn: Jocelyn Holguin, Chief Procurement Officer
855 Van Patten
Truth or Consequences, NM  87901

SIERRA COUNTY CONTACT INFORMATION:
Jocelyn Holguin, CPO
Telephone: 575-894-6215		E-mail: sierracountyprocurement@gmail.com	

APPENDIX:
A-- BID SIGNATORY FORM
B -- ACKNOWLEDGEMENT OF RECEIPT FORM
C – ACKNOWLEDGEMENT OF ADDENDA
D – CONFLICT OF INTEREST/DEBARMENT CERTIFICATION FORM
E – CAMPAIGN CONTRIBUTION DISLOSURE FORM
F -- VETERAN LOCAL PREFERENCE 
G – LOCAL PREFERENCE CERTIFICATE

EXHIBITS: 
A – QUESTION SUBMITTAL FORM
B – INSURANCE REQUIREMENTS
C – SAMPLE CONTRACT

I. INSTRUCTIONS TO BIDDERS

1. SUBMISSION OF BID: BIDS MUST BE RECEIVED FOR REVIEW AND EVALUATION BY THE CHIEF PROCUREMENT OFFICER OR DESIGNEE NO LATER THAN THE DATE INDICATED IN THE COVER SHEET. BIDS RECEIVED AFTER THIS DEADLINE FOR ANY REASON WILL NOT BE ACCEPTED OR CONSIDERED. The date and time of receipt will be recorded on each Bid. Bids must be addressed and delivered to the Chief Procurement Officer or her designee at the delivery address listed. Bids must be sealed and labeled on the outside of the package to clearly indicate that they are in response to the “AUTOMOTIVE AMBULANCE” and should reference “ITB# 2016-11-004”. Bids submitted by facsimile or other electronic means WILL NOT BE ACCEPTED. A public log will be kept of the names of all Bidders submitting Bids. Pursuant to Section 13-1-116 NMSA 1978, the contents of any Bid shall not be disclosed to competing Bidders prior to contract award.

2. ACKNOWLEDGEMENT OF ADDENDA:  Bidders shall acknowledge receipt of any addenda of this ITB by identifying the addendums number and date in the space provided on the Bid form. 

3. ALTERNATE BIDS:  Alternate Bids will be accepted and considered provided they are “equal to” and meet all specifications of this ITB which may include all specifications of the Brand used to identify the quality of the goods and/or services requested. The County reserves the right to make the final determination as to whether or not an alternate Bid is equal. It is the Bidder’s responsibility to provide, as part of the Bid, descriptive literature, specifications and information on all alternate products and services Bid. References of current users should be included. If the item(s) or service(s) Bid are not clearly identified as alternate item(s) or services, it is understood that the Bid is for item(s) and service exactly as specified in this ITB. 

4. AWARD INFORMATION:  Award information will be posted electronically on the County’s Procurement Department web site: http://www.sierraco.org

Please visit the Sierra County website:  http://www.sierraco.org- PROCURMENT- FREE VENDOR REGISTRY LINK- For the opportunity to fill out and submit the Sierra County Vendor Registry form, which will allow you notifications of all addenda’s and future projects. NOTE: You will be required to be a registered vendor in Vendor Registry to see any updates. 

5. [bookmark: _Toc276819787][bookmark: _Toc276820866]MANDITORY SITE VISIT AND PRE-BID CONFERENCE: NONE

6. [bookmark: _Toc276819788][bookmark: _Toc276820867]DEADLINE TO SUBMIT WRITTEN QUESTIONS: Potential Bidders may submit written questions as to the intent or clarity of this ITB until 2:00 PM MST on or before November 29, 2016 all written questions must be sent by e-mail to the Chief Procurement Officer or designated Representative Jocelyn Holguin, Chief Procurement Officer, sierracountyprocurement@sierraco.org 

7. [bookmark: _Toc276819789][bookmark: _Toc276820868]RESPONSE TO WRITTEN QUESTIONS/ITB AMENDMENTS: Written responses to written questions and any ITB amendments will be posted to the County Procurement Office web site link: http://www.sierraco.org-  See All Active RFP’s, ITB’s, RFQ’s Link located in Vendor Registry. Vendors must be registered in Vendor Registry for updates, changes and notifications. It is a free service to all prospective vendors. 

8. CANCELLATION:  The County reserves the right to cancel without penalty, this ITB, any resultant Purchase Order/Agreement, or any portion thereof for convenience, unsatisfactory performance, or unavailability of funds. 

9. CASH DISCOUNTS: The County will take advantage of cash discounts bid whenever possible; however, cash discounts will not be used as a means to determine the lowest cost. 

10. CLARIFICATIONS:  Any clarification of instructions, terms and conditions, insurance, bonds, or Bid preparation shall be made only by the CPO stated on the cover sheet of this ITB. Technical clarifications should be addressed to the individual identified on the cover sheet. Clarifications must be in writing and submitted as an addendum to be considered and relied upon as a part of this ITB solicitation. 

11. COPIES OF BID:  If submitting by hard copy or on CD, please submit the number of hard/CD copies of your Bid as stated on the cover sheet along with all supporting documents. Bids submitted on a CD must be in PDF format. 

12. LATE SUBMISSIONS: Late submissions of Bids will not be accepted or considered unless it is determined by County that the late receipt was due solely to mishandling by the County or the Bid is the only Bid received. Late submissions will be returned unopened. 

13. MODIFICATIONS:  Only modifications received prior to the date and time specified for the closing will be accepted. No modifications will be accepted after the opening. Technical clarifications of the Bid may be requested by the Procurement Officer or his designee following the opening. 

14. BID CLARIFICATION:  The Bids are to include with their Bid a local or toll-free number and e-mail address for Bid clarifications. Failure to do so may result in the bid being deemed non-responsive. 

15. PERIOD FOR BID ACCEPTANCE:  Bidder agrees that any Bid submitted will be good for a period of ninety (90) calendar days; an additional time period may be requested in the ITB Scope of Work. 

16. PUBLIC INFORMATION:  All information, except that classified as confidential, will become public information at the time that the ITB is awarded. Confidential information must be marked “CONFIDENTIAL” in red letters in the upper right hand corner of the pages containing the confidential information. Price and information concerning the specifications cannot be considered confidential.

17. REJECTION OF BIDS:  The County reserves the right to make an award based on the evaluation criteria contained herein, to reject any and all Bids or any part thereof, and to accept the Bid that is in the best interest of the County.

18. SUBMISSIONS OF DRAWINGS/LITERATURE:  The submission of samples, drawings and literature to be used in the evaluation of the Bid, must be submitted by the designated closing date and time in order to be considered. All submissions shall be made at no expense to the County. Returns shall only be made at the Bidder’s request and expense. Submissions provided on a CD shall be in PDF format. 


19. TAXES:  The County is exempt from Federal Excise Taxes and from New Mexico Gross Receipts Taxes on materials. Services are not exempt. Taxes on services should be included as a separate line item and not included in the base price Bid. Applicable taxes are excluded from the ITB evaluation. A non-taxable transaction certificate can be made available by the County to the awarded firm. 

20. WITHDRAWAL OF BIDS:  Bids may be withdrawn by written notice, electronically (email) or in person by a Bidder or an authorized representative at any time prior to the submittal due date and time. Bids requiring bid security will result in forfeiture of the bid security if the Bid is withdrawn following the opening.

21. ACCEPTANCE OF CONDITIONS GOVERNING THE PROCUREMENT:  Bidders must indicate their acceptance of the Conditions Governing the Procurement in the letter of transmittal form (see Appendix B). Submission of an Bid constitutes acceptance of the Evaluation Factors contained in Section II of this ITB.

22. INCURRING COST:  Any cost incurred by the Bidder in preparation, transmittal, presentation of any Bid or material or negotiation associated with their response to this ITB shall be borne solely by the Bidder.

23. PRIME CONTRACTOR RESPONSIBILITY:  Any contract that may result from this ITB shall specify that the prime contractor is solely responsible for fulfillment of the contract with the County. The County will only make contract payments to the prime contractor.
 
24. SUBCONTRACTORS:  Use of subcontractors must be clearly explained in the Bid and each must be identified by name. The prime contractor shall be wholly responsible for contract performance whether or not subcontractors are used. Substitution of subcontractors, after contract award, must receive prior written approval of the County Purchasing Office.

25. AMENDED BIDS:  An Bidder may submit an amended Bid before the deadline for receipt of Bids. Such amended Bids must be complete replacements for a previously submitted Bid and must be clearly identified as such in the transmittal letter. County personnel will not merge, collate, or assemble Bid materials.

26. BIDDERS RIGHT TO WITHDRAW BID:  Bidders will be allowed to withdraw their Bid at any time prior to the deadline for receipt of Bids. The Bidder must submit a written withdrawal request signed by the Bidder's duly authorized representative addressed to the Chief Procurement Officer or his designee. The approval or denial of withdrawal requests received after the deadline for receipt of the Bids is governed by the applicable procurement regulations.

27. FIRM BID:  Responses to this ITB, including Bid prices, will be considered firm for ninety (90) days after the due date for receipt of Bids or sixty (60) days after the due date for the receipt of a best and final Bid, if one is solicited.

28. DISCLOSURE OF BID CONTENTS:  All Bids and documents pertaining to an ITB will be open to the public, except for material which is proprietary or confidential. The Chief Procurement Officer or his designee will not disclose or make public any pages of a Bid on which the Bidder has stamped or imprinted "proprietary" or "confidential" subject to the following requirements. 

	Proprietary or confidential data shall be readily separable from the Bid in order to facilitate eventual public inspection of the remaining portions of the Bid. Confidential data is normally restricted to confidential financial information concerning the Bidder's organization and data that qualifies as a trade secret in accordance with the Uniform Trade Secrets Act, 57-3A-I to 57-3A-7 NMSA 1978. The price of products bid or the cost of services proposed shall not be designated as proprietary or confidential information.

If a request is received for disclosure of data for which a Bidder has made a written request for confidentiality, the Purchasing Agent shall examine the Bidder's request and make a written determination that specifies which portions of the bid should be disclosed. Unless the Bidder takes legal action to prevent the disclosure, the bid will be so disclosed. The bid shall be open to public inspection subject to any continued prohibition on the disclosure of confidential data.

29. NO OBLIGATION:  This procurement in no manner obligates Sierra County or any of its departments or other subdivisions to the eventual lease, purchase, etc., of any tangible personal property bid or services proposed until a valid written contract is approved by the Purchasing Agent and other required approval authorities.

30. TERMINATION:  This ITB may be canceled at any time and any and all bids may be rejected in whole or in part when the County determines such action to be in the best interest of the County.

31. SUFFICIENT APPROPRIATION:  Any contract awarded as a result of this ITB process may be terminated if sufficient appropriations or authorizations do not exist. Such termination will be effected by sending written notice to the contractor. The County's decision as to whether sufficient appropriations and authorizations are available will be accepted by the contractor as final.

32. LEGAL REVIEW:  The County requires that all Bidders agree to be bound by the General Requirements contained in this ITB.  Any Bidder concerns must be promptly brought to the attention of the Chief Procurement Officer or his designee.

33. GOVERNING LAW:  This procurement and any agreement with a successful Bidder shall be governed by the laws of the State of New Mexico.

34. BASIS FOR BID:  Only information supplied by the County in writing through the Chief Procurement Officer to his designee or in this ITB should be used as the basis for the preparation of bids.

35. BIDDER QUALIFICATIONS:  The Evaluation Committee may make such investigations as necessary to determine the ability of the Bidder to adhere to the requirements specified within this ITB. The Evaluation Committee will reject the bid of any Bidder who is not a responsible Bidder or fails to submit a responsive Bid as defined in Sections 13-1-83 and 13-1-85 NMSA 1978.

36. RIGHT TO WAIVE MINOR IRREGULARITIES:  The Evaluation Committee reserves the right to waive minor irregularities. The Evaluation Committee also reserves the right to waive mandatory requirements provided that all of the otherwise responsive bids failed to meet the same mandatory requirements or doing so does not otherwise materially affect the procurement. This right is at the sole discretion of the Evaluation Committee.

37. CHANGE IN CONTRACTOR REPRESENTATIVES:  The County reserves the right to require a change in contractor representatives if the assigned representatives are not, in the opinion of the County, meeting its needs adequately.

38. NOTICE:  The Procurement Code, Sections 13-1-28 through 13-1-199 NMSA 1978, imposes civil and misdemeanor criminal penalties for its violation. The State of New Mexico criminal statutes also impose felony penalties for bribes, gratuities and kick-backs.

39. COUNTY RIGHTS:  The County reserves the right to accept all or a portion of a Bidder's bid.


40. RIGHT TO PUBLISH:  Throughout the duration of this procurement process and contract term, potential Bidders and contractors must secure from the County written approval prior to the release of any information that pertains to the potential work or activities covered by this procurement or the subsequent contract. Failure to adhere to this requirement may result in disqualification of the Bidder’s bid or termination of the contract.

41. OWNERSHIP OF BIDS:  All documents submitted in response to the ITB shall become the property of the County. However any technical or user documentation submitted with the bid of a non-selected Bidder may be returned after the expiration of the protest period, by request, at the expense of the Bidder

42. AMBIGUITY, INCONSISTENCY OR ERRORS IN ITB:  Bidders shall promptly notify the Chief Procurement Officer or his designee, in writing, of any ambiguity, inconsistency or error which they discover upon examination of the ITB.

43. COMPETITION:  By submitting a bid, Bidder certifies that they have not, either directly or indirectly, entered into any action in restraint of full competition in connection with the Bid submitted to the County.

44. CONFIDENTIALITY:  Any confidential information provided to, or developed by, the contractor in the performance of any agreement resulting from this ITB shall be kept confidential and shall not be made available to any individual or organization by the contractor without the prior written approval of the County of Sierra.

45. ELECTRONIC MAIL ADDRESS REQUESTED:  A large part of the communication regarding this procurement will be conducted by electronic mail (e-mail). Bidders must have a valid e-mail address to receive this correspondence.



46. USE OF ELECTRONIC VERSIONS OF THIS ITB:  This ITB is being made available by electronic means. If accepted by such means, the Bidder acknowledges and accepts full responsibility to insure that no changes are made to the ITB. In the event of conflict between a version of the ITB in the Bidder’s possession and the version maintained by the County, the version maintained by the County shall govern.

47. BACKGROUND INVESTIGATIONS:  Sierra County is committed to the safety of its employees, contractors and the community it serves. To that end, any firm awarded a contract shall be required to assure that the personnel assigned to the project do not possess criminal records that would violate the standards for employment. The successful Bidder must certify that the company and its’ employees are or will be in compliance with those standards for the project awarded.

48. CANVASSING OF ELECTED MEMBERS AND COUNCIL OFFICERS: Canvassing of Elected Members or Council Officers will automatically lead to disqualification.

II. [bookmark: _Toc276819780][bookmark: _Toc276820859]DEFINITION OF TERMINOLOGY

This section contains definitions that are used throughout this procurement document, including appropriate abbreviations.

“Board of County Commissioners” (also “BCC”) means the elected board in whom all powers of the County are vested and who are responsible for the proper and efficient administration of the County government.

"Chief Procurement Officer" (also “CPO”) means the person or designee authorized by the County to manage or administer a procurement requiring the evaluation of competitive sealed Bids.

"Close of Business" means 5:00 P.M. Mountain Standard Time (MST) or Mountain Daylight Time (MDT), whichever is in effect on the date specified.

"Contract" or “Agreement” means a written agreement for the procurement of items of tangible personal property or services.

"Contractor" means a successful Bidder who enters into a binding contract.

"County" means the County of Sierra, State of New Mexico.

"Determination" means the written documentation of a decision of the Chief Procurement Officer including findings of fact required to support a decision. A determination becomes part of the procurement file to which it pertains.

“Desirable" refers to the terms "may", "can", "should", "preferably" or "prefers" which identify a desirable or discretionary item or factor (as opposed to a “mandatory” item or factor).

"Evaluation Committee" means a body appointed by County management to perform the evaluation of  Bids.

"Evaluation Committee Report" means a report prepared by the Chief Procurement Officer and the Evaluation Committee for submission to appropriate approval authorities for contract award that contains all written determinations resulting from the conduct of a procurement requiring the evaluation of competitive sealed Bids.

"Mandatory" refers to the terms "must", "shall", "will", "is required" or "are required" which identify a mandatory item or factor (as opposed to a “desirable” item or factor).  Failure to meet a mandatory item or factor will result in the rejection of the Bidder's Bid.

"Bidder" is any person, corporation, or partnership who chooses to submit a Bid.

"Page” means one (1) side of an 8 ½ X 11 inch sheet of paper. One (1) 8 ½ X 11 inch sheet of paper printed on both sides constitutes two (2) pages. (See, however, Section III.C for the one exception to the 8 ½ X 11 inch page size limitation.)

"Procuring agency of the County" means the department or other subdivision of the County of Sierra that is requesting the procurement of services or items of tangible personal property. 

"Purchase Order” or "PO" means the document which directs a contractor to deliver items of tangible personal property or services pursuant to an existing, valid contract.

"Purchasing” means the County of Sierra Purchasing Office or the Sierra County Chief Procurement Officer.

"Purchasing Agent" or "PA" means the Chief Procurement Officer for the County of Sierra.

"Invitation To Bids" or "ITB" means all documents, including those attached or incorporated by reference, used for soliciting Bids.

"Responsible Bidder" means an Bidder who submits a responsive bid and who has furnished required information and data to prove that their financial resources, production or service facilities, personnel, service reputation and experience are adequate to make satisfactory delivery of the services or items of tangible personal property called for in this solicitation.

"Responsive Bid" or "Responsive Bid" means an Bid or Bid which conforms in all material respects to the requirements set forth in the Invitation To Bid. Material respects of an Invitation To Bid include, but are not limited to, price, quality, quantity and delivery requirements.

“Statement of Compliance” and “Statement of Concurrence” mean an express, affirmative statement by the Bidder in their bid, which they agree with or agree to the stated requirement(s). Possible examples of acceptable responses include; “The [NAME HERE] Company agrees to comply with this requirement.”, “The [NAME HERE] Company concurs with this requirement.” and The [NAME HERE] Company agrees to participate as required.”


III. [bookmark: _Toc276819781][bookmark: _Toc276820860]PROCUREMENT LIBRARY

The Procurement Library consists of the following documents which may be accessed by their associated Internet links:


Sierra county Procurement Department Website
http://www.sierraco.org  Located in Vendor Registry- See All Active RFPs, ITBs, RFQs 

New Mexico Procurement Code
http://www.conwaygreene.com/nmsu/lpext.dll?f=templates&fn=main-h.htm&2.0



IV. INVITATION TO BID (ITB) STANDARD TERMS AND CONDITIONS

The purchases of materials and/or services awarded under this ITB shall be subject to the County’s “Standard Terms and Conditions” and all information and statements contained in this Invitation To Bid. The terms, conditions and specifications contained in this ITB along with any attachments and the Bidders’ response may be incorporated into any Purchase Order/ Agreement issued as a result of this ITB, including any addenda.  Any provisions in any Bid, quotation, acknowledgment or other forms or contract documents applicable to the services that are inconsistent, or in conflict, with any provisions of this ITB or the resultant contract will be ineffective and inapplicable. 

[bookmark: wp1150815][bookmark: wp1150817][bookmark: wp1150819][bookmark: wp1147509][bookmark: wp1147510][bookmark: wp1147511][bookmark: wp1147512]The deadline to encumber the money by contract with the vendor is May 1, 2017. All equipment purchased with grant funds must be inspected by the funding agency upon receipt.

Failure to meet deadlines will result in the loss of funds. Be advised that Grant recipients need the Council's written permission to make changes to their projects. Project modifications must be requested in writing, and the modification should not significantly alter the original purpose of the approved application. Extension and modification requests are reviewed on a case­ by-case basis and are not automatically granted.


V. SCOPE OF WORK

1.1 DESCRIPTION-		

Hillsboro Fire and Rescue are seeking a new or used, no earlier than 2014, Ambulance to perform necessary duties for the community. The ambulance shall be fully equipped and comply with the NFPA 1917 Standards for Automotive Ambulances 2016 Edition and KKK. 
Note:  The specifications for the approved equipment must be reviewed and approved by the funding Agency prior to encumbering any funds. The equipment to be purchased shall meet the requirements of the latest Editions of either the applicable NFPA Standards or current nationally accepted practices.

1.2 SCOPE:

COMPLETED VEHICLE DIMENSIONS- 
The vehicle described herein shall have the following approximate dimensions:
Conversion, Type I, Headroom, 72" (Standard) 
Headroom shall be 72"
Conversion, Type I, Body Width, 96" (Standard) 
Body Width shall be 96"
Conversion, Type I, Body Length, 170"_(Standard)
RUB RAILS - SKIRT
Skirt rub rails will be installed to protect the lower body and will extend the entire length of the body on the curb and street sides, exclusive of the wheel well area. They shall be made from custom 'C' channel that is cut at 45 degree angles on the ends. The rub rail shall be bolted to the lower side wall panel with 1/4" nylon spacers.
"C" channel rub rail with 45 degree ends mounted on 1/4" Nylon spacers.
The chassis listed below has been determined to best meet the needs of this agency. Bidders may offer an alternate chassis bid, but may not do so exclusive of the following specification:

F450 Super Duty Chassis Cab - 4x4 189" Wheelbase
F4H — F450 4x4 Cabin Chassis
189" Wheelbase
Z l — Oxford White
S — Interior Color Steel
99T — 6.7L OHV Power-Stroke Diesel V8 B20
47L — Ambulance Spec Emissions
98R - Manual Regeneration
X4N - 4.10 Limited Slip "Wide Track" rear axle
67A - Dual Heavy Duty Alternators
44W — Torq-Shift 6-Speed Select-Shift Automatic Overdrive
Brakes —Power 4-wheel disc/4-wheel disc anti-lock
40 Gallon Fuel Tank Aft-Axle
Battery — 750 CCA, 78-AH, dual
16,500# GVWR
41H — Engine block heater
213 — Electronic-Shift-On-The-Fly (auto-manual locking hubs & rotary control on I/P)
Axle — Mono-beam front axle w/ coil spring suspension
Bumper — front — chrome steel w/ grained MIC top cover
Fender vents — front
Grille — Chrome surround w/ medium platinum insert
Ford oval on grille
Front license plate bracket
TUB — 225/70R19.5x19.5G Traction (incl. 4 traction tires on the rear & 2 A/S tires on the front)
512 — Spare Tire & Wheels 61J — Hydraulic Jack
Manual air conditioning Glass — solar tinted
Fixed rear window
Lights — roof clearance
Halogen sealed beam headlamps 942 — Daytime Running Lamps 3-Blink Lane Change Signal Shock absorbers — heavy duty gas
Springs, rear auxiliary
Stabilizer bar — front & rear
Stationary Elevated Idle Control (SEIC)
Steering damper
Power steering
54K — Manual•telescoping trailer tow mirrors w/ power heated glass, heated convex spotter mirror & integrated
clearance lights/turn signals
Trailer tow hooks — front (2)
Wheels — 19.5" Argent painted steel
Instrument panel — color coordinated w/ glove box, (4) air registers w/ positive shutoff, power point & upfitter
switches (4)
Auxiliary power point
Perimeter anti-theft alarm & remote keyless entry
SecuriLock Anti-Theft Ignition
Dome lamp w/ dual map lights, RH/LH door activated & 1/P switch operated w/ delay

Instrumentation — multifunction switch message center w ice blue lighting (3 button message control on

steering wheel)
Power door locks w/ backlit switches
One-touch down power window
Power windows w/ backlit switches
Rearview Mirror — 11.5" day/night
AM/FM stereo w/ digital clock, single CD/MP3 player & 4 speakers
Horn — dual electric
Coat hooks, RH/LH
Dash-top tray
Grab handles, driver & front passenger
Roof ride handles, front passenger
3 — Cloth 40/20/40 Split Bench, manual lumbar support on driver's side
Steering Wheel — black vinyl, cruise control, telescoping steering wheel/column
Windshield wipers — interval control
Scuff plates — color coordinated
653A — Preferred Equipment Pkg — XLT Trim
62M - Adjustable gas and brake pedals
Door trim — color coordinated molded w/ grab handle & reflector
Headliner color coordinated molded cloth
Sunvisors — color coordinated vinyl, single w/ covered mirror
Hood release
166 — Carpet Delete (replaced w/ black floor mat)
Driver & passenger frontal & side air bag/curtain (incl. passenger side air bag deactivation switch)
Belt-minder chime & flashing warning lights on VP if belts not buckled
Underhood service light
Safety belts — color coordinated w/ height adjustment
SOS Post Crash Alert System — activates when air bag deploys -. Unlocks doors, activates horns & emergency flashers
		ITB #2016-11-004
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OEM Supplied - Jack w/handle OEM Supplied - Lug Wrench
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Running Boards. One f1) Pair ADP with Grip strut (Type I) RUNNING BOARDS	


Aluminum diamond plate (.1875" thick) running boards with grip strut inserts shall be fabricated and installed under the cab as indicated in the attached drawings. The running boards must incorporate a pair of splash guards behind the front wheel wells to further protect the cab.

CHASSIS LIQUID SPRINGS SUSPENSION

A Liquid Springs suspension system shall be provided and installed on the rear axle of the chassis. It shall include a 12V PUMP, main hydraulic tank, and low pressure indicator kit.
The system shall be wired to kneel whenever the left leaf of the rear entry door is open. When the door is closed with the ignition on, the system shall automatically return to ride height.
Dump Feature activated by the Left rear access door. Override switch to be near right rear entry door Ignition switch Hot, Standard.
Per KKK, the rear suspension shall only lower the module when the vehicle is in park and the parking brake is set.

CAB FLOORING 

The chassis shall have rubberized vinyl flooring to aid in cleaning and long term wear. 

SPARE TIRE

One (1) spare tire and wheel shall be provided and shipped loose in the back of the ambulance. 

WHEEL SIMULATORS 

A set of four (4) Phoenix DOT Liner polished stainless steel wheel sims shall be provided and installed on the chassis wheels. Wheel sims that require loosening or removal of the OEM lug nuts for installation will not be acceptable.

REAR TIRE AIR FILL EXTENSIONS 

A set of four (4) Phoenix "Air Max" series valve stem extensions shall be installed on the dual rear tires of this ambulance per the manufacturer's instructions.  Equal or like. 

DEF/UREA TANK FILL BEZEL

There shall be an external fill for DEF/Urea as provided by the OEM manufacturer. Because of the corrosive nature of urea the cast bezel for the fill must be powder coat protected with a stainless steel splash shield under the bezel to the bottom of the body.

DEF TANK FILL SPLASH GUARD

A brushed stainless steel fuel fill splash guard shall be provided and installed below the DEF tank fill opening to protect the body from fuel overflow or drips. The plate shall be fastened to the body using two-sided Acrylic tape and Butyl rubber sealant. Screws are not to be used for attaching this plate to the body.
Installed below DEF fill to protect body - attach to body using double sided tape - no screws - make sure edges are sanded smooth

IDLE CONTROL

A chassis idle control system Intermotive CVC501A shall be utilized to operate while this ambulance is parked "on-scene" to maintain an adequate DC electrical supply.
Set RPM of 1400

CAB / CHASSIS EXTERIOR LIGHTING WARNING LIGHTS - GRILLE

Two (2) Wheeling 500 series L.E.D. lights shall be mounted in, or near, the chassis grille in Cast Products aluminum bezels.
The lens colors (from passenger side to driver's side) will be: Red / Red WARNING LIGHTS- 

INTERSECTION

Two (2) Wheeling 4x6 series Super L.E.D. warning lights shall be installed, one (1) on each chassis fender. The lights are to be located approximately as shown on the attached drawings.
The lens colors (from passenger side to driver's side) will be: Red / Red

FLANGES:

Two (2) Cast Products warning light flanges shall be provided and installed on the chassis fender mounted intersection lights.  Each flange shall be fabricated of polished aluminum and shall have a fifteen degree forward tilt design.

SIREN SPEAKERS:

One (1) pair of Cast Products siren speakers with Ambulance Manufacturer’s name plate attached to the front of the speaker shall be installed in the front bumper outer edges per the instructions provided by its manufacturer.  Each speaker shall be rated for not less than 100 watts.

HEATING AND AIR CONDITIONING

Heating and air condition for the patient compartment will be provided by a combination heat/ac unit mounted within the interior cabinetry. 
The heater portion will have a BTUH capacity of 35,000, the air conditioner will have a BTUH capacity of 32,000. A three-speed blower fan capable of 650 CFM on the highest setting will be included.
To reduce the potential for condensate leakage, dual 3/8” ID drain hoses shall be installed on the AC drain pan. The drain hoses shall terminate below and outside the ambulance body.
The combo system shall be provided with an electrically controlled water shutoff valve which shall close to stop the flow of hot water to the heater whenever the air condition is operating. An external condenser shall be mounted under the module. The condenser shall be houseline BMC1006 it shall provide 2564 CFM and 45, 00 BTU’s. External condenser mounted below module. 

AUXILLARY HEAT/AIR CONDITIONING

An auxiliary skirt mounted air condition condenser with dual 12V fans shall be installed under the ambulance body, near the side entry, and connected to the ambulance AC system.

THERMOSTAT

A Pro Air digital low voltage heating and air conditioning thermostat shall be provided to control the specified environmental systems. With cover standard switch locations. Mount probe in front of evaporator.  A 12-volt pump shall be provided and installed in the water supply line to the heater in order to improve heat output at idle speed. Install in the water supply line to the heater.


DRIVER'S CONTROL CONSOLE

The driver's control console shall be constructed of .125" smooth aluminum which has been MultiSpec paint to compliment the cab interior, and located so as not to interfere with any OEM dash features such as radio/climate controls, etc. The top face must be 1/4" black Kydex or ABS material and be hinged to allow easy access to electrical components within the console. All corners must be free of sharp edges and the console must be fastened to the cab floor in a manner so as to allow for quick and easy removal for access to components below.
In addition to the driver's switch panel, this console shall house ammeter, voltmeter, and engine hour meters. It shall also house an electronic siren as well as allowing room for the subsequent mounting of this agency's mobile radio(s).
Multispec Color: Greystone MS99-6072 or equal

CHASSIS FRONT END ALIGNMENT

The alignment of the unit shall be Fluid Filmed at the factory during the Quality Control Process. The unit shall only be sent for a front end alignment if it is determined necessary by the quality control procedure.

GENERAL BODY CONSTRUCTION

Because of a concern regarding single point responsibility for the major components of this ambulance, the body shall be built directly by the prime contractor in the same or adjacent facilities in which the remainder of the conversion is completed. Bids that offer "third party" or sub-contractor built bodies, including leases, rentals, sub-corporations, etc., will not be acceptable.
The module body for this vehicle shall be constructed utilizing aluminum alloy materials consistent with the load and service requirements of an ambulance. Structural members and skin shall be attached by MIG welding along the edges and VHB tape along the flat side of the body to prevent oil canning. Rivets, screws, bolts, tape or other fastening devices will not be allowed as the primary method of attachment.
Structural members, i.e. tubes, corner extrusions, etc., are to be 6063-T1 and 6063-T6 aluminum. Sheet aluminum used for walls, doors, roof, etc., are to be of 50521132 aluminum. Sample sections of all structural extrusions shall be made available for inspection by representatives of this agency on or before the bid opening. 


ROOF CONSTRUCTION

The roof shall be a single .090" sheet of 5052-H32 alloy aluminum. The roof sheet shall be completely welded to the extruded roof assembly. The use of multi-section roofs shall not be acceptable due to the possibility of cracks causing environmental intrusion.
The roof substructure assembly shall consist of four perimeter roof rail extrusions, lateral roof bows and interconnecting corner caps. The roof rail extrusions shall be engineered and designed by the primary manufacturer and shall be double hollow of 6063-T6 .125 aluminum. An integrated roof recess shall be incorporated to create a smooth transition from the one piece roof sheet to the perimeter drip rail. The perimeter drip rail shall be extruded as a design feature of the roof rail extrusion. The roof rail extrusion shall overlay the side skin by one half inch. The roof sheet shall be seam welded to the perimeter roof extrusion. The lateral roof bows shall be two inch by two inch by .125 square extrusions of 6061-T6 alloy aluminum. The structural members shall be located to support the roof skin on fourteen (14") inches between roof bow centers. The roof bows shall interconnect with the roof rails and be continuously welded at all contact points. The finished roof shall incorporate a machine rolled crown of not less than one and half inches in height to provide additional strength and allow water run-off.
The corner caps shall be designed to interlock with the roof perimeter, vertical corner extrusions and roof sheet. The corner caps shall be cast aluminum made from matched metal dies to insure a smooth and pleasing appearance. The caps shall act as a stress relief device to absorb energy and disperse the force along the roof extrusions in the event of a collision. The visible welds will be ground and finished to provide a smooth, seamless appearance.
The use of these corner caps is essential to the overall integrity of modular body structural system. Designs which involve welding the corner and roof edge extrusions together without the use of this feature, or roof corners manufactured from separate extrusions will NOT be acceptable to this agency. In no case, shall the corner caps be weakened by the addition of corner cap lights.

WALL CONSTRUCTION 

The corners of the modular body shall be designed and engineered by the primary manufacturer and constructed of 6063-T6 alloy aluminum. The corner extrusion shall be double hollow with a minimum thickness of .125 and .250 at the outer corner. The extrusion is designed with a unique curved appearance while maintaining very high strength and impact energy absorption. A polyurethane sealer shall be applied to seal the crevice between the corner extrusions and the side assemblies.
The side assemblies shall be reinforced utilizing 6061-T6 alloy aluminum two by two box tubing and shall be a minimum of .125 in thickness. Vertical tubes shall be spaced fourteen (14") inches on center from each other. The side structures shall frame a perimeter around all door openings. Intermediate skin stiffeners shall be located vertically to preclude skin deformation. Additional gusset plates shall be .250 inch aluminum and shall be welded at all contact points between the corner assembly and the roof perimeter. There shall be a 6" x 1/2" aluminum bar stock welded to the vertical tubes at the back of the squad bench and another 4" x1/2" aluminum bar stock welded to the upper section of the body. There shall be similar supports on the street side behind the cabinets. These structures add strength to the body and mounting points for cabinets, seat belts, etc.
The front, sides, and rear of the modular shall be configured from a single sheet of .125 aluminum. The one piece sheets shall be used to maximize integrity against dust, toxic fumes, cracking, and moisture penetration. The openings for doors, warning lights and exterior compartments shall be cut on the horizontal plane with a computer controlled plasma cutter for accuracy and integrity of temper. The roof and side skins shall be installed utilizing a very high bond adhesive to allow absorption of vibration and to eliminate "panning".

CAB TO PATIENT COMPARTMENT PASS-THRU

A 13-3/4" wide x 11-3/8" high pass-through opening with a sliding Plexiglas window shall be framed into the front wall. It shall have a head bumper for occupant safety and shall coincide with an opening of equal size framed into the back wall of the chassis-cab. The space between the cab and module shall be sealed by the installation of a flexible rubber "accordion" style enclosure. Inflatable or rigid seals shall not be acceptable. Sliding window to be framed on the module side using extruded aluminum sliding cabinet door framing components. 

FLOOR CONSTRUCTION

The floor shall be at lowest level permitted by clearances, but not more than thirty three inches from the ground. The floor structure shall consist of two by two by .125 structural box section with 6061-T6 alloy aluminum. The floor structure shall be welded with eight inches of weld at every joint. The openings created for the placement of exterior compartments shall have six inches of weld to insure a smooth surface to fit the compartment in the structure. Tapping plates of one half inch of 6061-T6 aluminum shall be completely welded both sides to the floor assembly. The finished floor assembly shall be securely welded to the wall structures with eight inches of weld and skipped welded every four inches to the exterior compartments. All critical load points shall be reinforced with one quarter inch by three inch by four inch gusset plates. Above the floor channels there shall be an aluminum moisture shield .050 inches thick. The entire underside of the modular shall be sealed with a waterproof sealant. All hollow structural shapes or cavities shall be sealed utilizing expandable foam.
The rear patient access shall be equipped with an exterior aluminum threshold mounted to the lower door jamb. This threshold will protect the bottom door jamb, in addition the rear patient floor shall have a fourteen gauge stainless steel cot protector.
Over the aluminum sub-floor, 3/4" thick, seven (7) ply exterior grade plywood shall be secured, using one quarter inch UNF machine by two and one half inch screws driven through the wood and the aluminum structural members below. The plywood shall be marine resin coated prior to installation to prevent warping due to ambient moisture absorption. The plywood floor shall be one piece from the bulkhead to the rear doors between the patient door steeple and squad bench and extend under the street side cabinets. The floor shall be flat and all depressions and screw head penetrations must be filled with an elastic floor fill compound suitable for such applications. The entire floor shall then be sanded smooth prior to laying the finished flooring material.

BODY TO CHASSIS MOUNTING

The mounting system shall not cause any chassis frame deformation. There shall be ten mounting points, five on each frame rail. The modular body shall have full perimeter welded sill rails of one half inch by two and a half inch of 6061-16 alloy aluminum. The modular body shall be welded to the sill plates at every exposed seam. At all outrigger mounting locations a double compression, neoprene rubber isolator mounts shall be used to minimize chassis vibration transfer to the modular body. At all four corners of the body between the floor structures shall be a one half by six inch structural plate that shall be bolted to the sill plate with a 1/2 inch grade eight bolt. The modular body and sill plates shall be attached to the frame rails using three quarter inch grade eight bolts. Any method contrary to QVM which may void the chassis warranty shall not be accepted.

DROP SKIRT

The skirt line forward of the rear wheels on both sides of the module shall be dropped 4 inches.
(SO-DROP-1C6154)
Curbside drop skirt only

SIDE ENTRY STEPWELL 
Inside the side entry door, a step well shall be constructed using bright aluminum diamond plate. The approximate size shall be 30.75" wide with a 15" tread and 9.5" riser. All seams must be welded, sealed and shall have sound deadening material applied to the underside.

UNDERCOATING

A non-flammable / non-combustible water based automotive undercoating shall be applied to the entire underside of the module in accordance with the chassis manufacturer’s guidelines. Applied to the entire underside of module. 

BODY INSULATION

The module walls and ceiling shall be insulated with 2 1/4" thick, R-11 (expanded) fiberglass bats insulation. Applications using thickness greater than this shall NOT be acceptable because it will increase compression density and results in less insulating value overall. Plank foam insulation (1-7/8" thick) shall be installed in the exterior compartment doors. This insulation shall not interfere with the workings of the door latching hardware.




ENTRY DOOR INSULATION

Module entry doors shall be insulated with 1 7/8" expanded polystyrene plank foam. The insulation shall be cut so as not to interfere with door latching mechanisms and must be glued in place to prevent settling.

INSULATION ENHANCEMENT

In addition to the insulation listed above, the interior of the ambulance walls, ceiling and entry doors shall be insulated with a reflective heat barrier.

MODULE SOUND INSULATION 

Sound absorbing material made from polyurethane (synthetic or natural fibers) acoustical foam installed over the rear wheel wells.
Sound absorbing material made from polyurethane (synthetic or natural fibers) acoustical foam installed over the rear wheel wells.

DRIP RAIL MOULDING

Above each entry and compartment door (excluding doors within 6" of the roof drip rail), an extruded anodized bright finish aluminum drip rail shall be fastened to the body with Acrylic structural adhesive tape. These drip rails must be finished to eliminate rough or sharp edges.

STONE GUARDS 

A full width aluminum diamond plate stone chip guard will be mechanically fastened to the lower front wall of the ambulance to protect the paint finish from damage.
ADP on the lower front wall of the module full width - see prints

FENDER FLARES 

A polished aluminum fender flair shall be installed around the rear wheel well openings. They will be installed so as not to interfere with tire rotation, movement, or replacement. A rubber gasket shall be applied between the fender flares and the body panels for corrosion protection.


FUEL FILL BEZEL 

The fuel tank fill will be protected by a cast aluminum fuel fill guard with polished flanges. 

FUEL FILL SPLASH GUARD 

A brushed stainless steel fuel fill splash guard shall be provided and installed below the fuel fill opening to protect the body from fuel overflow or drips. The plate shall be fastened to the body using two-sided Acrylic tape and Butyl rubber sealant. Screws are not to be used for attaching this plate to the body.
Installed below fuel fill to protect body - attach to body using double sided tape - no screws - make sure edges are sanded smooth

REAR BUMPER

The rear bumper sub-structure must be constructed from formed 1/4" steel plate. The framework shall be bolted to the chassis frame. The outboard pods shall be covered with .100" diamond-plate and the center section shall incorporate a flip-up step of grated material. The outer corners of the aluminum diamond plate pods shall have a smooth rounded corner.
Rounded bumper pods 

REAR RISER PANEL

Extending from the rear step to the bottom of the rear doors, for the full width of the rear wall, shall be a section of aluminum diamond plate. It will be mechanically fastened to the body.

TOW EYES

Two (2) chrome tow eyes shall be provided and mounted in cast aluminum tow eye boxes in the rear riser. The tow eyes must be positioned so that they are in-line with the ends of the chassis frame rails and must be bolted to supporting steel structure which is attached directly to the frame rails.

LICENSE PLATE HOLDER
A cast aluminum license plate bracket with polished flanges shall be recessed into the rear riser. It shall be provided with one (1) LED license plate light.
When mounting bracket, please put fluid film on all mounting screws. 


REAR MUD FLAPS
One (1) pair of black rubber, anti-spray mud flaps shall be provided and installed behind the rear tires. They shall be attached with non-rusting bracketry so as to allow easy replacement when necessary.

EXTERIOR STORAGE COMPARTMENTS

The exterior compartments shall be constructed of aluminum and shall be formed by a computer controlled brake and shear to decrease the amount of welding to fully enclose the compartment. The compartment therefore, shall be water tight. The compartment shall be welded in place to the side and floor structure with an additional bracket welded to a bracket connecting the exterior wall two with the floor structure. The compartment floor shall be supported from beneath with one by two by .125 6061 T-6 rectangular tubing welded to the underside and the floor structure. All exterior compartments shall be vented above the floor line (except the Oxygen and Battery compartments) with machine stamp louvers. The exterior compartment shall be lockable with one key fitting all doors. The compartments shall be equipped with handle and door locks. Each exterior compartment shall be provided with a sealed light to be illuminated upon the door opening. The light shall be activated by a magnetic switch. A door open indicator light shall be visible on the driver's console. The compartment configuration shall be as described.

STREETSIDE-FRONT EXTERIOR STORAGE COMPARTMENT (#1) 

The street side-front exterior storage compartment shall be constructed using .090" smooth aluminum and shall be sized according to the attached drawings. The floor of this compartment will be of a sweep-out design to aid in cleaning. Smooth, DA Finish, add foam tape behind panel to prevent rattling. 

STREETSIDE #2 EXTERIOR STORAGE COMPARTMENT

The street side #2 exterior storage compartment shall be constructed using .090" smooth aluminum and shall be sized according to the attached drawings. The floor of this compartment will be dished approximately 3" to increase vertical storage capabilities. .090 smooth, DA finish 3” dished floor.

STREETSIDE WHEELWELL COMPARTMENT (#3)

There shall be a compartment above the streetside wheel well area - sized as indicated in the attached drawings. This compartment shall be fabricated of .090" smooth aluminum. The door to this compartment shall be fastened to a smooth aluminum slide-out tray with 200 lb. capacity ball bearing slides.
.090" smooth aluminum - DA finish - door attached to a smooth aluminum slide-out tray with 200# ball bearing slides - see prints

CPR SEAT

A 28" wide CPR seat shall be provided in the streetside cabinet wall, above the wheel well, between the Action Area and the monitor/defibrillator shelf areas. It shall feature a fixed backrest, padded vinyl seat, back, and head rest cushions.

STREETSIDE-REAR EXTERIOR STORAGE COMPARTMENT (#4) 

The streetside-rear exterior storage compartment shall be constructed using .090" smooth aluminum and shall be sized according to the attached drawings. The floor of this compartment will be dished approximately 3" to increase its vertical storage capabilities.
.090" Smooth Alum. 3" Dished Floor

CURBSIDE-REAR EXTERIOR STORAGE COMPARTMENT (#5) 

In here shall be a compartment immediately aft of the curbside wheel well area - sized as indicated in the attached drawings. This compartment shall be fabricated of .090" smooth aluminum. The floor of this compartment will be dished approximately 3".
.090" smooth alum. DA Finish - 3" dished floor

CURBSIDE INTERMEDIATE COMPARTMENT (#6)

There shall be a compartment immediately aft of the curbside wheel well area - sized as indicated in the attached drawings. This compartment shall be fabricated of .090" smooth aluminum. The floor of this compartment will be dished approximately 3".
.090" smooth aluminum w/ DA finish -3"

ALS CABINET EXTERIOR ACCESS DOOR

The ALS cabinet shall be accessible from the exterior of the ambulance via a door located on the curbside wall, just forward of the side entry door. The size of this door shall be as indicated in the attached drawings.

CURBSIDE COMPARTMENT (#9)

A storage compartment made of smooth aluminum shall be located on the curbside of the ambulance, forward of the side entry door as indicated in the attached drawings. The floor of the compartment shall be sweep-out design and the door shall be right side hinged with a single Nader pin and rotary latch.
Smooth .090" aluminum, sweep out style floor, front hinged door w/ single center mounted Nader, install nylon strap as door hold-open

BEDLINER SPRAY COATING FOR COMPARTMENTS 

The following compartment(s) shall receive Scorpion (or equal) spray-on bed liner coating. The coating shall be not less than 2 mils thick and the color shall be
Light Gray standard Coating to be applied to compartment walls, floor and ceiling 

VERTICAL DIVIDER

One (1) full height, fixed, 125" smooth aluminum divider shall be provided in the SS1 compartment to separate the backboard storage area from the oxygen cylinder storage area. This divider shall be attached to the back top and floor of the compartment and the outer edge shall be finished with 1/2" diameter aluminum bar stock. It will also have a DA finish on both sides.
SS1 compartment - DA finish Divider shall be 17" deep
Above measurements include the rod

VERTICAL DIVIDER

One (1) full height, fixed, 12" deep .125" smooth aluminum divider shall be provided in the curbside-rear compartment to separate the backboard storage area from the remainder of the compartment this divider shall be attached to the back, top and floor of the compartment. It will also have a DA finish on both sides.
Curbside-rear compartment - DA finish Divider shall be 17" deep


ADJUSTABLE SHELF

One (1) adjustable shelf shall be provided in compartment SS2. It will be formed from .125 aluminum and shall be full depth with a 1" high lip up on the forward side and a 1" downward lip back sides. The top edges of the shelf will be finish sanded to provide a smooth, rounded surface. A vinyl edge guard shall be placed over the outboard edge to prevent damage to the shelf and equipment during removal/replacement. The shelf shall be supported by (4) ninety degree cast angles that are bolted to Uni-Strut adjustable track on the sides of the compartment walls.
.125" smooth aluminum, includes four shelf brackets and black pinch trim installed on the outside edge of the shelf

ADJUSTABLE SHELF 

One (1) adjustable shelf shall be provided in the curbside-rear compartment. It will be formed from .125" smooth aluminum and shall be approximately 16" deep with a 2" high lip. The top edges of the shelf will be finish sanded to provide a smooth, rounded surface. A vinyl edge guard shall be placed over the outboard edge to prevent damage to the shelf and equipment during removal/replacement. The shelf shall be supported by (4) ninety degree cast angles that are bolted to Uni-Strut adjustable track on the sides of the compartment walls.
.125" smooth aluminum, includes two shelf brackets and black pinch trim installed on the outside edge of each shelf.

ADJUSTABLE SHELF TRACK

Four (4) Uni-strut brand aluminum adjustable shelf tracks are to be installed in each compartment, two (2) each side, requiring an adjustable shelf or tray. Each track shall feature a continuous adjustment slot and two (2) short spring channel nuts designed to accept 1/4-20 bolts.
A 1.75" x 1.7" gusseted angle shall to used to support the shelf and fastened to each adjustable track using two (2) 1/4-20 hex head bolts per bracket Loosening the nuts on these bolts will allow the shelf or tray to be easily adjusted. When tightened, the bolts shall secure the shelf or tray and prevent movement or "shake-down".

PLASTIC TILES
Dri-Dek soft PVC plastic interlocking tiles shall be provided and installed on the floor of all compartments, shelves and trays.
Includes Dri Deck matting on all compartments, shelves, and trays. The color shall be black. 


EXTRUDED DOOR CONSTRUCTION

The outer face of the door and door edges shall be formed from one sheet of 5052-H32 aluminum. The door shall be flush with the body side. The outer skin shall be 0.125 inches thick and shall be welded every six (6") inches to the inner door frame using a minimum of one and one-half inch (1-1/2") long bead. All corners shall be welded a minimum of two inches (2") in each direction. The edge of the door shall be seamless.
The door frame shall meet with the exterior skin with a smooth seamless transition. There shall be no seams or crevices on the door or the door frame which allows the possibility of corrosion.
Both patient compartment and exterior compartment doors shall be provided with extruded rubber seal system consisting of a hollow cell bulb gasket. The gasket shall insert into an appropriately designed groove in the inner door extrusion. This will provide the best seal possible. Glued on seals or seals that are mounted to the compartment openings are unacceptable as they will easily be torn by loading or loading of equipment stored in the compartment.
All doors shall be attached using minimum 1/4-20 stainless steel hex bolt with stainless steel piano hinges with a pin of at least 0.250 inch in diameter. The hinge must be slotted to provide field adjustments. A corrosion inhibitor shall be applied to the door frame and jamb bolt holes prior to installing the hinge.
All compartment doors shall be constructed the same as the entry doors. To ensure continued door alignment and successful latching capabilities, all access doors must be encased by a doorjamb that is separate from the body skin and welded to the 2" x 2" tubular body frame members. The door jamb shall be a 0.125"/0.380" thick 6063-T6 aluminum extrusion.
The interior surface of the patient compartment doors (rear and curb side) shall be finished in a safe and attractive manner that harmonizes with the interior appointments. The door panels shall be designed to allow removal without disturbing the door latching hardware. Door panels must be flush fitting not overlay. Doors using pliable materials such as upholstery are prohibited due to greater risk of contamination by blood born pathogens through stitching or when cut or torn.
The three (3) patient compartment entry doors shall be fitted with Tri-Mark, flush fit, "paddle latch" hardware on the interior and exterior. The patient compartment doors shall be provided with a keyed lock and the rear doors and side door shall be lockable from the inside without a key per FMVSS.
When the doors are opened, the hinges, latches and door Fluid Films shall not protrude into the access area. All patient compartment doors shall employ the same type locking hardware. All door latches shall comply with requirements of FMVSS 206.
The locking devices shall be two-stage rotary latches and shall be FMVSS 206 certified. Where applicable, there shall be two door latches, one at the top and one at the bottom, controlled by a single locking handle The latches shall lock into an adjustable "Nader" type pin located in the door frame. The Nader will utilize a captive nut to provide adjustment and replacement without loss of the nut plate. The locking system shall be actuated from the locking handle by metal push rods.
The outside door handles shall be a rugged "paddle style" that are near flush with the door skin. These handles shall provide adequate clearances for the use of gloves. On the curb side and rear doors, the inside handle shall be a "paddle style" type constructed from stainless steel and shall be equipped with an inside door lock. All exterior storage compartments and module entry doors shall be lockable with the same key.
The compartment and entry door shall be painted separately from the modular body. The doors shall then be installed on the painted module. A corrosion inhibitor shall be applied to the door frame and jamb painted extrusion prior to installing the doors to provide- a barrier between the hinge and the paint.
All entry and compartment doors shall be insulated with a 2-1/2" thick closed cell block foam insulation.
The side entry door will have pressurized gas strut overhead door Fluid Films which will hold the doors at not less than 90 degrees when open. The gas struts will include an "over-Fluid Film" feature to prevent failure due to the door leaf being moved past 90 degrees.

COMPARTMENT DOORS 

The inside of each compartment door will be finished with .063" bright aluminum diamond plate liner, bolted to the door extrusion flanges with machine screws that thread into automotive style spring clips that are fastened to the door extrusions to hold the skins securely to the door frame.

ENTRY DOORS

Inner door liners shall be .090" smooth aluminum, painted with Multi-spec paint to coordinate with the patient compartment interior and screwed to the door extrusion flanges with machined stainless steel screws into automotive style spring clips. Screws for both compartment and entry door liners are treated with Lock-Tice to prevent the screws from backing out on their own.
All modular body entrance doors shall be equipped with emergency over ride lock release latches. Each door shall have an upper and lower over ride lock release lever coated with black rubber.

COMPARTMENT SILL PROTECTORS 

All compartments shall have a stainless steel sill protector. The sill protectors shall be manufactured from 20 gauge stainless steel and cover the bottom door frame protecting it from scratches.

DOOR LATCHING HARDWARE

All module doors, compartment over 23" high and entry, shall utilize two (2) rotary style latches per door leaf, closing onto two (2) "Nader" striker pins with capped heads and adjustable cage nuts. Smaller doors, under 23" high shall be able to use (1) rotary style latch. Construction using other latching methods, striker pins without capped ends NOT acceptable.
Compartment doors in excess of 23" tall shall receive dual nadir pins 

COMPARTMENT DOOR LATCHES, HINGES AND HARDWARE

When the doors are opened, the hinges, latches and door Fluid Films shall not protrude into the patient compartment. All compartment doors shall employ the same type of locking hardware. All door latches shall comply with FMVSS 206. The locking devices shall be two stage rotary latches and shall be in accordance with FMVSS. There shall be two door latches, one at the top and one at the bottom, controlled by a single locking handles. The latches shall lock into an adjustable Nader type pin located in the door frame. The Nader will utilize a captive nut to provide adjustment and replacement without loss of the nut plate.
The compartment door handles shall be Trimark paddle style handle with a large enough space for gloved hands to operate the handle. The door handles shall be free floating with 1008 cold rolled steel mechanical components with Nitrotec treated wear components. The locks shall be a lock cylinder with a reversible key. The compartment door entry system shall have been tested to 50,000 cycles. The door handle shall be mounted to the exterior door panel using mechanical fasteners and rubber gaskets that will eliminate the possibility of electrolysis. All doors shall have closed cell block foam insulation.

COMPARTMENT DOOR LATCHES, HINGES AND HARDWARE

When the doors are opened, the hinges, latches and door Fluid Films shall not protrude into the patient compartment. All compartment doors shall employ the same type of locking hardware. All door latches shall comply with PMVSS 206. The locking devices shall be two stage rotary latches and shall be in accordance with FMVSS. There shall be two door latches, one at the top and one at the bottom, controlled by a single locking handles. The latches shall lock into an adjustable Nader type pin located in the door frame. The Nader will utilize a captive nut to provide adjustment and replacement without loss of the nut plate.
The compartment door handles shall be Trimark paddle style handle with a large enough space for gloved hands to operate the handle. The door handles shall be free floating with 1008 cold rolled steel mechanical components with Nitrotec treated wear components. The locks shall be a lock cylinder with a reversible key. The compartment door entry system shall have been tested to 50,000 cycles. The door handle shall be mounted to the exterior door panel using mechanical fasteners and rubber gaskets that will eliminate the possibility of electrolysis. All doors shall have closed cell block foam insulation.

COMPARTMENT HOLD-OPEN 

Each exterior compartment door shall have a gas-strut hold open to keep the doors open at a 90 degree angle. 

SIDE ENTRY DOOR

A side entry door to the patient compartment shall be provided, sized and located as shown in the attached prints. It shall have a full length stainless steel hinge, with pin not less than 1/4" in diameter, on the forward edge of the door and a gas strut controlled door Fluid Film which will hold the door at not less than 90 degrees when open.

PATIENT ENTRY DOOR LATCHES, HINGES AND HARDWARE

When the doors are opened, the hinges, latches and door Fluid Films shall not protrude into the patient compartment. All patient doors shall employ the same type of locking hardware. All door latches shall comply with FMVSS 206. The locking devices shall be two stage rotary latches and shall be in accordance with FMVSS. There shall be two door latches, one at the top and one at the bottom, controlled by a single locking handles. The latches shall lock into an adjustable Nader type pin located in the door frame. The Nader pin will utilize a captive nut to provide adjustment and replacement without loss of the nut plate. The door latching mechanism shall have an upper and lower patented "Emergency Release Latch" to allow egress from the vehicle if a system failure should occur.
The door handles shall be Trimark chrome paddle style handle with a large enough space for gloved hands to operate the handle. The door handles shall be free floating with 1008 cold rolled steel mechanical components with Nitrotec treated wear components. The locks shall be a lock cylinder with a reversible key. The rear trailing door shall have an exterior paddle handle that removes the necessity of reaching inside the patient compartment door. The door entry system shall have been tested to 100,000 cycles.

The locking system shall be from the locking handle by aluminum push rods. The patient compartment doors will be equipped with an inside door lock. All entry doors shall have horizontal aluminum reinforcements welded to the door frame and the entry doors shall have closed cell block loam insulation. CS and Rear access doors all have exterior handles. 

REAR ENTRY DOORS

Double leaf rear entry doors to the patient compartment shall be provided, sized and located as shown in the attached prints. They shall have a full length stainless steel hinges with pins not less than 1/4" in diameter.


REAR ENTRY DOOR

One (1) pair of 3-1/2" "Grabber" door hold open devices shall be installed on the exterior of the doors to hold them open when necessary. The devices shall be located on the approximate horizontal centerline of each door as indicated in the attached prints. The rubber insert into the "female" side of the hold open device shall be replaceable.
The grabbers shall be located on the approximate horizontal centerline of each door as indicated in the attached prints.

ENTRY DOOR WINDOW

A 19" x 18" black aluminum framed window is to be centered in the entry door, with the top of the window about 6" down from the top of the door. The dark tinted window shall be capable of opening via a sliding section of the glass. The sliding section must be positively latched when in the closed position to prevent it from being opened from the outside. It must also include a sliding screen section to cover the opening.

ENTRY DOOR WINDOW

A 19" wide x 18" high black aluminum framed window is to be centered in the entry door, with the top of the window about 6" down from the top of the door. The dark tinted window shall be single piece fixed glass.

EXTERIOR BODY REFLECTORS

Four (4) 2" x 2.75" Red reflectors shall be provided and installed as follows... One (1) each in the lower rear corner of each side of the module and, One (1) each in the lower right and left corners of the rear wall of the module.
Installed on the lower rear of the streetside and curbside just above the rubrail and in the right corners of the rear wall just above the rear riser.

CONVERSION ELECTRICAL SYSTEM

This vehicle's 12-Volt DC power supply shall be separate and distinct from the chassis (OEM) system, except that both will be powered by the same chassis generating system and batteries. The total ambulance electrical system shall be equipped with, but not limited to the following: dual 12-volt batteries, generating, starting, lighting, ignition, visual and audible warning systems, specified electrical equipment and devices including master switch consoles located in the cab and patient compartment, plus other specified accessory wiring. The electrical systems and equipment shall comply with all applicable FMVSS including Federal Motor Carrier Safety Regulations (FMCSR). It shall also conform to all the applicable Society of Automotive Engineers (SAE) recommended standards and practices, whether or not specifically referenced in this document.

All electrical and electronic components shall be selected to minimize loads, thereby not exceeding the vehicles generating system capacity. System components must be readily accessible through access panels or doors for routine service and maintenance. Likewise switches, indicators and controls shall be located and installed in such a manner so as to facilitate routine service, maintenance and replacement.
All electronic devices and equipment installed in this ambulance must have proper filters, suppressers or shielding to contain electromagnetic radiation and prevent radio frequency interference (RFI).

WIRING

The ambulance body and accessory electrical equipment shall be served by circuit(s) separate and distinct from the vehicle chassis circuits. Wiring methods must conform to SAE 51292. All wiring provided by the FSAM shall be copper and conform to all the SAE J1127 and SAE 31128 requirements. All low tension primary cable shall have GXL or better insulation. All low tension battery cable shall have SGX insulation. Documentation from the wiring manufacturer that the wire used by the FSAM is in compliance with this requirement shall be submitted with the proposal. Bids not meeting this requirement will not be accepted.
The wiring shall be permanently color coded to identify wire function. Wires shall be permanently heat ink embossed with both number and function codes. The function code shall be the descriptive name of the circuit served. The number code shall be the exact purpose of that circuit. This number code shall be completely referenced in a detailed wiring schematic provided with the vehicle. The function and number code shall be embossed at a minimum of four inch intervals the entire length of the wire terminating into all switch and control panels. The use of multi-conductor cable must be function and color coded and shown on the wiring

Wiring shall be routed in conduit or high temperature looms with a rating of 300 degrees Fahrenheit where necessary to protect it. All added wiring shall be located in accessible, enclosed, and protected locations and kept at least six inches from the exhaust system components. Electrical wiring and components shall not terminate or be routed in the oxygen storage compartment except for the oxygen controlled solenoid, compartment light, and switch plunger. All conduits, looms, and wiring shall be secured to the body or frame with insulated metal cable straps in order to prevent sagging and movement which results in chafing, pinching, snagging or any other damage. All apertures on the vehicle shall be properly grommeted and sealed for passing wiring and conform to SAE 1292. All items used for protecting or securing the wiring shall be appropriate for the specific application and be standard automotive, aircraft, marine, or electronic hardware.
Circuit connections shall be made on barrier style terminal blocks utilizing binding post screws for positive mechanical connections. To minimize the potential for wiring shorts and voltage drops all wiring terminals shall be brass, tin plated, annealed, ETP copper with nylon high heat insulation. Serration's, inside the barrel, provide maximum contact and tensile strength after crimping. Connection shall be machine crimped, to UL standards, with a high quality crimping tool that produces crimps for a given size wire and terminal that are precisely alike in appearance and performance. Crimping pressure must be controlled by a ratchet device on the hand tool or a corresponding pre-calibration in the crimping jaws of an automated machine. Crimping pressure can neither over-stress nor under stress the terminal-barrel-machined dies. Therefore, this agency requires a termination that is free of contamination and is extremely resistant to shock and critical environment conditions.
No splices shall be permitted except for connection of "pig-tail" devices. Butt splices are permitted for connection of "pig-tail" devices. The use of IDC (Insulation Displacement Connector) connectors, i.e.: "3M Scotchlok" type fasteners, is not acceptable.
The various wiring installations as supplied with this vehicle shall be of the automotive "harness" design. For ease of identification and future replacement these harnesses shall be engineered and manufactured in the following sections.
1. Engine compartment harness.
2. Driver's control console harness.
3. Main module harness.
4. Chassis rear lighting harness.

12 VOLT LOAD CENTER

The 12 volt load center is the location of the conversion electrical system's major 12 volt electrical control and distribution components. The load center will be within a designated interior cabinet located above the module walk/pass through and may not be mounted in the engine compartment nor in any outside or outside accessible compartment. This cabinet shall be accessible through a hinged, locked door.

12 VOLT ELECTRICAL SYSTEM

The electrical power control system that this ambulance shall incorporate must be based on modular printed circuit board technology. This type of system is required by this agency because of its concern for an electrical system that is reliable, efficient, and easily maintained.





12 VOLT ELECTRICAL SYSTEM

The electrical power control system that this ambulance shall incorporate must be based on modular printed circuit board technology. This type of system is required by this agency because of its concern for an electrical system that is reliable, efficient, and easily maintained.
The printed circuit board shall be designed and manufactured as follows: A screen printed board with all circuits fully numbered and labeled. The circuit board shall be a double-sided copper trace printed circuit with a double-sided laminated isolator. The board shall be non-photo imaginable solder mask over bare copper with hot air leveled solder over non masked copper. Fuse capacity is the beginning factor in calculating trace width to ensure proper current carrying capability. The circuits shall then be oversized as much as space permits for maximum cooling of the board.
All holes shall be plated through. The terminal strips shall be mounted on the board for connection of the above mentioned wiring harness. Automotive transient suppressers must be incorporated into circuit board at the point of cable entry to the board. All relays must include built in noise suppression. The suppression must be accomplished with a IN4001 parallel with the coil. The relay must have a 40 ampere continuous contact rating with one form C contact arrangement. Normally open contact must have a maximum initial voltage drop of 200 milli-volts at 40 ampere contact load. The relays must withstand 24 VDC for five minutes conducting rated contact current in case of accidental 24 volt jump start condition. Circuit board options must be programmable via jumpers to facilitate addition of options. The color of wire and circuit number must be screened printed at the terminal block connections on the board for rapid identification and relation schematics.
Documentation that the above requirements are met must be included with the bid document.
The printed circuit board shall incorporate red LED indicators for on board diagnostics for input, output, and switching circuits for troubleshooting at a glance.
CIRCUIT BOARD CERTIFICATION
The printed circuit board must meet the following specifications:
1. Packaging and Interconnecting Acceptability Standard number IPC 600
2. UL-796
3. Solder mask, IPC number SM-840
4. Solder in conformance with MIL SPEC QS-571
5. Laminate in conformance with IPC number 4101 Certification must be included with this bid.
DRIVER'S SWITCH PANEL
The driver's switch panel shall house fourteen (14) Carling rocker switches with tactile rubber switch caps and internal lighting to indicate relay status. The switches are to be arranged in two rows, the top row being for emergency circuits and the bottom for non-emergency circuits. The emergency switching shall be as follows. (Left to right)
a) EMERGENCY MASTER - Momentary - serves as a master control switch for all emergency circuits
b) PRIMARY/SECONDARY - On/Off/On - controls the flashing warning lights
c) FRONT LIGHT BAR - On/Off - switches the front light bar
d) HORN / SIREN - Momentary - switches OEM horn button between OEM horn and siren functions
e) Spare Switch - On/Off - for option/future use
Spare Switch - On/Off - for option/future use Spare Switch - On/Off - for option/future use
The non-emergency switching shall be as follows: (left to right)
Spare Switch - On/Off - for option/future use
f)  MODULE MASTER. - Momentary - serves as a master control switch for all non-emergency module circuits
g) LOW DOME - On/Off Module lights
h) LEFT FLOOD - On/Off - switches the left (streetside) scene lights
RIGHT FLOOD - On/Off - switches the right (curbside) scene lights I) 
i) REAR FLOOD - On/Off - switches the rear flood lights
m) BACK-UP ALARM CANCEL - Momentary - temporarily cancels the back-up alarm when activated by placing the vehicle in reverse. This circuit will automatically reset when the vehicle is taken out of reverse gear.
n) Spare Switch - On/Off- for option/future use
Four (4) indicator lights shall be installed on the Driver's Switch Console as follows:
o) BATTERY
p) DOOR OPEN - red lens - approximately 3/4" x 3/4" - flashes to indicate that a module entry door is open or not completely latched.
q) EXTERIOR COMPARTMENT OPEN - amber lens - apx. 3/4" x 3/4" - flashes to indicate that an exterior storage compartment door is open or not completely latched.
r) LOW VOLTAGE - red lens - apx. 3/4" x 3/4" - lights in conjunction with a warning buzzer to warn the driver that the system voltage has dropped to 11.8 volts or below.
ATTENDANT'S SWITCH PANEL 
The attendant's switch panel shall house eleven (11) Carling Contura rocker switches with tactile rubber switch caps and internal lighting to indicate relay status. The controls are to be arranged in a single row and shall be as follows: (left to right)
s) MODULE MASTER - Momentary - serves as a master control switch for all non-emergency module conversion circuits
t) LEFT DOMES - On/Off/On - switches the left (streetside) patient compartment dome lights to low or high intensity
u) RIGHT DOMES - On/Off/On - switches the right (curbside) patient compartment dome 112fils tu or high intensity
v) Spare Switch - On/Off - for option/future use
w) ATTENDANTS LIGHT - On/Off- activates the light in the action area
x) Spare Switch - On/Off - for option/future use
y) HEAT/AC - On/Off/On - Allows manual selection of heat or AC - middle switch position sets system to switch automatically via thermostat
z) HEAT/AC BLOWER FAN - On/On/On - controls the heat or AC fan speed - low/medium/high aa) POWER VENT FAN - On/Off - switches the rear dual power vent fans bb) Spare Switch - On/Off - for option/future use
cc) VACUUM - On/Off- switches the on-board electric vacuum system
Below each switch a white plastic translucent panel shall be installed, engraved with nomenclature defining the switch function. The engraved lettering must be filled with permanent black ink or paint. Spare switches shall include a blank panel for future engraving. Behind each panel, incorporated into the switch circuit board, amber LED lights shall serve as back-lighting.
Carling rocker switches




OPEN DOOR INDICATOR

One (1) "open door" indicator shall be provided and installed in the cab console. It shall feature an engraved top view diagram of an ambulance with flashing LED lights to indicate which exterior storage compartment and/or entry door is open.



DRIVER'S CONTROL CONSOLE GAUGES  
VOLT METER

It shall monitor system voltage in a range between 7 and 18 volts, and must be wired to eliminate erroneous readings from connection voltage drops.
Incorporated in the front switch panel 

WARNING LIGHT FLASHER

A Vanner 9860GCPE programmable flasher shall be provided and installed to flash the warning lights at a rate of 75 to 80 flashes per minute.

Warning Light Flash Pattern, Comet "Stutter" Flash 

The warning lights shall flash in a Comet "Stutter" flash pattern.

POWER LOCKS - MODULE ENTRY DOORS

Power locks shall be provided for the side and rear-curbside module entry doors. The system shall include the actuator, actuator connector, actuator pigtail, relay and relay connector. Two switches shall be installed to control the locks, one (1) on the curbside wall just inside the side entry door and one (1) on the rear wall, just inside the rear entry doors.
Includes actuator, actuator connector, actuator pigtail, relay connector - one switch installed on curbside entry door lock box panel, one switch installed on the curbside "rear" entry door lock box panel. Includes tie in to OEM cab chassis doors (including Key faubs if chassis is so equipped)

POWER LOCKS - EXTERIOR COMPARTMENT DOORS

Power locks shall be provided for exterior compartment door(s). The system shall include the actuator, actuator connector, actuator pigtail, relay, and relay connector. A single switch, located in the Action Area, shall serve to control the power locks.
Includes actuator, actuator connector, actuator pigtail, relay connector - Use same switch as entry doors 




REMOTE POWER DOOR LOCK CONTROL 

A remote momentary toggle switch with a rubber boot shall be provided to control the cab and module door locks. It shall be mounted Left side license plate frame.

LOW VOLTAGE ALARM

The electrical system shall be monitored by a system that provides both an audible and visual warning in case of low voltage in the ambulance. The alarm shall sound if the system voltage at the batteries drops below 11.8 Volts for a 12 Volt nominal system for more than 120 seconds.
Light in cab console and Buzzer in cab. 

BATTERY SYSTEM

The vehicle shall be supplied with a dual 12 volt battery system. Two OEM batteries. The battery system shall be wired in accordance with KKK - A - 1822F. The system must meet SAE J541 for starter circuit voltage drop. The batteries shall be activated through the OEM ignition switch. The ignition switch shall only turn off power the module and not the chassis circuits. When the ignition is shut off a five minute time keeps the module powered up for unloading patients. A momentary rocker switch shall be installed which will disable the timer. It shall be labeled TIMER BYPASS. It shall be located on the side of the center console.


MODULE POWER DISCONNECT SWITCH

This device shall be located on the driver's compartment console and shall be permanently labeled and back lit with a LED light and the brightness controlled by the head light rheostat. The "MODULE" disconnect switch shall be considerably different in size and feel from the other console switches.
Mounted in the .1-box and wired to operate with the ignition switch w/5 minute delay unless indicated otherwise.
There shall be a "Timer Bypass" switch located on the Driver's side of the console.

BATTERY CHARGER/CONVERTER

One (1) Iota brand 45 amp battery charger/converter with IQ4 auto-switch shall be provided and mounted in the cab behind the driver's seat. It shall be powered by the shoreline inlet.
Installed behind driver's seat or compartment #2
 
12 VOLT RECEPTACLES 

The patient compartment shall be supplied with a 12-Volt DC 20 amp service capacity. This circuit must incorporate a Schottky diode or similar device to isolate medical equipment connected to the system.

Two (2) cigar lighter style 12 volt receptacles shall be installed; one (1) in the action area, and one (1) in the curbside front inside/outside (ALS) compartment. They shall be battery hot at all times. The receptacle shall include a stainless steel face plate and a rubber cap to protect the opening when not in use.

(1) in the Action Area (1) in the ALS cabinet

Outlet Kussmaul. USB Dual Port, 5VDC. 3 Amp output. Switch panel Style PORT 5 VOLT DC POWER USB STYLE

The patient compartment shall be furnished with a 5 volt DC, 3 ampere capacity, separately protected circuit, with a Dual USB outlet. It shall be located in the action area switch panel.

(1) Located on the passenger side of the center console switches (1) located in the action area


RADIO SPEAKERS 

A set of speakers for the AM/FM radio shall be provided and mounted in the module ceiling per the attached prints. A volume control switch will be installed in the rear switch console.
With volume control in action area see prints


PATIENT COMPARTMENT CLOCK

One (1) Franklin 12 volt, digital clock with approximate dimensions of 7.5" high x 13.5" wide x 2.75" deep with a 4" twelve or twenty-four hour/minute display shall be provided and mounted  over rear doors

110 VOLT AC WIRING AND COMPONENTS 

This vehicle shall be furnished with a two (2) wire plus ground 110 volt AC wiring system completely separate from its 12 volt DC system. It must comply with Article 551 of the National Electrical Code and is to be used for powering maintenance devices, battery chargers, etc. while on standby.
Electrical system - 120-Volt 
SHORE POWER

A Kussmaul ."Super Auto Eject" system inlet or "shoreline inlet", shall be installed where indicated in the attached drawings. It must contain a male inlet connection rated and labeled for 20 amps, be suitable for wet conditions and be protected by a white spring loaded plastic cover. A properly sized female mating plug (three-pin design) must also be provided for connection to this agency's wiring.
To protect this device from arcing during connection or disconnection, a time delay and interrupter device shall be installed.


INVERTER PRE-WIRE

Wiring will be fun fished and installed for an inverter in the streetside #2 compartment. This wiring shall include power and ground feeds as well as system feeds connected to the interior outlets. This wiring shall be suitable for the installation and operation of an inverter, if specified elsewhere or agency supplied.
Pre wire for inverter in compt. #2 110 VOLT RECEPTACLES 
Three (3) hospital grade 110 volt AC duplex receptacles with green internal pilot lights shall be installed in the patient compartment as follows: one (1) in the action area; one (1) in the curbside front inside/outside (ALS) cabinet; one (1) on the street side wall in the monitor/defibrillator shelf area.
(1) in Action Area (1) in Defib. area, (1) in ALS cabinet
Recept, 110V AC Hospital Grade Duplex, Interior IATS 
In addition to the above specified recepts, one (1) additional recepts shall be installed as specified:
(1) center of squad bench


INTERIOR DOME LIGHTING

General lighting for the patient compartment shall be as follows: Eight (8) overhead L.E.D. dome lights shall be mounted, four (4) over the squad bench side and four (4) over the primary cot side. These lights must be recessed into the ceiling headliner, protruding not more than 1 1/2". They must be secured to aluminum backing plates welded to the roof structure above the headliner and may not be fastened solely to the headliner material.
Any lighting system using a rheostat to control lamp intensity is NOT acceptable to this agency. These lights are to be controlled by switches in the attendant's switch console.
Dome Lights, Curbside Activate on Opening of Entry Doors 
Additionally, the curbside dome lights shall automatically light on their "low" setting when either the side or rear entry doors are opened.

Curbside dome lights shall automatically light on their "low" setting when the rear entry doors or the side entry door is opened. (BATTERY HOT thru Timer) ECN 1785


F450 (4x4) 170" Medic or Equal

TIMER SWITCH

One (1) Intermatic 30 minute spring wound mechanical timer(s) shall be provided and installed to control the lights specified above. The timer shall be installed in the curbside wall adjacent to the side entry door.
Installed in the curbside wall adjacent to the side entry door.


STEPWELL LIGHTING

One (1) 3/4" recessed, two diode, LED light shall be provided and installed in the left (rear) wall of the side entry stepwell and shall be wired to operate when the side entry door is open.

Installed in the right forward stepwell wall - NOTE: apply silicone to the back side of the flange to seal the light to the diamond plate - wire the light to operate when the side entry door is open
3/4" Recessed 2 diode LED 

ENTRY DOOR WARNING LIGHTS / REFLECTORS 

One Red LED light/reflector shall be provided and installed in the lower corner of each module entry door. These lights shall flash whenever the entry doors are open and module power is on.
Installed at bottom of entry doors - see prints - lights are to flash whenever the module entry doors are open and battery power is enabled. If this is not a multiplex system, it will also require a wigwag flasher and three (3) 4-prongs relays. Add magnetic switch to left entry door leaf.
3" round reflector - Red Install 3" round reflectors

ACTION AREA LIGHTING
One (1) 8" LED strip light will be mounted in the action area. It will be controlled by a switch in the rear switch panel.

Activated by a switch on the rear switch console. Mount as close to rear wall as possible.

HANDHELD SPOTLIGHT

A 400,000cp hand held spotlight shall be provided with a minimum of one hundred thousand candle power lamp. It shall be in a corrosion proof housing with a protected momentary switch to prevent accidental activation. A minimum eight feet of heavy duty coiled cord will be supplied and it shall be hard wired in the cab area and accessible to the driver and passenger.
The spotlight shall be hard wired to connections installed in the console in the cab.

ALS CABINET_LIGHTING

Two (2) 2.5" recessed LED 9 diode light with clear lens and aluminum flange(s) shall be mounted in the ALS Cabinet.
2" Recessed 9 diode LED
(1) E1 (1) E2

EXTERIOR LIGHTING

Exterior lighting fixtures shall be corrosion and weather resistant. Fixtures attached to the sides of the ambulance below the 75" level shall be near flush mounted, not protruding more than 2".
Because of this agency's concern for corrosion protection, all exterior lighting shall be attached to the body or chassis using nylon inserts which shall serve to isolate the mounting screws from the aluminum or sheet metal. The holes into which the nylon inserts are placed must be drilled prior to painting the body so that paint protects the edge of the aluminum at each hole. Methods of attaching the light fixtures to the body or chassis that involve the screw coming into direct contact with the aluminum or sheet metal are not desired - even if purported "anti-corrosion" coatings are applied to the mounting screws beforehand.
All light fixtures to be installed using nylon inserts unless directed otherwise.
On secondary mode; grille, intersection, and center clear warning lights drop off.

CLEARANCE AND MARKER LIGHTING

Five (5) amber LED upper body marker/clearance lights are to be mounted at the extreme upper front edge of the module, above the drip rails, in accordance with FMVSS requirements. See attached drawings.
Five (5) red LED upper body marker/clearance lights are to be mounted at the extreme upper rear edge of the module, above the drip rails, in accordance with FMVSS requirements. See attached drawings.


One (1) red LED body marker/clearance light is to be mounted at the rear streetside vertical extrusion at approximately the midway point in accordance with FMVSS requirements. See attached drawings.
One (1) red LED body marker/clearance light is to be mounted at the rear curbside vertical extrusion at approximately the midway point in accordance with FMVSS requirements. See attached drawings.


WARNING LIGHTS 

Seven (7) Whelen 900 series L.E.D. flashing lights shall be provided and installed on the upper front wall of the ambulance body, below the drip rail, as per the attached prints.
The lens color (from passenger side to driver's side) will be: Red / Clear / Red / Clear 1 Red 1 Clear 1 Red. 

FLANGES

Seven (7) Whelen chrome plated flange(s) shall be provided and installed on the specified 900 Series lights as indicated in the attached drawings.

REAR MODULE WALL EXTERIOR LIGHTING WARNING LIGHTS

Three (3) Whelen 900 series Super L.E.D. lights shall be provided and installed on the upper front wall of the ambulance body, below the drip rail, as per the attached prints.

SCENE LIGHTS 

Two (2) Whelen 900 series scene lights with tilt optic lenses shall be mounted on the upper rear of the ambulance as shown in the attached drawings.
These lights will be controlled via a switch on the cab console and shall operate whenever the rear entry doors are open and also whenever the chassis is placed in "reverse" gear.
The lens color (from passenger side to driver's side) will be: Red / Scene I Amber \ Scene 1Red 




FLANGES

Five (5) Whelen chrome plated flange(s) shall be provided and installed on the specified 900 Series lights as indicated in the attached drawings

Warning Lights, Rear, Wire Pair to Brake Light Circuit IATS
Wire one pair of the specified Red rear warning lights to the brake light circuit to serve as additional high mount brake lights in addition to their function as warning lights.
Wired to thru window lights
Rear Scene Lights, Activate on Opening of Rear Entry Doors 
The rear wall scene lights of the ambulance shall be wired to operate in conjunction with the opening of the rear entry doors.
Module power on, Rear Load lights come on when the rear doors are open, with ON/OFF switch on Dash panel. 

STOP, TAIL, TURN AND BACKUP LIGHTING TAIL/BRAKE 

Two (2) Whelen 600 series Super L.E.D. tail/brake lights with Red lenses shall be installed on the rear of the module as shown in the attached drawings.

TURN SIGNAL 

Two (2) Whelen 600 series Super L.E.D. turn signal lights with amber arrow lenses, shall be mounted on the rear of the module as shown in the attached drawings.

BACKUP 

Two (2) Whelen 600 series Super L.E.D. backup lights with clear lenses shall be installed on the rear of the module as shown in the attached drawings.

FLANGES 

Six (6) Whelen chrome plated flange(s) shall be provided and installed on the specified 600 Series lights as indicated in the attached drawings. Includes one (1) pair of brake/tail lights, one (1) pair of turn signals, and one (1) pair of back-up lights mounted on the rear exterior module wall.

CURBSIDE MODULE WALL EXTERIOR LIGHTING WARNING LIGHTS

Two (2) Whelen 900 series Super L.E.D. lights shall be provided and installed on the upper curbside wall of the ambulance body, below the drip rail, as per the attached prints.

FLANGES 
Four (4) Whelen chrome plated flange(s) shall be provided and installed on the specified 900 Series lights as indicated in the attached drawings.

SCENE LIGHTS

Two (2) Whelen 900 series scene lights with tilt optic lenses shall be mounted on the upper curbside of the ambulance as shown in the attached drawings.
The lens color (from front to rear) will be: Red / Scene / Scene / Red these lights will be controlled via a switch on the cab console. 




STREETSIDE MODULE WALL EXTERIOR LIGHTING WARNING LIGHTS 

Two (2) Whelen 900 series Super L.E.D. lights shall be provided and installed on the upper streetside wall of the ambulance body, below the drip rail, as per the attached prints.

SCENE LIGHTS 

Two (2) Whelen 900 series scene lights with tilt optic lenses shall be mounted on the upper streetside of the ambulance as shown in the attached drawings.
These lights will be controlled via a switch on the cab console and shall operate whenever the side entry doors are open.
The lens color (from front to rear) will be: Red / Scene / Scene / Red 

FLANGES 

Four (4) Whelen chrome plated flange(s) shall be provided and installed on the specified 900 Series lights as indicated in the attached drawings.

COMPARTMENT LIGHTING

One (1) 2.5" recessed LED 9 diode light with clear lens and aluminum flange(s) shall be mounted in each exterior storage compartment except SS#2 which shall have two (2) lights. The lights shall operate whenever the compartment door is open and the battery disconnect switch is on. One (1) per compartment - if installed below the floor line, seal backside of flange w/ foam tape
one (1) in SS#1 two (2) in SS#2 two (2) in SS#4 three (3) in CS#5 one (1) in CS#6 one (1) in CS#9

Compartment Lights. 1/2" LED rope lights  one (1) SS #3
Patient Compartment Blue LED Strip Lighting (SO-BLED-1C6115)

Blue strip lighting on street side and curbside (@ anlde level when sitting in module) SS: Run from rear exit to front of action area and CS: Run from rear exit to front of bench (Kenequip Blue LED strip light) floor level lighting, curbside and street side.




RUNNING BOARD LIGHTS

One (1) 2.5" diameter LED light with clear lens and recess mount black plastic flange shall be installed on each side of the lower front module wall to illuminate the cab running boards when the cab doors are open.
Installed in the lower front module wall to illuminate the cab running boards when the cab doors are open 

BACK-UP ALARM

A solid state back-up alarm capable of sounding an alarm of at least 90 decibels shall be installed so that when the chassis gear selector is placed in "Reverse", it will automatically activate. The alarm must be able to be momentarily shut off via a switch located on the driver's switch console. However, the alarm must reset automatically so that it will sound again when reverse gear is selected.

SIREN

A Whelen #295HFSA7 siren shall be installed in the console located in the cab. It shall be wired so that it will operate when the Ignition switch is "On". The siren shall be capable of powering (2) 100 amp speakers.
Mount remote amp behind driver's seat


COMMUNICATION PROVISIONS AND EQUIPMENT 

ANTENNA BASE

A Motorola style antenna base shall be provided and mounted mid-line of the module roof.
Port 1 terminates behind driver’s seat Port 2 terminates in action area

ANTENNA POWER/GROUND WIRES

A 10 gauge Red power wire and a Black ground wire shall terminate. The power wire shall be protected by a 20A (minimum) breaker or fuse.

Terminate:
Ignition Hot
(1) Behind driver's seat (1) In action area



BACK-UP CAMERA SYSTEM

A backup camera system shall be provided and installed to aid the driver in safely maneuvering and positioning the ambulance. The system shall consist of a high resolution color camera mounted on the rear of the ambulance and a flat panel color display installed on the back side of the driver's sun visor. The system shall only operate when the chassis is in reverse gear.
Adjust Camera field of view to ensure visibility of edge of the rear bumper.
 
EXHAUST FANS 

The patient compartment of this ambulance will be ventilated with fresh outside air via one (1) static intake vent and one (1) power exhaust vents. The system shall be capable of completely exchanging the air volume within the patient compartment every two (2) minutes. The location of the intake and exhaust vents shall be as indicated in the attached drawings.

ENTRY DOOR LINERS 

The entry doors shall be finished using 14 GA brushed Stainless Steel. The liner shall be secured to the inside of the entry doors using black oxide or stainless steel screws and finish washers.
Attach using stainless or black oxide screws w/ finish washers

ENTRY DOOR LINERS 

The entry doors shall have a removable cover to allow the end user to maintain the door handles without having to disassemble and remove the entire door panel. This panel shall have red and white reflective striping to meet N.F.P.A. 1917.
Attach using stainless or black oxide screws w/ finish washers 

ENTRY DOOR GRAB BARS 

A 1.25" diameter stainless steel grab bar with 45 degree "V"-style bend shall be provided and installed on the inside of each entry door, as shown in the attached drawings.
Backer plates must be installed inside door before sending unit to paint.

INTERIOR GRAB BARS 

A grab handle shall be provided and installed on the lower section of the ALS cabinet.
An additional grab handle shall be provided and installed on the curbside rear lower cabinet.
A grab handle shall be provided and installed on the lower section of the ALS cabinet.
An additional grab handle shall be provided and installed on the curbside rear lower cabinet.
Grab Handle, Chrome 
The grab bar(s) shall have a chrome finish.
On/Off Switch For Lighting
(SO-SWI-1C6115)

Hansen Grab Bars and Patient Compartment Blue LED Strip Lighting will be on the same On/Off switch in the action area switch panel.

Hansen 96" Grab. Bar, Above Cot ILOS GRAB BAR ABOVE COT

One (1) aluminum grab bar shall be provided and mounted on the ceiling above the primary cot per the attached drawings. It shall be 1.25" diameter x 96" long and shall have slip resistant rubber inserts in the rail. The grab bar will include two (2) intermediate stanchions and all fastening points shall fall on roof tubes or backer plates for added strength and support.
(SO-GRAB1-1C6115) SR# C2016136F
Hansen #STKTRA1L96-BLUE 96" Knurled aluminum overhead grab rail, lighted with end stanchions and (2) center stanchions


Hansen 72" Grab Bar, Above Squad Bench ILOS GRAB BAR ABOVE SQUAD BENCH 

One (1) aluminum grab bar shall be provided and ceiling mounted above the squad bench per the attached drawings. It shall be 1.25" diameter x 72" long and shall have slip resistant rubber grip inserts. All fastening points must fall on roof structure or backer plates welded to roof structure.
(SO-GRAB2-1C6115) SR# C2016136F
Hansen #STKTRAlL72-BLUE 72" Knurled aluminum overhead grab rail, lighted with end stanchions and (2) center stanchions

UPHOLSTERY

The finish of the entire patient's compartment, including storage cabinets and equipment, shall be impervious to soap and water, disinfectants, bio fluids, mildew and shall be fire resistant per FMVSS 302. Upholstered cushions shall be a minimum of thirty two ounce nylon reinforced commercial vinyl material. Squad bench cushions and attendant seat and backrest cushions shall be fabricated in such a manner to eliminate exposed welting. Cushions with welting or beaded seams shall not be accepted due to the risk of bio fluid penetration. Describe below your method of cushion construction. The color of the upholstery shall be determined after award.

Solid color seamless
All cushion style backs to be installed with butterfly clips at the top and Velcro at the bottom.
Upholstery Color, Gunmetal 
The upholstery color shall be "Gunmetal"

PADDED TRIM 

To mitigate injury to passengers, trim pieces consisting of 1/4" plywood covered with 1/4" high density foam and wrapped with heavy duty vinyl to match seating upholstery will be installed:
A. At the vertical outside corner of the cabinet forward of the attendant seat
B. At the upper horizontal and vertical corners above the action area
C. At the upper horizontal and vertical corners above the defibrillator shelf
Vertical and horizontal edges above the monitor/defib and action area FLOORING
The finish flooring shall be one (1) piece, heavy duty commercial grade vinyl (Lon Seal Lon Plate II), permanently adhered to the sub-floor.
Because of this agency's concern for ease of cleaning and decontamination (when necessary) where the floor and the sidewall cabinets and squad bench base it shall be rolled u the vertical wall 3".
With approximately 3" roll up both street side and curbside.
Flooring Color, "Lon Plate II", Gunpowder 424TX The flooring color shall be Gunpowder 11424TX


ENTRY DOOR SILL PLATES 

20 ga. brushed stainless steel plates shall be provided and installed as follows:
A. Just inside the rear patient compartment entry doors at the floor. The plate shall extend from the door sill into the patient compartment approximately 3".
B. At the side entry stepwell / floor transition. The sill plates shall be formed to trim the edge of the floor cutout around the side entry stepwell structure. The width of these plates shall be approximately 2".

Sill plates shall be fastened using stainless steel screws countersunk flush with the surface. Additionally, clear silicone sealant shall be used to seal the plates to the flooring to prevent accumulation of fluids beneath.
ATTENDANT'S SEAT

An EVS brand seamless 6 degree stationary back with 3 point harness shall be provided and installed adjacent to the Action Area.

ATTENDANT'S SEAT BASE

An EVS brand pedestal style steel seat base shall be provided for the rear facing attendant's seat The assembly shall be bolted to the floor through mounting plates welded into the floor structural tubing.


INTERIOR CABINETRY 
CONSTRUCTION REQUIREMENTS

In general, the interior of this ambulance shall incorporate features to mitigate injuries to passengers caused by sudden hard braking or accident impact Exposed edges shall be protected by radius or chamfer trim and, where possible, corners shall be rounded with radius trim. All devices and equipment will be mounted as flush as possible with its surrounding surface. Padding shall be installed in areas where features may obstruct head movement as attendants work within the patient compartment.
The layout of interior cabinetry for this ambulance shall be as indicated in the enclosed drawings. Variation from this design may not serve the needs and requirements of this agency and may be cause for rejection of the bid. As stated earlier in this document, the bidder must supply drawings which will be considered when determining whether a particular design meets our needs.
The cabinets in this vehicle shall be constructed of Marine Grade Feather ply plywood which has been covered by a commercial grade high pressure plastic laminate on BOTH sides prior to its use in fabricating the cabinetry. The face and inside of the cabinets shall be covered by a commercial grade laminate, adhered to the cabinet face by a high quality poly vinyl adhesive using a thermal press application. The wood, adhesive and laminate shall be pressed together at 200 degrees for four minutes in a thermal platen press. There shall be no voids of the adhesive between the laminate and the cabinet surfaces. The manual application of laminate on one or both sides of cabinetry after or during assembly is NOT acceptable. Plastic, fiberglass, or composite wood will not be acceptable for use in the cabinetry structure. "Marine grade" plywood shall be defined as being devoid of gaps or spaces in each ply, not just outer surface layers. The thickness of the finished panels used to construct the cabinets, shelves and doors shall be 3/4 inches including mica and adhesive.
All cabinets will be fastened together using 8 mm dowels placed no farther than 32 mm apart. The dowels shall be a hardwood and pre-glued. Construction that staples or uses wood screws driven into the edge of the plywood is NOT acceptable due to the reduced holding capability of screws driven into the veneered edge additionally, cabinetry shall be firmly bolted to mounting plates welded to the body side structure.

CABINET LAMINATE COLOR

The laminate color for the outside finish of all cabinets shall be Gray Pampas #4168-6. The laminate color for the inside finish of the cabinetry shall be Gray Pampas #4168-6.

CEILING HEADLINER

The ceiling will be finished with 1/8" Luan backed padded white vinyl panels. Any seams shall be trimmed to prevent sagging and provide a clean attractive appearance. The ceiling panel shall be mechanically attached to the roof structure but all fasteners shall be hidden.
The use of un-backed fiberglass headliner materials will not be acceptable due to their potential for cracking and palling. Along the longitudinal center of the ceiling, a padded cover shall be installed to close-off the electrical wiring chase. It must be covered with vinyl to match the upholstery.

PVC backer w/ padded white vinyl cover ELECTRICAL (J-BOX) CABINET
The Electrical (J-Box) cabinet will be located at the front of the ambulance interior. It will be designed to house the primary components of the module electrical systems, both 12VDC and 110VAC. The cabinet will be configured as indicated in the attached drawings.
· F cabinet left hinged wood door
· S1 cabinet sliding plexi doors w/ 1 adjustable shelf

CABINET BELOW CAB PASS-THRU 
A cabinet shall be provided on the lower front wall below the pass-thru to the cab. It shall be sized and shall have openings as indicated in the attached drawings.
· S2 cabinet sliding plexi doors w/ 1 adjustable shelf ALS CABINET 
The ALS cabinet will be located at the right front corner of the ambulance interior. It will feature interior as well as exterior access to storage areas. The cabinet will be configured as indicated in the attached drawings


SQUAD BENCH LID 
The squad bench shall have a one (1) piece laminated 3/4" plywood lid will be hinged along the back of the bench, with a stainless steel continuous (piano) hinge. It shall have two (2) gas charged strut hold open devices installed beneath the lid. A stainless steel paddle handle latch, mounted on the squad bench riser, shall provide a positive latch point to prevent the bench lid from opening in the event of an accident.
One (1) seat cushion, two (2) gas charged strut hold open with (1) squad bench Latch
Lid to "Pop" Open when latch is released   


SQUAD

BENCH INTERIOR LINING
The area beneath the squad bench shall be lined with 3/4" plywood with commercial grade high pressure laminate to provide flat, easily cleanable storage.
SQUAD BENCH INTERIOR LINING
A black rubber liner material with embossed pebbled pattern shall be installed on the floor of the storage space beneath the squad bench.

Install on floor of storage space under squad bench - adhere rubber w/ adhesive SEAT BELTING SQUAD BENCH:
Seatbelt, Assy, (6) Point, (1) EA - Change Notice 8 -Compliant
(2) for squad bench (Standard)

GRAB BAR AT HEAD OF SQUAD BENCH
One (1) 1.25" diameter stainless steel "A" style grab bar shall be provided and mounted at the end of the squad bench. It shall be provided with sharps and trash brackets and shall be through bolted with an aluminum backer plate. Through bolted to squad bench end riser.
SHARPS CONTAINER - INSTALLED 
One (1) two-quart mail box drop style sharps container with wire mounting bracket shall be supplied and installed in the A-Bar at the end of the squad bench.
TRASH CONTAINER - INSTALLED 
One (1) two-gallon plastic trash container shall be supplied and installed in the A-bar at the end of the squad bench.
CABINET ABOVE SQUAD BENCH
A cabinet shall be provided on the upper curbside wall above the squad bench. It shall be sized and shall have openings as indicated in the attached drawings. The bottom of this cabinet shall have vinyl wrapped high density foam padding to protect occupants.
· R1 cabinet top hinged plexi door
· R2 cabinet top hinged plexi door
8" depth (overall) unless otherwise noted. See Prints. Maximum Height 8 1/4". No struts. STREETSIDE CABINETRY 
The Streetside cabinetry will be configured as indicated in the attached drawings.
- Al cabinet sliding plexi doors w/ 1 adjustable shelf
· A2 cabinet sliding plexi doors w/ I adjustable shelf


- B3 cabinet sliding plexi doors
- C cabinet top hinged plexi door - DI cabinet sliding plexi doors
SCUFF PLATE - STREETSIDE CABINET WALL
An 8" high brushed stainless steel scuff protection plate shall be provided and installed on the lower street side cabinets to help prevent damage. The material shall be bonded to the cabinetry - no screws are to be used in fastening it to the cabinet structure.
Installed from CPR seat down with bend to create lip at bottom Seatbelt, Assy, (6) Point., (1) EA - Change Notice 8 -Compliant (1) for CPR side seat
All wood doors and drawers to have 3/4" Satin J trim for both the door and Jamb. PLEX1GLAS_COLOR 
Plexiglas cabinet doors/windows will be Smoke.
Door/Drawer Latch, Southco M1-62-8, 2IN S/S, Non-Locking
(2) El
(2) E2
(1) Action area drawer
(1) C cabinet
(1)R1
(1) R2
CABINET DOOR LATCHES - LOCKING
One (1) polished stainless steel locking Southco M1 Series flush pull latch (s) shall be installed in cabinet doors.



OXYGEN SYSTEM
This ambulance shall incorporate an on-board piped medical oxygen system in accordance with the guidelines put forth in KKK-A-1822, as currently amended.
The system shall consist of a supply cylinder (when indicated below), low pressure, electrically conductive (green) hose approved for medical oxygen, and self-sealing oxygen outlets as indicated below. Industrial or welding oxygen hose is not acceptable. Medical certified hose and components must be utilized throughout.
On-Board Oxygen Regulator, Manual, 50 psi OXYGEN REGULATOR
One (1) oxygen regulator(s) shall be provided and attached to the oxygen supply hose(s) provided. The regulator shall feature a chrome plated brass body with all brass high-pressure chamber, 3,000 psi maximum inlet pressure, internal resealing relief valve protecting against over pressurization, 2" diameter gauge, foreign matter filter, neoprene diaphragm, DISS outlet, CGA-540 nut and nipple and UL listing.
Ship Loose unless otherwise directed
OXYGEN CYLINDER BRACKET
One (1) ZICO QR-MV oxygen cylinder bracket mounted on Uni-Strut track shall be provided and installed in the designated compartment.
To be mounted on two (2) 56" adjustable shelf tracks. Track, Unistrut for Oxygen Rack 
OXYGEN CYLINDER WRENCH
A cast aluminum oxygen cylinder wrench shall be supplied and tethered to the compartment wall next to the oxygen cylinder brackets.
OXYGEN OUTLETS
Two (2) self-sealing Ohio style quick disconnect oxygen outlets will be installed in the action area, as shown in the drawings.
(2) In Action Area


ADDITIONAL OXYGEN OUTLETS)
One (1) self-sealing Ohio style quick disconnect oxygen outlet(s) will be installed. Wall head of squad bench.

VACUUM PUMP 
An electric vacuum pump shall be installed in the streetside #2 compartment. This pump will be activated by a switch in the attendant's switch console. It will be protected from damage by shifting equipment by means of a fabricated expanded aluminum mesh guard.
IV HANGERS 
Two (2) Cast Products recessed aluminum fold down IV hangers shall be installed on the ceiling where indicated in the attached drawings. They must have rubber fold-down safety arms with Velcro straps. The base must be anchored to mounting plates welded to the roof structure.
Floor Plates for Installation of Power Load or Performance Load, Stryker Performance Load with Cot Up-grade kit
Center mount
Decals, 11=1" Logo
One on each fender (ship loose)
One on passenger rear - lower area (ship loose) one in Action Area (install)
One on curbside wall by side entry door (install)
Paint, Module, Sikkens -  or equal
White (Standard) BODY PAINT
The exterior of the top, sides, front and rear walls shall be painted with Sikkens White. Preparation of the body must follow the paint manufacturer's specifications and the painting must be done in a paint booth enclosure which has been specifically designed for such purpose, and meets Environmental Protection Agency requirements at the time.
All hardware and doors must be removed prior to painting. The doors must be painted at the same time as the remainder of the module to eliminate the potential for color differences. Any paint process that involves painting the doors while attached to the body will NOT be acceptable due to the incomplete coverage of paint in the hinge area of the jambs.
Prior to painting, all mounting holes for the door hardware, exterior lighting fixtures, vents, assist handles, etc., shall be made in the body. This will allow both primer and paint to cover the edges of the mounting holes and provide additional corrosion protection at these critical locations. Systems which cut mounting locations, or drill mounting screw holes after painting are NOT acceptable since they allow the potential exposure of raw aluminum after the paint process is complete. Use of an anti-corrosion material alone, which is applied after the painting process is complete, will NOT meet the requirements of this section.
The front, sides and rear of the module and the striping shall be covered by AkzoNobel (or equal) high quality automotive polyurethane acrylic paint, which is then to be wet sanded and buffed to a high gloss.
Wheels remain OEM color White: Standard 
STRETCHER STRAP 

An adjustable nylon web tie down strap with quick release connectors will be installed against the back wall of a designated compartment for securing short boards, folding stretchers, or stair chairs. The strap shall be secured to the compartment wall with two (2) footman's loops.
Installed in rear backboard compartment unless directed otherwise - nylon web strap w/ quick clip/buckle and two (2) footman’s loops
INTERIOR SAFETY SIGNAGE
Two (2) signs with the verbiage: "NO SMOKING - OXYGEN EQUIPPED" shall be installed in the vehicle. One (1) will be installed adjacent to the attendant's switch console, and the other shall be installed in a conspicuous location the cab.
Two (2) signs with the verbiage: "FASTEN SEAT BELTS" shall be installed in the vehicle. One (1) shall be installed in a conspicuous location in the patient compartment and one (1) shall be installed in a conspicuous location in the cab.
Two (2) NO SMOKING-OXYGEN EQUIPPED and two (2) FASTEN SEAT BELTS signs, one (1) each in the cab and in the patient compartment, 110V for each 110V outlet, "Authorized Service Only" sticker in J Box.
OWNER'S MANUALS
The chassis manufacturer's operating and warranty manuals will be turned over to this agency upon delivery and acceptance.
A reference handbook, in a three-ring binder, providing guidelines for the operation, care, and maintenance of systems or components found in/on this ambulance will also be given to this agency at delivery and acceptance. This booklet will also contain: the name, address and phone number of the manufacturer; general, paint, structural and electrical system warranty statements; drawings of this vehicle; electrical system information and schematics; copies of the completed pre-delivery check-off sheet; any other pertinent information applying to the proper and safe operation of this vehicle.
MODULE STRUCTURAL WARRANTY
The warranty terms on the ambulance module structure shall be for a term of fifteen (15) year. So called "lifetime" warranties are not acceptable unless they specifically identify in the warranty that they will be valid for at least fifteen (15) years.
AMBULANCE CONVERSION ELECTRICAL WARRANTY
The warranty terms on the ambulance conversion electrical system shall be for a term of twelve (12) months or twelve thousand (12,000) miles from the date of delivery of the completed new custom module to the end user. Regardless of subsequent ownership.

AMBULANCE GENERAL CONVERSION WARRANTY

The Manufacturer shall warrant to the original retail purchaser for an unlimited mileage for a period of twelve (12) months from the date of delivery that this product shall be free of substantial defects in materials and workmanship, which are attributable to manufacturer and which arise during the course of normal use and service.

AMBULANCE CABINET CONSTRUCTION WARRANTY

The Manufacturer shall provide a 12-month general warranty on the vehicle conversion, which covers defective parts and/or components, improper choice of materials, parts and/or components, improper design or engineering and poor or improper workmanship or quality control techniques. Upon expiration of the attached twelve (12) months standard conversion vehicle warranty. The following parts or components of the patient compartment cabinets of the vehicle will remain free from defects in material and workmanship:
· That the wood or non-wood material used for the construction of the cabinets shall not delaminate.
· That the wooden dowels used for the construction of the cabinets shall not allow the cabinet sections to separate.
· This Cabinet Construction Warranty commences upon the expiration of the original twelve (12) months standard conversion vehicle warranty and continues for the lifetime of the vehicle for the original owner on the original chassis. For the purpose of the Limited Lifetime Cabinet Construction Warranty, a lifetime is defined by the Manufacturer as; 10 years from the expiration of the original twelve (12) month standard conversion vehicle warranty for only the only original retail purchaser/owner.






MODULAR BODY PAINT WARRANTY

The ambulance manufacturer in conjunction with the paint supplier shall warrant to the original retail purchaser under normal use and service, each new modular body paint job is free of all material and workmanship defects for a prorated period of five (5) years from the date of delivery.
The warranty provided herein shall cover and extend to the following properties of the paint system according to the warranty schedule:
Loss of adhesion of the paint system resulting in rust
Cracking of paint system
Fading or loss of gloss

END OF SPECS LIST









1.3 QUALIFICATIONS AND REGULATORY REQUIREMENTS 
A. Qualifications: The following personnel and organizations shall be provided/performed by the contractor, developer, or subcontractors.

B. Regulatory Requirements.
1. NFPA as applicable
2. OSHA as applicable
3.     Chassis Standard Warranty- 3 Years/ 36,000 Miles

OEM Ambulance Chassis Warranty the OEM warranty terms on the ambulance chassis shall be for a term of three (3) years or 36.000 miles, whichever occurs first.
Developed with consideration of the Federal Specification KKK-A-1822 and NFPA 1901: Standard for Automotive Fire Apparatus, NFPA 1917 defines the minimum requirements for the design, performance, and testing of new automotive ambulances intended for use under emergency conditions to provide medical treatment and transportation of sick or injured people to appropriate medical facilities

1.4	SUBMITTALS

A. Shop Drawings: NAME design drawings and calculations shall be provided
B. 360 Photos- Front, sides, under tow, roof, rear and interior of unit will be submitted with  bid packet to insure ambulance meets requirements and for review prior to official award. 
C. Contract Closeout Submittals: Operation and Maintenance manual.
D. Warranty Documentation 
E. Estimated Delivery Date
  1.5	MANUFACTURER'S WARRANTY

A. The Ambulance Manufacturer shall warranty its product based on the description provided in the specifications pertaining to sections outlined requiring warranties. From the date of completion of its work to the extent that it will repair any defects of which It is notified during that period which may appear because of faulty design, workmanship or material furnished under the specifications. A copy of the manufacturer's warranty shall be submitted with the submittal package.

B.   All guarantees for equipment or accessories not manufactured by the Ambulance Manufacturer shall be provided to the owner.

PRODUCTS
 2.1	MATERIALS

A. Construction: a complete description of products, materials and components used in the ambulance. 
B. Foundation:
1. Description: of all components and accessories found in the unit. 

2.2	ACCESSORIES
The Ambulance manufacturer shall provide and install all accessories as described specifications unless specifically stated otherwise. Appurtenances shall include at least the following:
1.4 A.	SPECIFICATIONS: SEE: 1.2 SCOPE:


VI. [bookmark: _Toc276819782][bookmark: _Toc276820861]CONDITIONS GOVERNING THE PROCUREMENT

This section of the ITB contains the schedule for the procurement, describes the major procurement events and contains the general requirements governing the procurement.


[bookmark: _Toc276819783][bookmark: _Toc276820862]A. SEQUENCE OF EVENTS

The Chief Procurement Officer will make every effort to adhere to the following schedule:

	ACTION
	RESPONSIBILITY
	DATE

	1.  Issue ITB 
	Chief Procurement Officer (CPO)
	11/16/2016

	2.  Return of “Acknowledgment of Receipt” Form for Distribution List 
	Potential Offerors (PO)
	12/02/2016

	3.  Mandatory Pre-Bid Conference
	CPO
	N/A

	4.  Deadline to Submit Questions
	PO
	11/29/2016

	5.  Response to Written Questions/ ITB Amendments
	CPO
	TBD

	6.  Submission of Bid
	Bidders
	12/08/2016

	7.  Bid Evaluation
	Evaluation Committee (EC)
	To Be Determined

	8.  Contract Award*
	Purchasing Agent/BCC*
	12/20/2016

	9.  Protest Deadline
	Bidders
	15 Days of Notification

	       Start of Performance
	
	12/21/2016


           
   *Contract award is subject to approval of the Board of County Commissioners.

       
[bookmark: _Toc276819784][bookmark: _Toc276820863]B. EXPLANATION OF EVENTS

The following paragraphs further detail the activities listed in the sequence of events shown in Section II, Paragraph A.

[bookmark: _Toc276819785][bookmark: _Toc276820864]1. Issue ITB
This ITB is being issued by the County Chief Procurement Officer on behalf of Sierra County Fire Department.

[bookmark: _Toc276819786][bookmark: _Toc276820865]2. Return of “Acknowledgment of Receipt” Form for Distribution List
Potential Bidders should hand deliver or return by facsimile or e-mail or registered or certified mail the “Acknowledgement of Receipt” form that accompanies this document (See Appendix A) to have their organization placed on the procurement distribution list.  The form should be signed by an authorized representative of the organization, dated and returned to the attention of Jocelyn Holguin, Chief Procurement Officer, by the close of business on the date indicated in Section VI.A (Sequence of Events), above.

The procurement distribution list will be used to notify those that submitted the form of any written responses to questions and any ITB amendments. Failure to return this form shall constitute a presumption of receipt and rejection of the ITB, and the potential Bidder's organization name shall not appear on the distribution list.

22. 3. Site Visit and Pre-Bid Conference – NONE

23. 4. Deadline to submit written questions
Potential Bidders may submit written questions as to the intent or clarity of this ITB until November 29, 2016 @ 2:00 PM MST on the date indicated in Section VI.A (Sequence of Events), above. All written questions must be sent by e-mail to the County Procurement Agent.

5. Response to written questions/ITB Amendments
Written responses to written questions and any ITB amendments will be posted to the County Chief Procurement Officer web site link: http://www.sierraco.org under the Vendor Registry Link. 

Notification of such posting shall be provided to all potential Bidders that have returned the “Acknowledgement of Receipt” Form found at Appendix A. The “Acknowledgement of Receipt” Form will accompany the posted distribution package. The form should be signed by the Bidder's representative, dated, and hand-delivered or returned by facsimile or e-mail or by registered or certified mail by the date indicated thereon. Failure to return this form shall constitute a presumption of receipt and withdrawal from the procurement process.


[bookmark: _Toc276819790][bookmark: _Toc276820869]6. Submission of Bid
BIDS MUST BE RECEIVED FOR REVIEW AND EVALUATION BY THE CHIEF PROCUREMENT OFFICER OR DESIGNEE NO LATER THAN 2:00 PM MST ON December 8, 2016  IN SECTION II. PARAGRAPH A (SEQUENCE OF EVENTS), ABOVE. BIDS RECEIVED AFTER THIS DEADLINE FOR ANY REASON WILL NOT BE ACCEPTED OR CONSIDERED. 

The date and time of receipt will be recorded on each Bid. Bids must be addressed and delivered to the Chief Procurement Officer or his designee at the delivery address listed in Section I, Paragraph C. Bids must be submitted sealed and labeled on the outside of the package to clearly indicate that they are in response to the “AUTOMOTIVE AMBULANCE” Invitation To Bid and should reference “ITB#2016-11-004”. Bids submitted by facsimile or other electronic means WILL NOT BE ACCEPTED.

A public log will be kept of the names of all Bidders submitting bids. Pursuant to Section 13-1-116 NMSA 1978, the contents of any Bid shall not be disclosed to competing Bidders prior to contract award.

[bookmark: _Toc276819791][bookmark: _Toc276820870]7. Bid Evaluation
The Chief Procurement Officer may at his/her option initiate discussions with bidders who submit responsive or potentially responsive Bids for the purpose of clarifying aspects of the Bids;  please note Bids may be accepted and evaluated without such discussion. Discussions SHALL NOT be initiated by the Bidder.

8. Contract Award
Any contract awarded shall be awarded to the Bidder whose bid is most advantageous to the County, taking into consideration the evaluation factors set forth in this ITB. Such award shall be subject to the prior review and approval of the County Commission.

The selected firm will be submitted to the County Commission for approval of award.  The County will then enter into construction contract consistent with AIA Document A201 – 2007 and Supplementary Conditions (Appendix C).  
 
[bookmark: _Toc276819798][bookmark: _Toc276820877]9. Protest Deadline
Any protest by an Bidder must be timely, in conformance with, and will be governed by Sections 13-1-172 through 13-1-176 NMSA 1978 and Sierra County Procurement Policy. The fifteen (15) day protest period for the submittal of a timely protest shall begin on the day following the contract award.  Protests must be written and must include the name and address of the protestor and the Request For Proposal number. It must also contain a statement of grounds for protest including appropriate supporting exhibits, and it must specify the ruling requested from the Chief Procurement Officer. The protest must be delivered to the Chief Procurement Officer and/or her designee:


Sierra County Procurement
Attn. Jocelyn Holguin, Chief Procurement Officer
855 Van Patten
Truth or Consequences, New Mexico 87901

NOTE: Protests received after the deadline will not be accepted.


VII. [bookmark: _Toc276819830][bookmark: _Toc276820909]RESPONSE FORMAT AND ORGANIZATION

[bookmark: _Toc276819831][bookmark: _Toc276820910]A. NUMBER OF RESPONSES
[bookmark: _Toc276819832][bookmark: _Toc276820911]Bidder’s may submit only one (1) response to this ITB.

B. NUMBER OF COPIES
Bidders shall deliver four (4) printed and one (1) electronic copies of their Bid to the location specified for the delivery and receipt of Bids on or before the closing date and time for receipt of Bids. (Identical copies are defined as the original plus the number of additional copies needed to fulfill the requirement. For example, a requirement for four (4) identical copies would be fulfilled by submitting the original and four [4] copies of the original.) The original copy should be clearly marked “ORIGINAL” on the front cover and shall contain original signatures.




VIII.   EVALUATION CRITERIA

The mandatory requirements listed below requires a vendor response, as indicated. Failure to respond to, or properly comply with, a mandatory requirement may result in the disqualification of the Bidder’s Bid. Note: failure to respond to a mandatory requirement will result in receiving a score of zero (0) for that requirement.
The following is a summary of evaluation factors with point value assigned to each or a Pass/Fail evaluation. These, along with the requirements of this ITB, will be used in the evaluation of individual Bid submittals.
A.  License									(PASS/FAIL)
State of New Mexico License 

B.  Prior Business Experience						(PASS/FAIL)

Must have been in business performing similar and like services for a period of 5 years or more.

BASIS OF AWARD:  Contracts awarded as a result of this solicitation shall be awarded to the responsible Bidder(s) whose Bid represents the best value and is in the County’s best interest


APPENDIX A
BID SIGNATORY  FORM
Relationship of County (“Owner”) and the successful Contractors - The successful Contractor accept a relationship of trust and confidence between itself and Sierra County. The Contractor shall agree to furnish his/her/its’ best skill and best judgment and to cooperate with County, any and all regulatory agencies, and any design professionals associated with the oversight and funding of each project to be awarded as a result of this Invitation To Bid solicitation. The successful Contractor shall furnish efficient Contractor reviews, business administration, field supervision and shall use his/her/its’ best efforts to perform the work in the best and most expeditious, economical manner consistent with the interests of the County, and in strict conformity with all funding requirements, State, Federal and local rules, laws and regulations. 

This ITB contains specific requests for information.  In responding to this ITB, Bidders are encouraged to provide additional information if Bidder believes that information is to be relevant. 



CONTRACT SUM
The Contract Sum is based upon the following combination of Bids and Bid alternates, if any, offered.  Base bid amounts include all parts, labor, material, equipment, supplies, design fees, licensure, permits, delivery, bonds, insurance, etc. required to design, furnish on Emergency Services Fully Equipped Ambulance. 

	Base Bid :				$ _________.00

	New Mexico Gross Receipt Tax:	(___%)	 $______________________
TOTAL NOT TO EXCEED FEE:
	The Owner shall pay the Contractor in current funds for the Contractor’s performance of the Contract the Contract Sum of ___________________________________ ($_________.00), excluding NMGRT, subject to additions and deductions as provided in the Contract Documents.
	Total compensation including NMGRT shall not exceed $___________________________________.


SUBCONTRACTOR LISTING:
	Contactor is required to identify each subcontractor to be engaged in this project for which the sub-contractor will perform services in an amount of $5,000 or more.  For each listed sub-contractor, Contractor is required to complete and submit the attached “Exhibit A – Attachment 1A, Subcontractor Listing Form”.
SUBSTANTIAL COMPLETION:
	The Contractor shall achieve Substantial Completion of the entire work not later than March 15, 2017 consecutive calendar days from the date of commencement, subject to adjustments of this Contract Time as provided in the Contract Documents.
LIQUIDATED DAMAGES:
	The Contractor agrees to pay as liquidated damages, the sum of two hundred Dollars ($200.00) for each consecutive calendar day after the stipulated contract time the work remains incomplete
Signature:_______________________________________________________________

Typed/Printed Name:________________________________________________________

Title:___________________________________________________________________

Date:__________________________________________

Phone:______________________________Fax:________________________________				
Company:_______________________________________________________________	

Address:________________________________________________________________	

City/State/Zip:____________________________________________________________





Subcontractor Listing Form
Pursuant to Section 13-4-34 of the New Mexico Procurement Code, the listing threshold for this Public Works Project is established at $5,000.00. Any person submitting a bid shall set forth: 
1. The name and location of the place of business of each subcontractor under subcontract to the contractor who will perform work or labor or render service to the contractor in or about the construction of the Public Works Construction Project in an amount in excess of the listing threshold; and 
2. The nature of the work which will be done by each subcontractor. List only one subcontractor for each category of work or trade. 
If my Quote is accepted, the following subcontractor(s) may perform work under this contract. (If you do not plan to utilize subcontractors, write "None".) 
Company Name: ________________________________DOL Reg. #__________________ 
Address: __________________________ City: _________________ State: _____ Zip: ________ 
E-Mail Address: ______________________License No: ______________________ 
Phone No.:_______________ Fax No.:_________________ 
Work to be performed ____________________________________________________________ 

Company Name: __________________________________DOL Reg. #__________________ 
Address: __________________________ City: _________________ State: _____ Zip: ________ 
E-Mail Address: ______________________License No: ______________________ 
Phone No.:_______________ Fax No.:_________________ 
Work to be performed ____________________________________________________________ 


 (Please complete each section. Use the entire company name, not just initials unless the initials are officially used in the company name. Use additional sheets if necessary.) 
RRPS must be notified of and must approve of any changes of proposed subcontractor(s) which may occur during the life of the Purchase Order for this Project. The Contractor shall be fully responsible for the work of the subcontractor(s), at any tier, to the full extent of the requirements of the Contract. 
(Make additional copies if necessary) 
Name of Contractor: _____________________________________ 
By: _______________________________________________ Date: ________________ 
[signature] 
Typed/Printed Name: ________________________________________________________ 
Title: _____________________________________________________________________ 
Date: __________________________________________ 
Phone: ______________________________Fax:_________________________________ 
Address: _________________________________________________________________ 
City/State/Zip: ____________________________________________________________ 



[bookmark: _Toc276819857][bookmark: _Toc276820937]APPENDIX B
[bookmark: _Toc276819858][bookmark: _Toc276820938]ACKNOWLEDGEMENT OF RECEIPT FORM
Invitation To Bid
SIERRA COUNTY ITB #2016-11-004
AUTOMOTIVE AMBULANCE
In acknowledgment of receipt of this Invitation To Bid, the undersigned agrees that he/she has received a complete copy of the above referenced ITB including all Appendix and Exhibits.
The acknowledgment of receipt should be signed and returned (by fax, e-mail, courier or hand delivery) to the County Procurement Officer no later than December 2, 2016.
The firm listed below does/does not (circle one) intend to respond to this Invitation To Bids.
FIRM: ___________________________________________________________
REPRESENTED BY:_______________________________________________ 
TITLE:___________________________________________________________
E-MAIL ADDRESS:________________________________________________
PHONE NO.:________________________  FAX NO: ____________________
ADDRESS:_______________________________________________________
CITY: _________________________ STATE: ______ ZIP CODE:__________
SIGNATURE: ____________________________________________________ DATE:__________________
This name and address will be used for all correspondence related to the Invitation To Bid.
Please return to:
Jocelyn Holguin, CPO
Sierra County Purchasing 
855 Van Patten
Truth or Consequences, NM 87901
Phone: (575) 894-6215
Fax: (575) 894-9548
E-mail: sierracountyprocurement@gmail.com


APPENDIX C

ACKNOWLEDGMENT OF ADDENDA

THE FOLLOWING BIDDER INFORMATION MUST BE COMPLETED AND RETURNED WITH THE ITB. 

ACKNOWLEDGMENT OF ADDENDA
The undersigned acknowledges receipt of the following addenda:

Addenda No.	 Dated	 Addenda No.	 Dated	

Addenda No.	 Dated	 Addenda No.	 Dated	

The undersigned, as an authorized representative for the Company named below, acknowledges that the Bidder has examined this ITB with its related documents and is familiar with all of the conditions surrounding the described materials, labor and/or services.  Bidder hereby agrees to furnish all labor, materials and supplies necessary to comply with the specifications in accordance with the Terms and Conditions set forth in this ITB and at the prices stated within the ITB.

The undersigned further states that the company submitting this ITB is not in violation of any applicable Conflict of Interest laws or regulations or any other related clauses included in this ITB.

COMPANY NAME	

ADDRESS	

CITY/STATE/ZIP	

TELEPHONE:	FAX:	EMAIL:	

NEW MEXICO GROSS RECEIPTS TAX NO	

FEDERAL EMPLOYER ID NUMBER (FEIN)	

NEW MEXICO LOCAL PREFERENCE NUMBER:__________________________

SIGNATURE OF AUTHORIZED REPRESENTATIVE	

PRINTED OR TYPED NAME	

TITLE	

DATE: _________________________________________________________________

                                   APPENDIX D
CONFLICT OF INTEREST-DEBARMENT/SUSPENSION CERTIFICATION FORM
SIERRA COUNTY CONFLICT OF INTEREST AND
DEBARMENT/SUSPENSION CERTIFICATION FORM
THE FOLLOWING MUST BE CERTIFIED IF ANY RESULTANT PURCHASE ORDER/AGREEMENT IS $20,000 OR GREATER

CONFLICT OF INTEREST; GOVERNMENTAL CONDUCT ACT.
	A.	The Contractor represents and warrants that it presently has no interest and, during the term of this Agreement, shall not acquire any interest, direct or indirect, which would conflict in any manner or degree with the performance or services required under the Agreement.  

	B.	The Contractor further represents and warrants that it has complied with, and, during the term of this Agreement, will continue to comply with, and that this Agreement complies with all applicable provisions of the Governmental Conduct Act, Chapter 10, Article 16 NMSA 1978.  Without in anyway limiting the generality of the foregoing, the Contractor specifically represents and warrants that:
		1)	in accordance with Section 10-16-4.3 NMSA 1978, the Contractor does not employ, has not employed, and will not employ during the term of this Agreement any County employee while such employee was or is employed by the County and participating directly or indirectly in the County’s contracting process; 
		2) 	this Agreement complies with Section 10-16-7(B) NMSA 1978 because (i) the Contractor is not a public officer or employee of the County; (ii) the Contractor is not a member of the family of a public officer or employee of the County; (iii) the Contractor is not a business in which a public officer or employee or the family of a public officer or employee has a substantial interest; or (iv) if the Contractor is a public officer or employee of the County, a member of the family of a public officer or employee of the County, or a business in which a public officer or employee of the County or the family of a public officer or employee of the County has a substantial interest, public notice was given as required by Section 10-16-7(B) NMSA 1978 and this Agreement was awarded pursuant to a competitive process; 
		3)	in accordance with Section 10-16-8(C) NMSA 1978, (i) the Contractor is not, and has not been represented by, a person who has been a public officer or employee of the County within the preceding year and whose official act directly resulted in this Agreement and (ii) the Contractor is not, and has not been assisted in any way regarding this transaction by, a former public officer or employee of the County whose official act, while in County employment, directly resulted in the County's making this Agreement; 
		4)	in accordance with Section 10-16-13 NMSA 1978, the Contractor has not directly participated in the preparation of specifications, qualifications or evaluation criteria for this Agreement or any procurement related to this Agreement; and
		5)	in accordance with Section 10-16-3 and Section 10-16-13.3 NMSA 1978, the Contractor has not contributed, and during the term of this Agreement shall not contribute, anything of value to a public officer or employee of the County.

	C.	Contractor’s representations and warranties in Paragraphs A and B of this Article 13 are material representations of fact upon which the County relied when this Agreement was entered into by the parties.  Contractor shall provide immediate written notice to the County if, at any time during the term of this Agreement, Contractor learns that Contractor’s representations and warranties in Paragraphs A and B of this Article 13 were erroneous on the effective date of this Agreement or have become erroneous by reason of new or changed circumstances. If it is later determined that Contractor’s representations and warranties in Paragraphs A and B of this Article 13 were erroneous on the effective date of this Agreement or have become erroneous by reason of new or changed circumstances, in addition to other remedies available to the County and notwithstanding anything in the Agreement to the contrary, the County may immediately terminate the Agreement.

	D.	All terms defined in the Governmental Conduct Act have the same meaning in this Article 13(B).

DEBARMENT/SUSPENSION STATUS 
The Vendor certifies that it is not suspended, debarred or ineligible from entering into contracts with the Executive Branch of the Federal Government, or in receipt of a notice or proposed debarment from any Agency. The vendor agrees to provide immediate notice to the County Chief Procurement Officer in the event of being suspended, debarred or declared ineligible by any department or federal agency, or upon receipt of a notice of proposed debarment that is received after the submission of the quote or Bid but prior to the award of the /Purchase Order/Agreement or contract. 

CERTIFICATION 
The undersigned hereby certifies that he/she has read the above CONFLICT OF INTEREST and DEBARMENT/SUSPENSION Status requirements and that he/she understands and will comply with these requirements. The undersigned further certifies that they have the authority to certify compliance for the vendor named and that the information contained in this document is true and accurate to the best of their knowledge. 
Signature: ______________________ Title: _________________Date: __________________ 
Name Typed: __________________________________
Company Name: ____________________________________________ 
Address ______________________________________ City/State/zip: 


APPENDIX E

CAMPAIGN CONTRIBUTION DISCLOSURE FORM

Pursuant to the Procurement Code, Sections 13-1-28, et seq., NMSA 1978 and  NMSA 1978, § 13-1-191.1 (2006), as amended by Laws of 2007, Chapter 234, any prospective contractor seeking to enter into a contract with any state agency or local public body for professional services, a design and build project delivery system, or the design and installation of measures the primary purpose of which is to conserve natural  resources must file this form with that state agency or local public body.  This form must be filed even if the contract qualifies as a small purchase or a sole source contract.  The prospective contractor must disclose whether they, a family member or a representative of the prospective contractor has made a campaign contribution to an applicable public official of the state or a local public body during the two years prior to the date on which the contractor submits an bid or, in the case of a sole source or small purchase contract, the two years prior to the date the contractor signs the contract, if the aggregate total of contributions given by the prospective contractor, a family member or a representative of the prospective contractor to the public official exceeds two hundred and fifty dollars ($250) over the two year period.

Furthermore, the state agency or local public body may cancel a solicitation or proposed award for a proposed contract pursuant to Section 13-1-181 NMSA 1978 or a contract that is executed may be ratified or terminated pursuant to Section 13-1-182 NMSA 1978 of the Procurement Code if: 1) a prospective contractor, a family member of the prospective contractor, or a representative of the prospective contractor gives a campaign contribution or other thing of value to an applicable public official or the applicable public official’s employees during the pendency of the procurement process or 2) a prospective contractor fails to submit a fully completed disclosure statement pursuant to the law. 

The state agency or local public body that procures the services or items of tangible personal property shall indicate on the form the name or names of every applicable public official, if any, for which disclosure is required by a prospective contractor.

THIS FORM MUST BE INCLUDED IN THE INVITATION TO BID AND MUST BE FILED BY ANY PROSPECTIVE CONTRACTOR WHETHER OR NOT THEY, THEIR FAMILY MEMBER, OR THEIR REPRESENTATIVE HAS MADE ANY CONTRIBUTIONS SUBJECT TO DISCLOSURE. 

The following definitions apply: 

“Applicable public official” means a person elected to an office or a person appointed to complete a term of an elected office, who has the authority to award or influence the award of the contract for which the prospective contractor is submitting a competitive sealed bid or who has the authority to negotiate a sole source or small purchase contract that may be awarded without submission of a sealed competitive bid.

“Campaign Contribution” means a gift, subscription, loan, advance or deposit of money or other thing of value, including the estimated value of an in-kind contribution, that is made to or received by an applicable public official or any person authorized to raise, collect or expend contributions on that official’s behalf for the purpose of electing the official to statewide or local office.  “Campaign Contribution” includes the payment of a debt incurred in an election campaign, but does not include the value of services provided without compensation or unreimbursed travel or other personal expenses of individuals who volunteer a portion or all of their time on behalf of a candidate or political committee, nor does it include the administrative or solicitation expenses of a political committee that are paid by an organization that sponsors the committee. 

“Family member” means spouse, father, mother, child, father-in-law, mother-in-law, daughter-in-law or son-in-law of (a) a prospective contractor, if the prospective contractor is a natural person; or (b) an owner of a prospective contractor.

“Pendency of the procurement process” means the time period commencing with the public notice of the Invitation To Bid and ending with the award of the contract or the cancellation of the Invitation To Bid. 

“Prospective contractor” means a person or business that is subject to the competitive sealed ITB process set forth in the Procurement Code or is not required to submit a competitive sealed bid because that person or business qualifies for a sole source or a small purchase contract.

“Representative of a prospective contractor” means an officer or director of a corporation, a member or manager of a limited liability corporation, a partner of a partnership or a trustee of a trust of the prospective contractor.

Name(s) of Applicable Public Official(s): Frances Luna, Ken Lyon, and Sherry Fletcher 

(Completed by State Agency or Local Public Body)

 DISCLOSURE OF CONTRIBUTIONS BY PROSPECTIVE CONTRACTOR:

Contribution Made By: __________________________________________

Relation to Prospective Contractor: ____________________________________

Date Contribution(s) Made: __________________________________________
										
Amount(s) of Contribution(s)		__________________________________________
										
Nature of Contribution(s)		__________________________________________
					
					__________________________________________
										
Purpose of Contribution(s)		__________________________________________
					
					__________________________________________
										
(Attach extra pages if necessary)

___________________________	_______________________
Signature				Date

___________________________
Title (position)

--OR--

NO CONTRIBUTIONS IN THE AGGREGATE TOTAL OVER TWO HUNDRED FIFTY DOLLARS ($250) WERE MADE to an applicable public official by me, a family member or representative.


______________________________		_______________________
Signature							Date 

______________________________
Title (Position)







APPENDIX F

RESIDENT VETERANS PREFERENCE CERTIFICATION

 	(NAME OF CONTRACTOR) hereby certifies the following in regard to application of the resident veterans' preference to this procurement:

PLEASE CHECK ONLY ONE BOX FROM THE (2) CHECK BOXES LISTED BELOW:

___ I declare that my firm is ineligible to receive New Mexico Resident Veterans Preference.

Please Indicate: Veteran Preference_________ 10% under $3 Million
                           Local Preference: __________5%
AN ACT
RELATING TO PROCUREMENT; AMENDING THE RESIDENT VETERAN BUSINESS PREFERENCE; REPEALING LAWS 2012, CHAPTER 56, SECTION 2 AND LAWS 2012, CHAPTER 56, SECTION 6.
        BE IT ENACTED BY THE LEGISLATURE OF THE STATE OF NEW MEXICO: SECTION 1. Section 13-1-21 NMSA 1978 (being Laws 1979, Chapter 72, Section 1, as amended) is amended to read: "13-1-21. APPLICATION OF PREFERENCES.--
A. For the purposes of this section:
(1) "business" means a commercial enterprise carried on for the purpose of selling goods or services, including growing, producing, processing or distributing agricultural products;
(2) "formal bid process" means a competitive bid process;
(3) "formal request for proposals process" means a competitive proposal process, including a competitive qualifications-based proposal process;
(4)  "public body" means a department, commission, council, board, committee, institution, legislative body, agency, government corporation, educational institution or official of the executive, legislative or judicial branch of the government of the state or a political subdivision of the state and the agencies, instrumentalities and institutions thereof, including two-year post-secondary educational institutions, school districts, local school boards and all municipalities, including home-rule
municipalities;
(5) "recycled content goods" means supplies and materials composed twenty-five percent or more of recycled materials; provided that the recycled materials content meets or exceeds the minimum content standards required by bid specifications;
(6) "resident business" means a business that has a valid resident business certificate issued by the taxation and revenue department pursuant to Section 13-1-22 NMSA 1978 but does not include a resident veteran business; and
(7) "resident veteran business" means a business that has a valid resident veteran business certificate issued by the taxation and revenue department pursuant to Section 13-1-22 NMSA 1978.
B. Except as provided in Subsection C of this section, when a public body makes a purchase using a formal bid process, the public body shall deem a bid submitted by a:
(1) resident business to be five percent lower than the bid actually submitted; or
(2) resident veteran business with annual gross revenues of up to three million dollars ($3,000,000) in HB 93 the preceding tax year to be ten percent lower than the bid actually submitted.
C. When a public body makes a purchase using a formal bid process and the bids are received for both recycled content goods and non-recycled content goods, the public body shall deem:
(1) bids submitted for recycled content goods from any business, except a resident veteran business, to be five percent lower than the bids actually submitted; or
(2) bids submitted for recycled content goods from a resident veteran business with annual gross revenues of up to three million dollars ($3,000,000) in the preceding tax year to be ten percent lower than the bids actually submitted.
D. When a public body makes a purchase using a formal request for proposals process, not including contracts awarded on a point-based system, the public body shall award an additional:
(1) five percent of the total weight of all the factors used in               evaluating the proposals to a resident business; and
(2) ten percent of the total weight of all the factors used in evaluating the proposals to a resident veteran business that has annual gross revenues of up to
three million dollars ($3,000,000) in the preceding tax year. HB 93
E. When a public body makes a purchase using a formal request for proposals process, and the contract is awarded based on a point-based system, the public body shall award additional points equivalent to:
(1) five percent of the total possible points to a resident business; or
(2) ten percent of the total possible points to a resident veteran business that has annual gross revenues of up to three million dollars ($3,000,000) in the preceding tax year.
F. When a joint bid or joint proposal is submitted by a combination of resident veteran, resident or nonresident businesses, the preference provided pursuant to Subsection B, C, D or E of this section shall be calculated in proportion to the percentage of the contract, based on the dollar amount of the goods or services provided under the contract, that will be performed by each business as specified in the joint bid or proposal.
G. A resident veteran business shall not benefit from the preference pursuant to this section for more than ten consecutive years. A person that is an owner of a business that is a resident veteran business shall not benefit from the preference pursuant to this section for more than ten consecutive years. A person shall not benefit from the provisions of this section based on more than one business concurrently.
H. A public body shall not award a business both a resident business preference and a resident veteran business preference.
I. The procedures provided in Sections 13-1-172 through 13-1-183 NMSA 1978 or in an applicable purchasing ordinance apply to a protest to a public body concerning the awarding of a contract in violation of this section.
J. This section shall not apply when the expenditure includes federal funds for a specific purchase." SECTION 2. Section 13-4-2 NMSA 1978 (being Laws 1984, Chapter 66, Section 2, as amended) is amended to read: "13-4-2. APPLICATION OF PREFERENCE.--
A. For the purposes of this section:
(1) "formal bid process" means a competitive sealed bid process;
(2) "formal request for proposals process" means a competitive sealed proposal process, including a competitive sealed qualifications-based proposal process;
(3) "public body" means a department, commission, council, board, committee, institution, legislative body, agency, government corporation, educational institution or official of the executive, legislative or judicial branch of the government of the state or a political subdivision of the state and the agencies, instrumentalities and institutions thereof, including two-year post-secondary educational institutions, school districts, local school boards and all municipalities, including home-rule municipalities;
(4) "public works contract" means a contract for construction, construction management, architectural, landscape architectural, engineering, surveying or interior design services;
(5) "resident contractor" means a person that has a valid resident contractor certificate issued by the taxation and revenue department pursuant to Section 13-1-22 NMSA 1978 but does not include a resident veteran contractor; and
(6) "resident veteran contractor" means a person that has a valid resident veteran contractor certificate issued by the taxation and revenue department pursuant to Section 13-1-22 NMSA 1978.
B. For the purpose of awarding a public works contract using a formal bid process, a public body shall deem a bid submitted by a:
(1) resident contractor to be five percent lower than the bid actually submitted; or
(2) resident veteran contractor with annual gross revenues of up to three million dollars ($3,000,000) in the preceding tax year to be ten percent lower than the bid
actually submitted.
C. When a public body awards a contract using a formal request for proposals process, not including contracts awarded on a point-based system, the public body shall award an additional:
(1) five percent of the total weight of all the factors used in evaluating the proposals to a resident contractor; or
(2) ten percent of the total weight of all the factors used in evaluating the proposals to a resident veteran contractor that has annual gross revenues of up to three million dollars ($3,000,000) in the preceding tax year.
D. When a public body makes a purchase using a formal request for proposals process, and the contract is awarded based on a point-based system, the public body shall award an additional of the equivalent of:
(1) five percent of the total possible points to a resident contractor; or
(2) ten percent of the total possible points to a resident veteran contractor that has annual gross revenues of up to three million dollars ($3,000,000) in the preceding tax year.
E. When a joint bid or joint proposal is submitted by a combination of resident veteran, resident or nonresident contractors, the preference provided pursuant to Subsection
B, C or D of this section shall be calculated in proportion to the percentage of the contract, based on the dollar amount of the goods or services provided under the contract that will be performed by each contractor as specified in the joint bid or joint proposal.
F. A resident veteran contractor shall not benefit from the preference pursuant to this section for more than ten consecutive years. A person that is an owner of a business that is a resident veteran contractor shall not benefit from the preference pursuant to this section for more than ten consecutive years. A person shall not benefit from the provisions of this section based on more than one business concurrently.
G. A public body shall not award a contractor both a resident contractor preference and a resident veteran contractor preference.
H. The procedures provided in Sections 13-1-172 through 13-1-183 NMSA 1978 or in an applicable purchasing ordinance apply to a protest to a public body concerning the awarding of a contract in violation of this section." SECTION 3. A new section of the Procurement Code is enacted to read:
"DUTY TO PROMULGATE RULES.--The secretary of general services shall promulgate rules necessary to implement the provisions of this 2016 act."
SECTION 4. REPEAL.--Laws 2012, Chapter 56, Section 2 and Laws 2012, Chapter 56, Section 6 are repealed.
SECTION 5. EFFECTIVE DATE.--The effective date of the provisions of this act is July 1, 2016.	
"I agree to submit a report, or reports, to the State Purchasing Division of the General Services Department declaring under penalty of perjury that during the last calendar year starting January 1 and ending on December 31, the following to be true and accurate:
"In conjunction with this procurement and the requirements of this business' application for a Resident Veteran Business Preference/Resident Veteran Contractor Preference under Sections 13-1-21 or 13-1-22 NMSA 1978, when awarded a contract which was on the basis of having such veterans preference, I agree to report to the State Purchasing Division of the General Services Department the awarded amount involved. I will indicate in the report the award amount as a purchase from a public body or as a public works contract from a public body as the case may be.
"I understand that knowingly giving false or misleading information on this report constitutes a crime."
I declare under penalty of perjury that this statement is true to the best of my knowledge. I understand that giving false or misleading statements about material fact regarding this matter constitutes a crime.

(Signature of Business Representative)*                                        (Date)                                                
*Must be an authorized signatory for the Business.
The representations made in checking the boxes constitutes a material representation by the business that is subject to protest and may result in denial of an award or un-award of the procurement involved if the statements are    proven to   be    incorrect.


APPENDIX G
LOCAL PREFERNCE

Sierra County Preference Certificate
	
	

	
	855 Van Patten, T or C, NM 87901 | (575) 894-6215 | Fax (575)9548


description Appendix g
	
	

	
	The phrase “Sierra County Business” shall mean a business that has its primary and permanent office or business location or primarily conducts its business within the boundaries of Sierra County for at least one  (1) year preceding the submission of an application for a Sierra County procurement preference, and which, if a foreign corporation, has filed a unitary return pursuant to the Corporate Income and Franchise Tax Act and NMSA 1978, Section 7-2A-8.3 at the time of application for a preference certificate. Whereas, local businesses pay local Gross Receipt Taxes, spend their dollars locally, and reinvest in the community. All applicants will be reviewed and by the Procurement Manager. 




Eligibility OF THE SIERRA COUNTY PROCUREMENT PREFERENCE 
	
	

	
	SIERRA COUNTY BUISNESS 
A Sierra County Business shall be eligible to claim the 0.99% preference established only when presenting, prior to or at the time established in the solicitation for receipt of proposals or invitations for bids, a Sierra County Preference Certificate is issued by the Procurement Manager. 

	
	Application Fee
$25.00- Non Refundable- Does Not Guarantee Acceptance.  
EXPERATION OF CERTIFICATE 
A Preference Certificate shall be valid for four (4) years from the date of its issue or once the applicant no longer meets the criteria. 
DENIAL OF CERTIFICATE; PROTEST; REVOCATION
1. Purchasing Manager shall determine if an applicant is eligible for certification.
2. If application is denied a notice of denial shall be issued. 
3. A business whose application for a Preference Certificate is denied may protest the denial to the Procurement Manager in conformity with the protest procedure of the Sierra County Purchasing Policy. 
4. Through developing facts the Procurement Manager will revoke the certificate and notify the applicate, if the information provided is inaccurate or misleading information.


obtaining a  LOCAL preference certificate
	
	

	
	DATE: __________________________________________
COMPANY NAME: _________________________________________________
CONTACT PERSON: ________________________________________________
PHONE NUMBER:  (            )                   -
EMAIL ADDRESS: _________________________________________________
Please, check appropriate answer:

	
	1. ______YES _______NO is your business registered in the State of New Mexico and in good standing? 
 
2. ______YES _______NO has your business been established within the boundaries of Sierra County for longer than (1) year? (A copy of the business Gross Receipt Tax Return for the year preceding must be attached to application. Income amounts and taxes paid may be redacted).


3. ______YES _______NO Do you have a valid municipal business license? (A copy must be attached to application to be considered). 

4. ______YES _______NO Are you a foreign corporation? – If so, copies of the most recent State and Federal Tax returns applicable to the business. 


	
	

	
	


Certificate	
	
	



Once all requirements are met and verified, a Certificate from the County of Sierra will be issued to you and business. Thank you for your submission. 






EXHIBIT A

ITB Question Submittal Form

ITB# 2015-11-004

All written questions must be addressed to the Buyer for this ITB.  Bidders are to submit written questions using the format below.  Written responses to the questions received will be distributed by Sierra County Procurement Agent as addenda to this ITB solicitation.


	Question #
	Reference Page/Paragraph/Sec
	Question

	1
	
	

	2
	
	

	3
	
	

	4
	
	

	5
	
	

	6
	
	

	7
	
	

	8
	
	

	9
	
	

	10
	
	





 
EXHIBIT B

INSURANCE REQUIREMENTS

CERTIFICATES OF INSURANCE:
The Contractor shall furnish the Owner one copy each of Certificates of insurance herein required for each copy of the Purchase Order/Agreement showing coverage, limits of liability, covered operations, effective dates of expiration of policies of insurance carried by the Contractor.  The Contractor shall furnish to the Owner copies of limits.  The Certificate of Insurance shall be in the form of AIA Document G-705 or similar format acceptable to the Owner. Such certificates shall be filed with the Owner and shall also contain the following statements:

“Sierra County Commissioners, Sierra County its agents, servants and employee are held as additional insured.”

“The insurance coverage certified herein shall not be canceled or materially changed except after forty five (45) days written notice has been provided to the owner.”

COMPENSATION INSURANCE:
The Contractor shall procure and shall maintain during the life of this contract Worker’s Compensation as required by applicable State law for all Contractor’s employees to be engaged at the site of the project under this project and in case of any such work sublet the Contractor shall require the subcontractor or sub subcontractor similarly to provide Worker’s Compensation Insurance for all the subcontractor’s or sub subcontractor’s Workers which are covered under the Contractor’s Worker’s Compensation Insurance.  In case any class of employee engaged in work on the project under this contract is not protected under a Worker’s Compensation Status, the Contractor shall provide and shall cause each subcontractor or sub subcontractor to provide Employer’s insurance in any amount of not less than $500,000.

CONTRACTOR’S PUBLIC LIABILITY INSURANCE
The contractor shall procure and shall maintain during the life of this contract Public Liability Insurance as required by applicable State law.  In case of any work being sublet, the Contractor shall require the subcontractor or sub-subcontractor similarly to provide Public Liability Insurance for all the subcontractor’s or sub-subcontractor’s work being performed under this Purchase Order/Agreement.  In any case, whereby the Contractor’s sub-contractor or sub-subcontractor services are not covered under separate policy, the Contractor shall provide and shall cause each subcontractor or Sub-subcontractor to be covered under the contractor’s policy.  The insurance must remain in force for the life of the contract including all contract extensions or renewals. The limits effective June 8, 2012 are:

$1,000,000 per occurrence; $1,000,000 annual aggregate.






CONTRACTOR’S VEHICLE LIABILITY INSURANCE:
The Contractor shall procure and shall maintain during the life of this contract Vehicle Liability Insurance coverage “equal to the maximum liability amounts set forth in the New Mexico Tort Claims Act Section 41-4-1 et.seq. NMSA 1978.”  The insurance must remain in force for the life of the contract including all contract extensions or renewals. The limits effective July 1, 1992 are:

Bodily Injury	$750,000 Each Occurrence
Property Damage	$100,000 Each Occurrence

SUBCONTRACTOR’S AND SUB CONTRACOTR’S PUBLIC AND VEHICLE LIABILITY INSURANCE:
The Contractor shall either:
1. Require each subcontractor or sub-contractor to procure and maintain during the life of the subcontract or sub subcontract public Liability Insurance of the types and amounts specified above or, 
2. Insure the activities of the subcontractors of sub subcontractors in the Contractor’s Policy as required under this Article.

GENERAL:
All Insurance policies are to be issued by companies authorized to do business under the laws of the state in which work is to be done and acceptable to owner.

The Contractor shall not violate, permit to be violated, any conditions of any said policies, and shall at all times satisfy the requirements for the insurance companies writing said policies.

PROFESSIONAL LIABILITY:
Minimum limits: $1,000,000 per occurrence and $3,000,000 aggregate.

The Vendor shall procure and shall maintain during the life of this contract Professional Liability insurance as required by applicable State law.  In case of any work being sublet, the Vendor shall require the subcontractor or sub-subcontractor similarly to provide professional liability Insurance for all the subcontractor’s or sub-subcontractor’s work being performed under this agreement.  In any case whereby the Vendor’s sub-contractors or sub-subcontractors services are not covered under separate policy, the Vendor shall provide and shall cause each subcontractor or sub-subcontractor to be covered under the Vendor’s








SIERRA COUNTY
SAMPLE CONTRACT #2016-11-004

THIS AGREEMENT is made and entered into by and between the County of Sierra, hereinafter referred to as the "County" and NAME OF CONTRACTOR, hereinafter referred to as the "Contractor”, and is effective as of the date set forth below upon which it is executed by the Chief Procurement Officer and the Board of County Commissioners.
 

IT IS AGREED BETWEEN THE PARTIES:

1.	Scope of Work.
	The Contractor shall perform the work outlined in the Scope of Work attached hereto as Attachment 1 and incorporated herein by reference.

2.	Compensation.
	A.	The County shall pay to the Contractor in full payment for services satisfactorily 
performed ______________ dollars ($__________) annually, to be invoiced in equal monthly amounts after performance of the services. The New Mexico gross receipts tax levied on the amounts payable under this Agreement totaling (AMOUNT) shall be paid by the County to the Contractor in equal monthly amounts. The total amount payable to the Contractor under this Agreement, including gross receipts tax and expenses, shall not exceed (AMOUNT).  In no event will the Contractor be paid any amount in excess of the specified total amount payable without this Agreement being amended in writing.

	B.	Payment is subject to availability of funds pursuant to the Appropriations Paragraph set forth below and to any negotiations between the parties from year to year pursuant to Paragraph 1, Scope of Work.  All invoices MUST BE received by the County no later than fifteen (15) days after the termination of the Fiscal Year in which the services were delivered.  Invoices received after such date WILL NOT BE PAID.
		  
	C. 	Contractor must submit a detailed statement accounting for all services performed, specified on a minimum of a quarter hour basis, and expenses incurred.  If the County finds that the services are not acceptable, within thirty days after the date of receipt of written notice from the Contractor that payment is requested, it shall provide the Contractor a letter of exception explaining the defect or objection to the services, and outlining steps the Contractor may take to provide remedial action.  Upon certification by the County that the services have been received and accepted, payment shall be tendered to the Contractor within thirty days after the date of acceptance. If payment is made by mail, the payment shall be deemed tendered on the date it is postmarked.  However, the County shall not incur late charges, interest, or penalties for failure to make payment within the time specified herein.
		  
	D. 	The payment of taxes due for any money received under this Agreement shall be the Contractor's sole responsibility and shall be reported under the Contractor's Federal and State tax identification number(s).

3.	Term.
	This Agreement is for one (1) year from the date of approval by the Sierra County Board of County Commissioners. One (1) year term unless terminated pursuant to paragraph 4 (Termination), or paragraph 5 (Appropriations).  In accordance with Section 13-1-150 NMSA 1978, no term for a professional services contract, including extensions and renewals, shall exceed four years, except as set forth in Section 13-1-150 NMSA 1978.  

4.	Termination.
	A.	Termination.  This Agreement may be terminated by either of the parties hereto upon written notice delivered to the other party at least thirty (30) days prior to the intended date of termination.  Except as otherwise allowed or provided under this Agreement, the County’s sole liability upon such termination shall be to pay for acceptable work performed prior to the Contractor’s receipt of the notice of termination, if the County is the terminating party, or the Contractor’s sending of the notice of termination, if the Contractor is the terminating party; provided, however, that a notice of termination shall not nullify or otherwise affect either party’s liability for pre-termination defaults under or breaches of this Agreement.  The Contractor shall submit an invoice for such work within thirty (30) days of receiving or sending the notice of termination.  Notwithstanding the foregoing, this Agreement may be terminated immediately upon written notice to the Contractor if the Contractor becomes unable to perform the services contracted for, as determined by the County or if, during the term of this Agreement, the Contractor or any of its officers, employees or agents is indicted for fraud, embezzlement or other crime due to misuse of government funds or due to the Appropriations paragraph herein. THIS PROVISION IS NOT EXCLUSIVE AND DOES NOT WAIVE THE COUNTY’s OTHER LEGAL RIGHTS AND REMEDIES CAUSED BY THE CONTRACTOR'S DEFAULT/BREACH OF THIS AGREEMENT.

	B	Termination Management.  Immediately upon receipt by either the County or the
Contractor of notice of termination of this Agreement, the Contractor shall: 1) not incur any further obligations for salaries, services or any other expenditure of funds under this Agreement without written approval of the County; 2) comply with all directives issued by the County in the notice of termination as to the performance of work under this Agreement;  and 3) take such action as the County shall direct for the protection, preservation, retention or transfer of all property titled to the County and records generated under this Agreement. Any non-expendable personal property or equipment provided to or purchased by the Contractor with contract funds shall become property of the County upon termination and shall be submitted to the County as soon as practicable.  

5.	Appropriations.
	The terms of this Agreement are contingent upon sufficient appropriations and authorization being made by the Board of County Commissioners for the performance of this Agreement.  If sufficient appropriations and authorization are not made by the Board of County Commissioners, this Agreement shall terminate immediately upon written notice being given by the County to the Contractor. The County's decision as to whether sufficient appropriations are available shall be accepted by the Contractor and shall be final. If the County proposes an amendment to the Agreement to unilaterally reduce funding, the Contractor shall have the option to terminate the Agreement or to agree to the reduced funding, within thirty (30) days of receipt of the proposed amendment.

6.	Status of Contractor.
	The Contractor and its agents and employees are independent contractors performing professional services for the County and are not employees of the County of Sierra. The Contractor and its agents and employees shall not accrue leave, retirement, insurance, bonding, use of county vehicles, or any other benefits afforded to employees of the County of Sierra as a result of this Agreement.  The Contractor acknowledges that all sums received hereunder are reportable by the Contractor for tax purposes, including without limitation, self-employment and business income tax.  The Contractor agrees not to purport to bind the County of Sierra unless the Contractor has express written authority to do so, and then only within the strict limits of that authority.

7.	Assignment.
	The Contractor shall not assign or transfer any interest in this Agreement or assign any claims for money due or to become due under this Agreement without the prior written approval of the County.

8.	Subcontracting.
	The Contractor shall not subcontract any portion of the services to be performed under this Agreement without the prior written approval of the County. No such subcontract shall relieve the primary Contractor from its obligations and liabilities under this Agreement, nor shall any subcontract obligate direct payment from the County. In all cases, the contractor is solely responsible for fulfillment of this Agreement.

9.	Release.
	Final payment of the amounts due under this Agreement shall operate as a release of the procuring agency of the County, its officers and employees, and the County of Sierra from all liabilities, claims and obligations whatsoever arising from or under this Agreement.  

10.	Confidentiality.
	Any confidential information provided to or developed by the Contractor in the performance of this Agreement shall be kept confidential and shall not be made available to any individual or organization by the Contractor without the prior written approval of the County. 



11.	Product of Service -- Copyright.
	All materials developed or acquired by the Contractor under this Agreement shall become the property of the County of Sierra and shall be delivered to the County no later than the termination date of this Agreement.  Nothing developed or produced, in whole or in part, by the Contractor under this Agreement shall be the subject of an application for copyright or other claim of ownership by or on behalf of the Contractor.

12.	Conflict of Interest; Governmental Conduct Act.
	A.	The Contractor represents and warrants that it presently has no interest and, during the term of this Agreement, shall not acquire any interest, direct or indirect, which would conflict in any manner or degree with the performance or services required under the Agreement.  

	B.	The Contractor further represents and warrants that it has complied with, and, during the term of this Agreement, will continue to comply with, and that this Agreement complies with all applicable provisions of the Governmental Conduct Act, Chapter 10, Article 16 NMSA 1978.  Without in anyway limiting the generality of the foregoing, the Contractor specifically represents and warrants that:
		1)	in accordance with Section 10-16-4.3 NMSA 1978, the Contractor does not employ, has not employed, and will not employ during the term of this Agreement any County employee while such employee was or is employed by the County and participating directly or indirectly in the County’s contracting process; 
		2) 	this Agreement complies with Section 10-16-7(B) NMSA 1978 because (i) the Contractor is not a public officer or employee of the County; (ii) the Contractor is not a member of the family of a public officer or employee of the County; (iii) the Contractor is not a business in which a public officer or employee or the family of a public officer or employee has a substantial interest; or (iv) if the Contractor is a public officer or employee of the County, a member of the family of a public officer or employee of the County, or a business in which a public officer or employee of the County or the family of a public officer or employee of the County has a substantial interest, public notice was given as required by Section 10-16-7(B) NMSA 1978 and this Agreement was awarded pursuant to a competitive process; 
		3)	in accordance with Section 10-16-8(C) NMSA 1978, (i) the Contractor is not, and has not been represented by, a person who has been a public officer or employee of the County within the preceding year and whose official act directly resulted in this Agreement and (ii) the Contractor is not, and has not been assisted in any way regarding this transaction by, a former public officer or employee of the County whose official act, while in County employment, directly resulted in the County's making this Agreement; 
		4)	in accordance with Section 10-16-13 NMSA 1978, the Contractor has not directly participated in the preparation of specifications, qualifications or evaluation criteria for this Agreement or any procurement related to this Agreement; and
		5)	in accordance with Section 10-16-3 and Section 10-16-13.3 NMSA 1978, the Contractor has not contributed, and during the term of this Agreement shall not contribute, anything of value to a public officer or employee of the County.

	C.	Contractor’s representations and warranties in Paragraphs A and B of this Article 12 are material representations of fact upon which the County relied when this Agreement was entered into by the parties.  Contractor shall provide immediate written notice to the County if, at any time during the term of this Agreement, Contractor learns that Contractor’s representations and warranties in Paragraphs A and B of this Article 12 were erroneous on the effective date of this Agreement or have become erroneous by reason of new or changed circumstances. If it is later determined that Contractor’s representations and warranties in Paragraphs A and B of this Article 12 were erroneous on the effective date of this Agreement or have become erroneous by reason of new or changed circumstances, in addition to other remedies available to the County and notwithstanding anything in the Agreement to the contrary, the County may immediately terminate the Agreement.

	D.	All terms defined in the Governmental Conduct Act have the same meaning in this Article 12(B).

13.	Amendment.
	This Agreement shall not be altered, changed or amended except by instrument in writing executed by the parties hereto and all other required signatories.

14.	Merger.
	This Agreement incorporates all the Agreements, covenants and understandings between the parties hereto concerning the subject matter hereof, and all such covenants, Agreements and understandings have been merged into this written Agreement.  No prior Agreement or understanding, oral or otherwise, of the parties or their agents shall be valid or enforceable unless embodied in this Agreement.

15.	Penalties for violation of law.
	The Procurement Code, Sections 13-1-28 through 13-1-199, NMSA 1978, imposes civil and criminal penalties for its violation.  In addition, the New Mexico criminal statutes impose felony penalties for illegal bribes, gratuities and kickbacks.

16.	Equal Opportunity Compliance.
	The Contractor agrees to abide by all federal, state and county laws and rules and regulations, pertaining to equal employment opportunity.  In accordance with all such laws, the Contractor assures that no person in the United States shall, on the grounds of race, religion, color, national origin, ancestry, sex, age, physical or mental handicap, or serious medical condition, spousal affiliation, sexual orientation or gender identity, be excluded from employment with or participation in, be denied the benefits of, or be otherwise subjected to discrimination under any program or activity performed under this Agreement.  If Contractor is found not to be in compliance with these requirements during the life of this Agreement, Contractor agrees to take appropriate steps to correct these deficiencies.

17.	Applicable Law.
	In any action, suit or legal dispute arising from this Agreement, the Contractor agrees that the laws of the State of New Mexico shall govern and that venue will lie in the Seventh Judicial District Court in Sierra County. By execution of this Agreement, Contractor acknowledges and agrees to the jurisdiction of the courts of the State of New Mexico over any and all lawsuits arising under or out of any term of this Agreement.

18.	Workers Compensation.
	The Contractor agrees to comply with state laws and rules applicable to workers compensation benefits for its employees. If the Contractor fails to comply with the Workers Compensation Act and applicable rules when required to do so, this Agreement may be terminated by the County.

19.	Records and Financial Audit.
	The Contractor shall maintain detailed time and expenditure records that indicate the date; time, nature and cost of services rendered during the Agreement’s term and effect and retain them for a period of three (3) years from the date of final payment under this Agreement.  The records shall be subject to inspection by the County, the Department of Finance and Administration and the State Auditor.  The County shall have the right to audit billings both before and after payment.  Payment under this Agreement shall not foreclose the right of the County to recover excessive or illegal payments

20.	Disclaimer and Hold Harmless.
	Sierra County shall not be liable to the Contractor, or the Contractor’s successors, heirs, administrators, or assigns, for any loss, damage, or injury, whether to Contractor's person or property, occurring in connection with Contractor's performance of Contractor's duties according to this Agreement.  Contractor shall hold the Sierra County harmless from all loss, damage, and injury, including court costs and attorney fees, incurred by Sierra County in connection with the performance by Contractor of Contractor's duties according to this Agreement.

21.	Indemnification.
	The Contractor shall defend, indemnify and hold harmless the County of Sierra from all actions, proceeding, claims, demands, costs, damages, attorneys’ fees and all other liabilities and expenses of any kind from any source which may arise out of the performance of this Agreement, caused by the negligent act or failure to act of the Contractor, its officers, employees, servants, subcontractors or agents, or if caused by the actions of any client of the Contractor resulting in injury or damage to persons or property during the time when the Contractor or any officer, agent, employee, servant or subcontractor thereof has or is performing services pursuant to this Agreement.  In the event that any action, suit or proceeding related to the services performed by the Contractor or any officer, agent, employee, servant or subcontractor under this Agreement is brought against the Contractor, the Contractor shall, as soon as practicable but no later than two (2) days after it receives notice thereof, notify the legal counsel of the County of Sierra and the New Mexico Association of Counties by certified mail.

22.	Invalid Term or Condition.
	If any term or condition of this Agreement shall be held invalid or unenforceable, the remainder of this Agreement shall not be affected and shall be valid and enforceable.

23.	Enforcement of Agreement.
	A party's failure to require strict performance of any provision of this Agreement shall not waive or diminish that party's right thereafter to demand strict compliance with that or any other provision.  No waiver by a party of any of its rights under this Agreement shall be effective unless express and in writing, and no effective waiver by a party of any of its rights shall be effective to waive any other rights.


24.	Authority.
	If Contractor is other than a natural person, the individual(s) signing this Agreement on behalf of Contractor represents and warrants that he or she has the power and authority to bind Contractor, and that no further action, resolution, or approval from Contractor is necessary to enter into a binding contract. 

25.       Lobbying.
No federal appropriated funds can be paid or will be paid, by or on behalf of the CONTRACTOR, or any person for influencing or attempting to influence an officer or employee of any County, a Member of Congress, an officer or employee of Congress, or an employee of a Member of Congress in connection with the awarding of any Federal contract, or the making of any Federal grant, the making of any federal loan, the entering into of any cooperative agreement, or modification of any Federal contract, grant, loan, or cooperative agreement.  If any funds other than federal appropriated funds have been paid or will be paid to any person influencing or attempting to influence an officer or employee of any County, a Member of Congress, an officer or employee of Congress, or an employee of a Member of Congress in connection of this federal contract, grant, loan, or cooperative agreement, the CONTRACTOR shall complete and submit Standard Form LLL, “Disclosure Form to Report Lobbying,” in accordance with its instructions.

26.	Approval of Contractor Personnel.
Personnel proposed in the Contractor's written proposal to the County are considered material to any work performed under this Agreement. No changes of personnel will be made by the Contractor without prior written consent of the procuring agency of the County.  Replacement of any Contractor personnel, if approved, shall be with personnel of equal ability, experience and qualifications.  The Contractor will be responsible for any expenses incurred in familiarizing the replacement personnel to insure their being productive to the project immediately upon receiving assignments.  Approval of replacement personnel shall not be unreasonably withheld. The procuring agency of the County shall retain the right to request the removal of any of the Contractor's personnel at any time. 

27.	Survival.
The agreement paragraphs titled “Patent, Copyright, Trademark, and Trade Secret Indemnification” and “Indemnification” shall survive the expiration of this agreement. Software licenses, leases, maintenance and any other unexpired agreements that were entered into under the terms and conditions of this agreement shall survive this agreement

28.	Succession.
This agreement shall extend to and be binding upon the successors and assigns of the parties.


29.	Force Majeure.
A party shall be excused from performance under this agreement for any period that the party is prevented from performing as a result of an act of God, strike, war, civil disturbance, epidemic, or court order, provided that the party has prudently and promptly acted to take any and all steps that are within the party's control to ensure performance.  Subject to this provision, such non-performance shall not be deemed a default or a ground for termination.


30.	Mediation.
	In the event a dispute arises as to the rights and obligations among the parties hereto, the parties agree to attempt to resolve the dispute through mediation as a condition precedent to seeking legal and equitable remedies.   The parties agree to evenly split the costs of any such mediation services.  The parties shall mutually agree upon the choice of mediator.  In the event the parties have not agreed upon a mediator within twenty (20) days of written notice to the other regarding the dispute, then a list of seven potential mediators will be obtained from the New Mexico Association of Counties and the parties shall utilize a striking process until a mediator is agreed upon.

31.	Notice to Proceed.
It is expressly understood that this Agreement is not binding upon the County until it is executed by the Board of County Commissioners after voting on the contract at a public meeting. Further, the Contractor is not to proceed with its obligations under the Agreement until the Contractor has received a fully signed copy of the Agreement.

32.	Attorney’s Fees.
In the event this Agreement results in dispute, mediation, litigation, or settlement between the parties to this Agreement, the prevailing party of such action shall NOT be entitled to an award of attorneys' fees and court costs.

33.	Cooperation.
All parties hereto will fully cooperate with the other and their respective counsel, accountant, and agents in connection with any steps required to be taken under this Agreement.

34.	Incorporation and Order of Precedence.
Request for Proposals No. [2016-11-004] and the contractor's proposal are incorporated by reference into this agreement and are made a part of this agreement. In the event of any conflict among these documents, the following order of precedence shall apply:

1.	Any contract amendment(s), in reverse chronological order; then
2.	this contract itself; then
3.	the Request for Proposals; then
4.	the Contractors Best and Final Offer(s), in reverse chronological order; then
5.	the contractor’s proposal; then
6.	the contractor's standard agreement terms and conditions (which may or may not 
	have been submitted as part of the contractor's proposal).

35.	Patent, Copyright, Trademark and Trade Secret Indemnification.

A.	The contractor shall defend, at its own expense, the County of Sierra against any claim that any product or service provided under this agreement infringes any patent, copyright or trademark in the United States or Puerto Rico, and shall pay all costs, damages and attorneys' fees that a court finally awards as a result of any such claim.  In addition, if any third party obtains a judgment against the County of Sierra based upon the contractor's trade secret infringement relating to any product or service provided under this agreement, the contractor agrees to reimburse the County of Sierra for all costs, attorneys' fees and the amount of the judgment.  To qualify for such defense and/or payment, the County of Sierra shall:

i.	give the contractor prompt written notice of any claim;

ii.	allow the contractor to control the defense or settlement of the claim; and

iii.	cooperate with the contractor in a reasonable way to facilitate the defense or settlement of the claim.

B.	If any product or service becomes, or in the contractor's opinion is likely to become the subject of a claim of infringement, the contractor shall at its option and expense:  

i. 	provide a procuring agency of the County the right to continue using the product or service;

ii.	replace or modify the product or service so that it becomes non-infringing; or 

iii. 	accept the return of the product or service and refund an amount equal to the depreciated value of the returned product or service, less the unpaid portion of the purchase price and any other amounts which are due to the contractor.  The contractor's obligation will be void as to any product or service modified by the procuring agency of the County to the extent such modification is the cause of the claim.

36.	Professional Liability Insurance.
	Contractor agrees to maintain in full force throughout the duration of the Agreement a liability insurance policy with a minimum coverage of [insert appropriate coverage amounts depending on assignment].
















SCOPE OF WORK
The Contractor Shall:
· Meet NFPA 1917 Standards for Automotive Ambulances 2016 Editions
· Meet KKK Federal Standards for the life of the Ambulance
· Insure EMS Vehicle must be fully equipped to meet these needs
· Provide milestones of unit prior to delivery to insure construction is meeting the  specifications and requirements
· Provide 360 Photos of the unit- interior, exterior, under carriage, front, rear, roof, engine, excreta. 
· Provide an expected delivery date in bid documents 


BOARD OF COUNTY COMMISSIONERS OF THE COUNTY OF SIERRA
37. Notices: 
Any notice required to be given to either party by this Agreement shall be in writing and shall be delivered in person, by courier service or by U.S. mail, either first class or certified, return receipt requested, postage prepaid, as follows:

To:  County of Sierra
Jocelyn Holguin, Chief Procurement Officer 
855 Van Patten
Truth or Consequences, NM 87901

To the Contractor: 
                               
Printed Name: 
Address:  


IN WITNESS WHEREOF, the parties have executed this Agreement as of the date of signature by the County Chief Procurement Officer below:

Contractor Signature: __________________________ Date: ________________


By: ____________________________ Date: ____________________________
Bruce Swingle, County Manager 


BOARD OF COUNTY COMMISSIONERS

APPROVED, ADOPTED AND PASSED on this _20th_ day of _December_, 2016.
_______________________________________________________________

______________________________________
 Ken Lyon, Chair

______________________________________
Frances Luna, Vice- Chair

______________________________________
Sherry Fletcher, Commissioner

Attest:
_________________________________
Connie Greer
Sierra County Clerk


Sierra County Chief Procurement Officer:

By: ______________________________ Date: ___________________________
Jocelyn Holguin, CPO
Sierra County
Address: 855 Van Patten, Truth or Consequences, NM 87901
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