{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Itemized Bid Schedule"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Itemized Bid Schedule","index":0,"n_rows":316,"n_cols":7,"rows_kept":316,"merged":[[0,1,0,6],[2,1,2,6],[3,1,3,6],[4,3,4,6],[7,1,7,5],[79,2,79,5],[80,1,80,5],[98,2,98,5],[99,1,99,5],[130,2,130,5],[131,1,131,5],[140,2,140,5],[141,1,141,5],[156,2,156,5],[158,1,158,5],[159,1,159,5],[161,1,161,5],[172,1,172,5],[184,2,184,5],[186,2,186,5],[187,1,187,5],[302,2,302,5],[304,1,304,5],[305,1,305,5],[307,1,307,5],[309,1,309,6],[310,1,310,6],[311,1,311,6],[312,1,312,6],[313,1,313,6],[314,1,314,6],[315,1,315,6]],"flags":["formulas_cached_only"]}
[null,"                                                                                                                        ITEMIZED BID SCHEDULE                                                                                *  ADDENDUM #3"]
[]
[null,"PROJECT NAME: SR 60 AND 43RD AVENUE INTERSECTION IMPROVEMENTS"]
[null,"IRC PROJECT NO: IRC-0853, FM NO. 431759-2-54-01, BID NO. 2019073"]
[null,null,"                                                                                                          BIDDER'S NAME:","________________________________________________________________"]
[]
[null,"Item No.","Description","Unit","Unit Price","Quantity","Total"]
[null,"ROADWAY CONSTRUCTION"]
[null,"0101 1","MOBILIZATION","LS",null,1,0]
[null,"0102 1","MAINTENANCE OF TRAFFIC (INCLUDES PEDESTRIAN MOT)","LS",null,1,0]
[null,"0102 14","TRAFFIC CONTROL OFFICER (OFF DUTY LAW ENFORCEMENT) ","MH",null,300,0]
[null,"0102 99","PORTABLE CHANGEABLE MESSAGE SIGN, TEMPORARY (18)","ED",null,{"v":7520,"d":"7,520"},0]
[null,"0104","N.P.D.E.S. COMPLIANCE","LS",null,1,0]
[null,"0104 10 3","SEDIMENT BARRIER","LF",null,{"v":16456,"d":"16,456"},0]
[null,"0104 11","FLOATING TURBIDITY BARRIER","LF",null,560,0]
[null,"0104 18","INLET PROTECTION SYSTEM","EA",null,69,0]
[null,"0110 1 1","CLEARING & GRUBBING","LS",null,1,0]
[null,"0120 1","REGULAR EXCAVATION","CY",null,{"v":12656,"d":"12,656"},0]
[null,"0120 6","EMBANKMENT (COMPACTED IN PLACE)","CY",null,{"v":5781,"d":"5,781"},0]
[null,"0160 4","TYPE B  STABILIZATION (12\" SUBGRADE, LBR 40)","SY",null,{"v":44072,"d":"44,072"},0]
[null,"0285 707","OPTIONAL BASE, BASE GROUP 07 (9\" CEMENTED COQUINA)","SY",null,{"v":40580,"d":"40,580"},0]
[null,"0286 1","TURNOUT CONSTRUCTION/DRIVEWAY BASE (CONCRETE)","SY",null,{"v":1526,"d":"1,526"},0]
[null,"0286 2","TURNOUT CONSTRUCTION-ASPHALT/DRIVEWAY BASE-ASPHALT MATERIAL","TN",null,98,0]
["*","0327 70 1","MILL EXIST ASPH PAVT, 1\" AVG DEPTH","SY",null,{"v":17144,"d":"17,144"},0]
["*","0327 70 8","MILL EXIST ASPH PAVT, 2.5\" AVG DEPTH","SY",null,{"v":2944,"d":"2,944"},0]
["*","0334 1 13","SUPERPAVE ASPHALTIC CONC, TRAFFIC C (SP-12.5 OVERBUILD)","TN",null,{"v":7200,"d":"7,200"},0]
["*","0334 1 13A","SUPERPAVE ASPHALTIC CONC, TRAFFIC C, PG 76-22, (SP-12.5,               1-1/2\" THICK) (WITH POLYMER)","TN",null,{"v":4760,"d":"4,760"},0]
["*","0337 7 82","ASPHALT CONCRETE FRICTION COURSE, FC-9.5, TRAFFIC C, PG 76-22, (WITH POLYMER) 1\" THICK","TN",null,{"v":3173,"d":"3,173"},0]
[null,"0400 0 11","CONCRETE, CLASS NS, GRAVITY WALL","CY",null,81.9,0]
[null,"0400 1 2","CONCRETE CLASS I, ENDWALLS","CY",null,6.33,0]
[null,"0425 1311 ","INLETS, CURB, TYPE P-1, <10'","EA",null,5,0]
[null,"0425 1321","INLETS, CURB, TYPE P-2, <10'","EA",null,4,0]
[null,"0425 1341","INLETS, CURB, TYPE P-4, <10'","EA",null,1,0]
[null,"0425 1351","INLETS, CURB, TYPE P-5, <10'","EA",null,16,0]
[null,"0425 1352","INLETS, CURB, TYPE P-5, >10'","EA",null,2,0]
[null,"0425 1361","INLETS, CURB, TYPE P-6, <10'","EA",null,12,0]
[null,"0425 1421","INLETS, CURB, TYPE J-2, <10'","EA",null,2,0]
[null,"0425 1451","INLETS, CURB, TYPE J-5, <10'","EA",null,1,0]
[null,"0425 1452","INLETS, CURB, TYPE J-5, >10'","EA",null,1,0]
[null,"0425 1461","INLETS, CURB, TYPE J-6, <10'","EA",null,2,0]
[null,"0425 1521","INLETS, DT BOT, TYPE C, <10'","EA",null,27,0]
[null,"0425 1521A","INLETS, DT BOT, TYPE C, <10' (MODIFIED)","EA",null,2,0]
[null,"0425 1559","INLETS, DT BOT, TYPE E, <10'","EA",null,2,0]
[null,"0425 1715","INLETS, GUTTER, TYPE V, <10'","EA",null,2,0]
[null,"0425 2 41","MANHOLES, P-7, <10'","EA",null,4,0]
[null,"0425 2 43","MANHOLES, P-7, PARTIAL","EA",null,1,0]
[null,"0425 2 61","MANHOLES, P-8, <10'","EA",null,3,0]
[null,"0425 2 71","MANHOLES, J-7, <10'","EA",null,3,0]
[null,"0425 2 91","MANHOLES, J-8, >10'","EA",null,11,0]
[null,"0425 4","INLETS, ADJUST","EA",null,7,0]
[null,"0425 5","MANHOLE, ADJUST","EA",null,7,0]
[null,"0425 6","VALVE BOXES, ADJUST","EA",null,38,0]
[null,"0430 174 115","PIPE CULVERT, ROUND, 15\" SD (RCP)","LF",null,30,0]
[null,"0430 174 118","PIPE CULVERT, ROUND, 18\" SD (RCP)","LF",null,{"v":4054,"d":"4,054"},0]
[null,"0430 174 124","PIPE CULVERT, ROUND, 24\" SD (RCP)","LF",null,{"v":1143,"d":"1,143"},0]
[null,"0430 174 130","PIPE CULVERT, ROUND, 30\" SD (RCP)","LF",null,198,0]
[null,"0430 174 136","PIPE CULVERT, ROUND, 36\" SD (RCP)","LF",null,{"v":2231,"d":"2,231"},0]
[null,"0430 174 142","PIPE CULVERT, ROUND, 42\" SD (RCP)","LF",null,853,0]
[null,"0430 175 148","PIPE CULVERT, ROUND, 48\" SD (RCP)","LF",null,85,0]
[null,"0430 982 140","MITERED END SECTION, 42\" SD","EA",null,1,0]
[null,"0430 984 125","MITERED END SECTION, 18\" SD","EA",null,1,0]
[null,"0430 984 138","MITERED END SECTION, 36\" SIDE DRAIN","EA",null,1,0]
[null,"0430 984 141","MITERED END SECTION, 48\" SD","EA",null,1,0]
[null,"0443 70 3","FRENCH DRAIN, 18\"","LF",null,{"v":1616,"d":"1,616"},0]
[null,"0515 1 2","PIPE HANDRAIL - GUIDERAIL, ALUMINUM","LF",null,{"v":1187,"d":"1,187"},0]
[null,"0520 1 10","CONCRETE CURB & GUTTER, TYPE F","LF",null,{"v":21539,"d":"21,539"},0]
[null,"0520 5 41","TRAFFIC SEPARATOR CONCRETE - TYPE IV, 4' WIDE","LF",null,457,0]
["*","0520 70","CONCRETE TRAFFIC SEPARATOR, SPECIAL-VARIABLE WIDTH (COLOR TREATED AND STAMPED CONCRETE)","SY",null,832,0]
["*","0522 2","CONCRETE SIDEWALK AND DRIVEWAYS, 6\" THICK","SY",null,{"v":8612,"d":"8,612"},0]
[null,"0524 1 2","CONCRETE DITCH PAVEMENT, NON REINFORCED, 4\"","SY",null,49,0]
[null,"0527 2","DETECTABLE WARNINGS","SF",null,480,0]
[null,"0530 3 4","RIPRAP, RUBBLE, F&I, DITCH LINING","TN",null,146,0]
[null,"0550 10 222","FENCING, TYPE B, 5.1-6.0, W/ VINYL COATING","LF",null,{"v":1040,"d":"1,040"},0]
[null,"0570 1 2","PERFORMANCE TURF, SOD","SY",null,{"v":16393,"d":"16,393"},0]
[null,"0630 2 11A","CONDUIT, (F&I), (2-2\" PVC) ","LF",null,20,0]
[null,"0635 2 12","PULL & SPLICE BOX, F & I (30\"x48\"x24\")","EA",null,2,0]
[null,"0999-1","RECORD DRAWINGS/AS-BUILTS","LS",null,1,0]
[null,"1050 31206","UTILITY PIPE - POLYVINYLCHLORIDE, F&I, 6\"","LF",null,845,0]
[null,"1050 4126","6\" HDPE FORCE MAIN CASING","LF",null,85,0]
[null,null,"SUB-TOTAL OF ROADWAY CONSTRUCTION",{"$nulls":3},0]
[null,"SIGNING & PAVEMENT MARKINGS"]
[null,"0700 1 11","SINGLE POST SIGN, F&I GROUND MOUNT, UP TO 12 SF","AS",null,73,0]
[null,"0700 1 13","SINGLE POST SIGN, F&I GROUND MOUNT, 21-30 SF","AS",null,1,0]
[null,"0700 1 50","SINGLE POST SIGN, RELOCATE","AS",null,15,0]
[null,"0705 11 1","DELINEATOR, FLEXIBLE TUBULAR","EA",null,18,0]
[null,"0706 3 ","RETRO-REFLECTIVE RAISED PAVEMENT MARKER","EA",null,796,0]
[null,"0710 11 290","PAINTED PAVEMENT MARKINGS, STANDARD, YELLOW, ISLAND NOSE","SF",null,67,0]
[null,"0711 11 122","THERMOPLASTIC, STANDARD, WHITE, SOLID, 8\" ","GM",null,{"v":0.4,"d":"0.40"},0]
[null,"0711 11 123","THERMOPLASTIC, STANDARD, WHITE, SOLID, 12\" FOR CROSSWALK AND ROUNDABOUT","LF",null,{"v":2611,"d":"2,611"},0]
[null,"0711 11 124","THERMOPLASTIC, STANDARD, WHITE, SOLID, 18\" FOR DIAGONALS AND CHEVRONS","LF",null,455,0]
[null,"0711 11 125","THERMOPLASTIC, STANDARD, WHITE, SOLID, 24\" FOR STOP LINE AND CROSSWALK","LF",null,585,0]
[null,"0711 11 160","THERMOPLASTIC, STANDARD, WHITE, MESSAGE OR SYMBOL","EA",null,20,0]
[null,"0711 11 170","THERMOPLASTIC, STANDARD, WHITE, ARROW","EA",null,86,0]
[null,"0711 11 222","THERMOPLASTIC, STANDARD, YELLOW, SOLID, 18\" FOR DIAGONAL OR CHEVRON","LF",null,77,0]
[null,"0711 16 101","THERMOPLASTIC, STANDARD - OTHER SURFACES, WHITE, SOLID, 6\"","GM",null,{"v":3.1,"d":"3.10"},0]
[null,"0711 16 131","THERMOPLASTIC, STANDARD - OTHER SURFACES, WHITE, 6\", 10-30 SKIP OR 3-9 LANE DROP","GM",null,3.59,0]
[null,"0711 16 201","THERMOPLASTIC, STANDARD-OTHER SURFACES, YELLOW, SOLID, 6\"","GM",null,2.37,0]
[null,"0711 16 231","THERMOPLASTIC, STANDARD - OTHER SURFACES, YELLOW, SKIP, 6\"","GM",null,0.44,0]
[null,null,"SUB-TOTAL OF SIGNING & PAVEMENT MARKING IMPROVEMENTS",{"$nulls":3},0]
[null,"SIGNALIZATION"]
[null,"0630 2 11B","CONDUIT (F&I) (UNDERGROUND)","LF",null,{"v":12072,"d":"12,072"},0]
[null,"0630 2 12","CONDUIT (F&I) (UNDER PAVEMENT) (DIRECTIONAL BORE)","LF",null,{"v":1083,"d":"1,083"},0]
[null,"0630 2 15","CONDUITS (F&I) (BRIDGE MOUNTED)","LF",null,{"v":1620,"d":"1,620"},0]
[null,"0632 7 1","CABLE (SIGNAL) (F&I)","PI",null,1,0]
[null,"0633 1 123","FIBER OPTIC CABLE (F&I) (UNDERGROUND) (96 SINGLE MODE)","LF",null,{"v":7296,"d":"7,296"},0]
[null,"0633 3 15","FIBER OPTIC CONNECTION HARDWARE (F&I) (PRETERMINATED PATCH PANEL)","EA",null,1,0]
[null,"0635 2 11A","PULL & SPLICE BOXES (F&I)","EA",null,23,0]
[null,"0635 2 13","PULL & SPLICE BOXES (F&I) (FIBER OPTICS)","EA",null,26,0]
[null,"0639 1 123","ELECTRICAL POWER SERVICE (F&I) (UNDERGROUND)","AS",null,1,0]
[null,"0639 2 1","ELECTRICAL SERVICE WIRE (F&I) (POLE)","LF",null,200,0]
[null,"0639 3 11","ELECTRICAL SERVICE DISCONNECT (F&I) (POLE)","EA",null,1,0]
[null,"0641 2 12","PRE-STRESSED CONCRETE POLE (F&I) (p-11)","EA",null,1,0]
[null,"0641 2 80","CONCRETE POLE REMOVAL (COMPLETE/DEEP)","EA",null,4,0]
[null,"0646 1 11","ALUMINUM SIGNAL POLES (F&I) (PEDESTAL)","EA",null,8,0]
[null,"0649 31 105","MAST ARM (F&I) (SINGLE ARM W/O LUM) (78')","EA",null,1,0]
[null,"0649 31 109","MAST ARM (F&I) (SINGLE ARM W/ LUM) (70.5')","EA",null,2,0]
[null,"0649 31 118","MAST ARM (F&I) (DOUBLE ARM W/O LUM) (70.5'-60')","EA",null,1,0]
[null,"0650 1 24","TRAFFIC SIGNAL (F&I) (3-SECT) (1 WAY) (ALUM)","AS",null,16,0]
[null,"0650 1 29","TRAFFIC SIGNAL (F&I) (5-SECT) (1 WAY) (ALUM)","AS",null,4,0]
[null,"0653 1 11","PEDESTRIAN SIGNAL (F&I) (LED, 1 WAY)","AS",null,8,0]
[null,"0660 4 11","VEHICLE DETECTION (F&I) (VIDEO) (CABINET EQUIPMENT)","EA",null,4,0]
[null,"0660 4 12","VEHICLE DETECTION (F&I) (VIDEO) (ABOVE GROUND)","EA",null,4,0]
[null,"0665 1 11","PEDESTRIAN DETECTOR (F&I) (STD)","EA",null,8,0]
[null,"0670 5 110","TRAFFIC CONTROLLER ASSEMBLY (F&I) (NEMA)","AS",null,1,0]
[null,"0670 5 600","CONTROLLER ASSEMBLY (REMOVE)","AS",null,1,0]
[null,"0682 1 133","CCTV CAMERA (F&I) (NON-PRESSURIZED) (IP, HIGH DEF)","EA",null,1,0]
[null,"0684 1 1","MANAGED FIELD ETHERNET SWITCH (F&I)","EA",null,1,0]
[null,"0685 106","SYSTEMS AUXILIARIES (UNINTERRUPTABLE POWER SOURCE) (F&I)","EA",null,1,0]
[null,"0700 3 201","SIGN PANEL (F&I) (OVERHEAD) (12 SF)","EA",null,4,0]
[null,"0700 5 21","INTERNALLY ILLUMINATED SIGN (F&I) (NAME) (OVERHEAD) (12 SF)","EA",null,4,0]
[null,null,"SUB-TOTAL OF SIGNALIZATION IMPROVEMENTS",{"$nulls":3},0]
[null,"HIGHWAY LIGHTING SYSTEM"]
[null,"0635 2 11","PULL BOX (F&I) (ROADSIDE), MOULDED","EA",null,71,0]
[null,"0715 1 13","LIGHTING CONDUCTOR, F & I, INSULATED, NO. 4","LF",null,{"v":36765,"d":"36,765"},0]
[null,"0715 4 13","STANDARD LIGHT POLE COMPLETE W/ CONCRETE BASE, F&I, WIND SPEED 160","EA",null,30,0]
[null,"0715 4 33","CONFLICT LIGHT POLE COMPLETE W/ CONCRETE BASE, F&I, WIND SPEED 160","EA",null,36,0]
[null,"0715 5 30","LUMINAIRE AND BRACKET ARM MOUNTED ON SIGNAL POLE, F&I","EA",null,4,0]
[null,"0715 7 11","LOAD CENTER (INCLUDES ALL COMPONENTS LISTED ON SERVICE POINT DETAILS DRAWING)","EA",null,3,0]
[null,"0715 500 1","POLE CABLE DISTRIBUTION SYSTEM, IP-68","EA",null,70,0]
[null,"1050 31102","LIGHTING CONDUCTOR, F & I, UNDERGROUND, 2\" PVC SCH. 40","LF",null,{"v":11094,"d":"11,094"},0]
[null,null,"SUB-TOTAL OF LIGHTING IMPROVEMENTS",{"$nulls":3},0]
[null,"LANDSCAPE, HARDSCAPE AND IRRIGATION"]
[null,"0520 2 13","HEADER CURB","LF",null,632,0]
[null,"0523 1","PATTERNED PAVEMENT, VEHICULAR AREAS (DURATHERM, INTEGRATED PAVING CONCEPTS, CINNAMON, WAGON WHEEL)","SY",null,800,0]
[null,"0526 1 2","PAVERS, ARCHITECTURAL, SIDEWALK (BELGARD, HOLLAND 4\"x8\" 80mm, RED/CHESTNUT/CHARCOAL, 45˚ HERRINGBONE)","SY",null,290,0]
[null,"0580 4 235","PHOENIX SYLVESTRIS (SYLVESTER DATE PALM) (16' CT)","EA",null,3,0]
[null,"0580 4 345","SABAL PALMETTO (SABAL PALM) (16-20' CT)","EA",null,5,0]
[null,"0580 5 5532","GORDONIA IASIANTHUS (LOBLOLLY BAY) (8-10'x4-5' 2.75 CAL.)","EA",null,9,0]
[null,"0580 5 572","LIGUSTRUM JAPONICUM (JAPANESE PRIVET) (8-10' OA MULTISTEM)","EA",null,14,0]
[null,"0580 7 177","ILEX BOMITORIA \"SHILLINGS\" (DWARF YAUPON HOLLY) (#7 FULL) (24\" OC)","EA",null,48,0]
[null,"0580 7 337","MYRCIANTHES FRAGRANS (SIMPSON'S STOPPER) (#7) (24\" O.C.)","EA",null,59,0]
[null,"E575 1","BAHIA SOD (PASPALUM NOTATUM)","SY",null,{"v":5450,"d":"5,450"},0]
[null,"E575 1 4","ST. AUGUSTINE SOD","SY",null,{"v":3400,"d":"3,400"},0]
[null,"E580326 4","MULCH WOOD CHIPS ","SY",null,16,0]
[null,"E580337 5","HERBICIDE, ROOT CONTROL FABRIC- 20\" WIDE","LF",null,145,0]
[null,"0590 1","IRRIGATION SYSTEM ","LS",null,1,0]
[null,null,"SUB-TOTAL OF LANDSCAPE, HARDSCAPE AND IRRIGATION IMPROVEMENTS",{"$nulls":3},0]
[]
[null,"STRUCTURAL"]
[null,"BRIDGE"]
[null,"0110 3","REMOVAL OF EXISTING STRUCTURE/BRIDGES","LS",null,1,0]
[null,"SUPERSTRUCTURE"]
[null,"0400 2 4A","CONC CLASS II, BRIDGE SUPERSTRUCTURE","CY",null,138,0]
[null,"0400 2 4B","CONC CLASS II, BRIDGE SUPERSTRUCTURE (LIGHTWEIGHT)","CY",null,153.7,0]
[null,"0400 7","BRIDGE DECK GROOVING, LESS THAN 8.5\"","SY",null,523,0]
[null,"0400 147","COMPOSITE NEOPRENE PADS","CF",null,1.64,0]
[null,"0415 1 4","REINFORCING STEEL-BRIDGE SUPERSTRUCTURE","LB",null,{"v":63459.3,"d":"63,459.30"},0]
[null,"0450 1 2","PRESTRESSED BEAMS TYPE III","LF",null,778.13,0]
[null,"0458 1 11","CONSTRUCTION, F&I POURED JOINT WITH BACKER ROD","LF",null,{"v":80,"d":"80.00"},0]
[null,"0458 1 21","BRIDGE DECK EXPANSION JOINT, REHABILITATION, POURED JOINT WITH BACKER ROD","LF",null,{"v":180,"d":"180.00"},0]
[null,"0515 4 2","BULLET ALUMINUM RAIL, DOUBLE RAIL","LF",null,348.67,0]
[null,"0521 5 4","CONCRETE TRAFFIC RAILING- BRIDGE, 32\" VERTICAL FACE","LF",null,348.67,0]
[null,"SUBSTRUCTURE"]
[null,"0400 2 5","CONCRETE CLASS II, BRIDGE SUBSTRUCTURE","CY",null,60,0]
[null,"0400 2 10","CONCRETE CLASS II, APPROACH SLABS","CY",null,62,0]
[null,"0415 1 5","REINFORCING STEEL- BRIDGE SUBSTRUCTURE","LB",null,{"v":16156,"d":"16,156"},0]
[null,"0415 1 9","REINFORCING STEEL-APPROACH SLABS","LB",null,{"v":12170,"d":"12,170"},0]
[null,"0455 34 3A","PRESTRESSED CONCRETE PILING, 18\" SQ (END BENTS)","LF",null,550,0]
[null,"0455 34 3B","PRESTRESSED CONCRETE PILING, 18\" SQ (WING BENTS)","LF",null,100,0]
[null,"0455 34 3C","PRESTRESSED CONCRETE PILING, 18\" SQ (INTERMEDIATE BENTS, DEBRIS PILES)","LF",null,650,0]
[null,"0455 137 1","LOAD TEST (DYNAMIC), INTERNAL GAUGES","EA",null,2,0]
[null,"0455 143 3A","TEST PILES-PRESTRESSED CONCRETE,18\" SQ","LF",null,130,0]
[null,"0530 4 9","ARTICULATING CONCRETE BLOCK REVETMENT SYSTEM, THICKNESS 6\"","SF",null,{"v":2934,"d":"2,934"},0]
[null,"1050 31204D","UTILITY PIPE- POLY VINYL CHLORIDE, FURNISH & INSTALL, WATER/SEWER, 4\"","LF",null,{"v":1400,"d":"1,400"},0]
[null,null,"SUB-TOTAL OF STRUCTURAL IMPROVEMENTS",{"$nulls":3},0]
[null,"0999-25","FORCE ACCOUNT",{"$nulls":3},{"v":1300000,"d":"$1,300,000.00"}]
[null,null,"TOTAL ROADWAY IMPROVEMENTS (INCLUDING FORCE ACCOUNT)",{"$nulls":3},{"v":1300000,"d":"1,300,000.00"}]
[null,"UTILITY WORK BY HIGHWAY CONTRACTOR (UWHC)"]
[null,"0104 10 3A","EROSION CONTROL - SEDIMENT BARRIER","LS",null,1,0]
[null,"0110 1 1A","CLEARING AND GRUBBING","LS",null,1,0]
[null,"0160 4A","TYPE B STABILIZATION (DRIVEWAYS)","SY",null,{"v":1085.3333333333333,"d":"1,085"},0]
[null,"0334 1 13A","SUPERPAVE ASPHALTIC CONCRETE (SP-12.5) TRAFFIC \"C\" (1-1/2\")","SY",null,{"v":1085.3333333333333,"d":"1,085"},0]
[null,"0425 2 71A","MANHOLE, J-7, LESS THAN 10'","EA",null,1,0]
[null,"0522 2A","R & R, 6\" CONCRETE SIDEWALK","SY",null,{"v":1255,"d":"1,255"},0]
[null,"0570 1 1","INSTALL SEED & MULCH","SY",null,{"v":9320,"d":"9,320"},0]
[null,"0570 1 2A","INSTALL SOD - BAHIA","SY",null,{"v":1860,"d":"1,860"},0]
[null,"0570 1 2B","INSTALL SOD - FLORATAM","SY",null,200,0]
[null,"0999 2","AS-BUILT SURVEYING ","LS",null,1,0]
[null,"1050 16001","REMOVE & DISPOSE EXISTING 1\" WATER MAIN AND APPURTENANCES (0-1.9\")","LF",null,265,0]
[null,"1050 16002","REMOVE & DISPOSE EXISTING 2\"-3\" WATER MAIN AND APPURTENANCES (2-4.9\")","LF",null,305,0]
[null,"1050 16002A","REMOVE & DISPOSE EXISTING 3\" FORCE MAIN AND APPURTENANCES (2-4.9\")","LF",null,560,0]
[null,"1050 16003","REMOVE & DISPOSE EXISTING 6\" FORCE MAIN AND APPURTENANCES (5-7.9\")","LF",null,{"v":2120,"d":"2,120"},0]
[null,"1050 16003A","REMOVE & DISPOSE EXISTING 6\" WATER MAIN AND APPURTENANCES (5-7.9\")","LF",null,790,0]
[null,"1050 16004","REMOVE & DISPOSE EXISTING 8\" WATER MAIN AND APPURTENANCES (8-19.9\")","LF",null,{"v":5560,"d":"5,560"},0]
[null,"1050 16004A","REMOVE & DISPOSE EXISTING 8\" FORCE MAIN AND APPURTENANCES (8-19.9\")","LF",null,{"v":2330,"d":"2,330"},0]
[null,"1050 16004B","REMOVE & DISPOSE EXISTING 6\" SANITARY SEWER SERVICE PIPE","LF",null,100,0]
[null,"1050 18002","GROUT FILL AND ABANDON EXISTING 2\" WATER MAIN (2-4.9\")","LF",null,190,0]
[null,"1050 18002A","GROUT FILL AND ABANDON EXISTING 3\" FORCE MAIN (2-4.9\")","LF",null,795,0]
[null,"1050 18003","GROUT FILL AND ABANDON EXISTING 6\" WATER MAIN (5-7.9\")","LF",null,400,0]
[null,"1050 18003A","GROUT FILL AND ABANDON EXISTING 6\" SANITARY MAIN (5-7.9\")","LF",null,170,0]
[null,"1050 18004","GROUT FILL AND ABANDON EXISTING 8\" WATER MAIN (8-19.9\")","LF",null,990,0]
[null,"1050 18004A","GROUT FILL AND ABANDON EXISTING 8\" SANITARY MAIN (8-19.9\")","LF",null,55,0]
[null,"1050 31202","F & I, 2” PVC SDR21 (BLUE) WATER MAIN PRESSURE PIPE (ITEM TO INCLUDE ALL NECESSARY PVC OR BRASS FITTINGS PER PLANS AND SPECIFICATIONS) (SEE APPENDIX E)","LF",null,20,0]
[null,"1050 31202A","F & I, 2” PVC SDR21 (GREEN) FORCE MAIN  PRESSURE PIPE (ITEM TO INCLUDE ALL NECESSARY PVC OR BRASS FITTINGS PER PLANS AND SPECIFICATIONS) (SEE APPENDIX E)","LF",null,20,0]
[null,"1050 31202B","F & I, 2 1/2” PVC SDR21 (BLUE) WATER MAIN PRESSURE PIPE (ITEM TO INCLUDE ALL NECESSARY PVC OR BRASS FITTINGS PER PLANS AND SPECIFICATIONS) (SEE APPENDIX E)","LF",null,40,0]
[null,"1050 31203","F & I, 3” PVC C-900 DR-18 (GREEN) FORCE MAIN PRESSURE PIPE. (ITEM TO INCLUDE ALL NECESSARY M.J. D.I. FITTINGS AND PIPE RESTRAINTS PER PLANS AND SPECIFICATIONS)   (SEE APPENDIX E)","LF",null,20,0]
[null,"1050 31204","F & I, 4” PVC C-900  DR-18 (GREEN) FORCE MAIN PRESSURE PIPE (ITEM TO INCLUDE ALL NECESSARY M.J. D.I. FITTINGS AND PIPE RESTRAINTS PER PLANS AND SPECIFICATIONS)  (SEE APPENDIX E)","LF",null,200,0]
[null,"1050 31206","F & I, 6” PVC C-900 DR-18 (BLUE) WATER MAIN PRESSURE PIPE (ITEM TO INCLUDE ALL NECESSARY M.J. D.I. FITTINGS AND PIPE RESTRAINTS PER PLANS AND SPECIFICATIONS)   (SEE APPENDIX E)","LF",null,180,0]
[null,"1050 31206A","F & I, 6” PVC C-900 DR-18 (GREEN) FORCE MAIN PRESSURE PIPE (ITEM TO INCLUDE ALL NECESSARY M.J. D.I. FITTINGS AND PIPE RESTRAINTS PER PLANS AND SPECIFICATIONS)   (SEE APPENDIX E)","LF",null,140,0]
[null,"1050 31206B","F & I, 6” PVC C-900 DR-18 (GREEN) PRESSURE PIPE WITH SEWER FITTINGS (SEWER SERVICES)","LF",null,100,0]
[null,"1050 31208","F & I, 8\" PVC C-900 DR-18 (BLUE) WATER MAIN PRESSURE PIPE","LF",null,{"v":3380,"d":"3,380"},0]
[null,"1050 31208A","F & I, 8” PVC SDR-35 (GREEN) SANITARY SEWER PIPE","LF",null,40,0]
[null,"1050 31208B","F & I, 8\" PVC C-900 DR 18 CL150 (GREEN) FORCE MAIN PRESSURE PIPE","LF",null,{"v":2480,"d":"2,480"},0]
[null,"1050 31210","F & I, 10\" PVC C-900 DR 18 CL150 (GREEN) FORCE MAIN PRESSURE PIPE","LF",null,20,0]
[null,"1050 31212","F & I, 12” PVC C-900 DR-18 (BLUE) WATER MAIN PRESSURE PIPE","LF",null,{"v":2340,"d":"2,340"},0]
[null,"1050 41201","F & I, 1” PE3408 SDR-9 PE (BLUE) WATER MAIN PRESSURE PIPE ","LF",null,400,0]
[null,"1050 41202","F, I, & R 2” PE3408 SDR-9 PE (BLUE) WATER MAIN PRESSURE PIPE (REMOVE AFTER NEW W.M. IS IN SERVICE)","LF",null,{"v":1040,"d":"1,040"},0]
[null,"1050 42202A","F & I, 2” PE3408 SDR-9 PE (BLUE) WATER MAIN  PRESSURE PIPE ","LF",null,530,0]
[null,"1050 42202B","F & I, 2” PE3408 SDR-9 PE (GREEN) FORCE MAIN PRESSURE PIPE ","LF",null,400,0]
[null,"1050 42208","F & I, 8” PE3408 SDR-11 PE (BLUE) WATER MAIN PRESSURE PIPE ","LF",null,160,0]
[null,"1050 42208A","F & I, 8” PE3408 SDR-11 PE (GREEN) FORCE MAIN PRESSURE PIPE ","LF",null,120,0]
[null,"1050 42212","F & I, 12” PE3408 SDR-11 PE (BLUE) WATER MAIN PRESSURE PIPE ","LF",null,760,0]
[null,"1055 51108","F & I, 8” MJ C-153 11.25° BEND (WATER) WITH MEGA-LUG RESTRAINTS","EA",null,4,0]
[null,"1055 51108A","F & I, 8” MJ C-153 11.25° BEND (SEWER-LINED) WITH MEGA-LUG RESTRAINTS","EA",null,4,0]
[null,"1055 51108B","F & I, 8” MJ C-153 22.5° BEND (SEWER-LINED)  WITH MEGA-LUG RESTRAINTS","EA",null,7,0]
[null,"1055 51108C","F & I, 8” MJ C-153 45° BEND (WATER) WITH MEGA-LUG RESTRAINTS","EA",null,34,0]
[null,"1055 51108D","F & I, 8” MJ C-153 45° BEND (SEWER-LINED) WITH MEGA-LUG RESTRAINTS","EA",null,36,0]
[null,"1055 51108E","F & I, 8” MJ C-153 90° BEND (WATER) WITH MEGA-LUG RESTRAINTS","EA",null,3,0]
[null,"1055 51108F","F & I, 8” MJ C-153 90° BEND (SEWER-LINED) WITH MEGA-LUG RESTRAINTS","EA",null,1,0]
[null,"1055 51112","F & I, 12” MJ C-153 11.25° BEND (WATER) WITH MEGA-LUG RESTRAINTS","EA",null,4,0]
[null,"1055 51112A","F & I, 12” MJ C-153 22.5° BEND (WATER) WITH MEGA-LUG RESTRAINTS","EA",null,1,0]
[null,"1055 51112B","F & I, 12” MJ C-153 45° BEND (WATER) WITH MEGA-LUG RESTRAINTS","EA",null,10,0]
[null,"1055 51112C","F & I, 12” MJ C-153 90° BEND (WATER) WITH MEGA-LUG RESTRAINTS","EA",null,4,0]
[null,"1055 51208","F & I, 8X8X6 MJ C-153 TEE (WATER) WITH MEGA-LUG RESTRAINTS","EA",null,7,0]
[null,"1055 51208A","F & I, 8X8X4 MJ C-153 TEE (SEWER-LINED) WITH MEGA-LUG RESTRAINTS","EA",null,2,0]
[null,"1055 51208B","F & I, 8X8X6 MJ C-153 TEE (SEWER-LINED) WITH MEGA-LUG RESTRAINTS","EA",null,1,0]
[null,"1055 51208C","F & I, 8X8X8 MJ C-153 TEE (SEWER-LINED) WITH MEGA-LUG RESTRAINTS","EA",null,2,0]
[null,"1055 51212","F & I, 12X12X6 MJ C-153 TEE (WATER) WITH MEGA-LUG RESTRAINTS","EA",null,5,0]
[null,"1055 51212A","F & I, 12X12X12 MJ C-153 TEE (WATER) WITH MEGA-LUG RESTRAINTS","EA",null,1,0]
[null,"1055 51310","F & I, 10X8 MJ C-153 REDUCER (SEWER-LINED) WITH MEGA-LUG RESTRAINTS","EA",null,1,0]
[null,"1055 51312","F & I, 12X8 MJ C-153 REDUCER (WATER) WITH MEGA-LUG RESTRAINTS","EA",null,2,0]
[null,"1055 51408","F & I, 8” MJ C-153 L.B. SLEEVE (WATER) WITH MEGA-LUG RESTRAINTS","EA",null,3,0]
[null,"1055 51408A","F & I, 8” MJ C-153 L.B. SLEEVE (SEWER-LINED) WITH MEGA-LUG RESTRAINTS","EA",null,6,0]
[null,"1055 51410","F & I, 10” MJ C-153 L.B. SLEEVE (SEWER-LINED) WITH MEGA-LUG RESTRAINTS","EA",null,1,0]
[null,"1055 51412","F & I, 12” MJ C-153 L.B. SLEEVE (WATER) WITH MEGA-LUG RESTRAINTS","EA",null,1,0]
[null,"1055 51506","F & I, 6\" MJ C-153 PLUG TAPPED 2\" (WATER) WITH MEGA-LUG RESTRAINTS","EA",null,2,0]
[null,"1055 51508","F & I, 8\" MJ C-153 PLUG TAPPED 2\" (WATER) WITH MEGA-LUG RESTRAINTS","EA",null,2,0]
[null,"1055 51508A","F & I, 8\" MJ C-153 PLUG TAPPED 2\" (SEWER-LINED) WITH MEGA-LUG RESTRAINTS","EA",null,1,0]
[null,"1055 51608","F & I, 8X8X4 MJ C-153 TEE WYE (SEWER-LINED) WITH MEGA-LUG RESTRAINTS","EA",null,1,0]
[null,"1055 51608A","F & I, 8X8X6 MJ C-153 TEE WYE (WATER) WITH MEGA-LUG RESTRAINTS","EA",null,1,0]
[null,"1055 51608B","F & I, 8X8X8 MJ C-153 TEE WYE (WATER) WITH MEGA-LUG RESTRAINTS","EA",null,1,0]
[null,"1060 15","ADJUST EXISTING SANITARY SEWER MANHOLE RING & COVER","EA",null,2,0]
[null,"1060 16","REMOVE EXISTING SANITARY SEWER MANHOLE AND APPURTENANCES","EA",null,1,0]
[null,"1080 21101","F & I, 1\" SINGLE SHORT (<20FT) WATER SERVICE","EA",null,28,0]
[null,"1080 21101A","F & I, 1\" SINGLE LONG (>20FT) WATER SERVICE","EA",null,1,0]
[null,"1080 21102","F & I, 2\" SINGLE LONG (>20FT) WATER SERVICE","EA",null,1,0]
[null,"1080 21102A","F & I, 2\" DOUBLE SHORT (<20FT)WATER SERVICE","EA",null,2,0]
[null,"1080 23102","F & I, 8” X 2” MAIN TAP WITH 2\" TAPPING VALVE (CORP.) BRANCH CONNECTION WATER MAIN","EA",null,8,0]
[null,"1080 23102A","F & I, 8” X 2” MAIN TAP WITH 2\" TAPPING VALVE (CORP.) BRANCH CONNECTION FORCE MAIN","EA",null,1,0]
[null,"1080 23108","F & I, 8” X 8” MAIN TAP WITH 8\" TAPPING VALVE, AND VALVE BOX WATER MAIN","EA",null,1,0]
[null,"1080 23108A","F & I, 8” X 8” TAPPING SLEEVE, 8\" TAPPING VALVE, 8\" MAIN TAP AND VALVE BOX FORCE MAIN","EA",null,1,0]
[null,"1080 23108B","F & I, 8”X 2”  SERVICE TAPPING SADDLE WITH CORPORATION VALVE  WITH FDEP JUMPER ASSEMBLY WATER MAIN","EA",null,3,0]
[null,"1080 23112","F & I, 12”X 2”  SERVICE TAPPING SADDLE WITH CORPORATION VALVE  WITH FDEP JUMPER ASSEMBLY WATER MAIN","EA",null,1,0]
[null,"1080 23118","F & I, 18” X 12” TAPPING SLEEVE, 12\" TAPPING VALVE, 12\" MAIN TAP, AND VALVE BOX WATER MAIN","EA",null,1,0]
[null,"1080 23118A","F & I, 18”X 2”  SERVICE TAPPING SADDLE WITH CORPORATION VALVE  WITH FDEP JUMPER ASSEMBLY WATER MAIN","EA",null,1,0]
[null,"1080 24102","F & I, 2” RESILIENT SEATED GATE VALVE AND VALVE BOX WATER MAIN ","EA",null,2,0]
[null,"1080 24102A","F & I, 2” RESILIENT SEATED GATE VALVE AND VALVE BOX FORCE MAIN ","EA",null,1,0]
[null,"1080 24102B","F & I, 2 1/2” RESILIENT SEATED GATE VALVE AND VALVE BOX WATER MAIN","EA",null,1,0]
[null,"1080 24103","F & I, 3” RESILIENT SEATED GATE VALVE WITH MEGA-LUG RESTRAINTS AND VALVE BOX FORCE MAIN","EA",null,2,0]
[null,"1080 24104","F & I, 4” RESILIENT SEATED GATE VALVE WITH MEGA-LUG RESTRAINTS AND VALVE BOX FORCE MAIN","EA",null,5,0]
[null,"1080 24106","F & I, 6” RESILIENT SEATED GATE VALVE WITH MEGA-LUG RESTRAINTS AND VALVE BOX WATER MAIN","EA",null,4,0]
[null,"1080 24106A","F & I, 6” RESILIENT SEATED GATE VALVE WITH MEGA-LUG RESTRAINTS AND VALVE BOX","EA",null,2,0]
[null,"1080 24108","F & I, 8” RESILIENT SEATED GATE VALVE WITH MEGA-LUG RESTRAINTS AND VALVE BOX WATER MAIN","EA",null,14,0]
[null,"1080 24108A","F & I, 8” RESILIENT SEATED GATE VALVE WITH MEGA-LUG RESTRAINTS AND VALVE BOX FORCE MAIN","EA",null,7,0]
[null,"1080 24108B","F & I, 8” CHECK VALVE WITH MEGA-LUG RESTRAINTS FORCE MAIN","EA",null,1,0]
[null,"1080 24112","F & I, 12” RESILIENT SEATED GATE VALVE WITH MEGA-LUG RESTRAINTS AND VALVE BOX WATER MAIN","EA",null,5,0]
[null,"1080 24500","ADJUST EXISTING VALVE BOX WATER MAIN","EA",null,3,0]
[null,"1080 24500A","ADJUST EXISTING VALVE BOX FORCE MAIN","EA",null,3,0]
[null,"1080 26102","F & I, 2\" AUTOMATIC AIR RELEASE VALVE ASSEMBLY FORCE MAIN","EA",null,4,0]
[null,"1080 26112","2\" AUTOMATIC AIR RELEASE VALVE ASSEMBLY WATER MAIN","EA",null,1,0]
[null,"1080 26400","F & I, RELOCATE 2\" MANUAL AIR RELEASE VALVE ASSEMBLY FORCE MAIN","EA",null,2,0]
[null,"1080 27106","F & I, 6\" LINE STOP WATER MAIN","EA",null,1,0]
[null,"1080 27108","F & I, 8\" LINE STOP WATER MAIN","EA",null,1,0]
[null,"1080 29104","F & I, 4” MEGA-LUG BELL RESTRAINTS WATER MAIN","EA",null,1,0]
[null,"1080 29106","F & I, 6” MEGA-LUG BELL RESTRAINTS ON EXIST. C.I.P. WATER MAIN","EA",null,5,0]
[null,"1080 29106A","F & I, 6” MEGA-LUG BELL RESTRAINTS FORCE MAIN","EA",null,4,0]
[null,"1080 29108","F & I, 8” MEGA-LUG BELL RESTRAINTS ON EXIST. C.I.P. WATER MAIN","EA",null,5,0]
[null,"1080 29108A","F & I, 8” MEGA-LUG BELL RESTRAINTS FORCE MAIN","EA",null,33,0]
[null,"1080 29112","F & I, 12” MEGA-LUG BELL RESTRAINTS WATER MAIN","EA",null,34,0]
[null,"1080 32108","F & I & R, TEMPORARY SAMPLE POINT AND BLOWOFF ASSEMBLY (8\") WATER MAIN","EA",null,4,0]
[null,"1080 32112","F & I & R, TEMPORARY SAMPLE POINT AND BLOWOFF ASSEMBLY (12\") WATER MAIN","EA",null,12,0]
[null,"1644 11308","F & I, FIRE HYDRANT ASSEMBLY, 6\"GV, 2-6\" ANCHOR COUPLINGS, WITH MAIN CONNECTION AND 42” RISER","EA",null,10,0]
[null,null,"SUB-TOTAL OF UTILITY WORK BY HIGHWAY CONTRACTOR (UWHC)",{"$nulls":3},0]
[null,"0999-25A","FORCE ACCOUNT",{"$nulls":3},{"v":200000,"d":"$200,000.00"}]
[null,"TOTAL BID AMOUNT UTILITY WORK BY HIGHWAY CONTRACTOR (INCLUDING FORCE ACCOUNT)  ",{"$nulls":4},{"v":200000,"d":"200,000.00"}]
[null,"TOTAL BID AMOUNT (INCLUDING FORCE ACCOUNT) SR 60 AND 43RD AVENUE ROADWAY IMPROVEMENTS WITHOUT UWHC (PAGE 00310-11)",{"$nulls":4},{"v":1300000,"d":"$1,300,000.00"}]
[]
[null,"TOTAL BID AMOUNT SR 60 AND 43RD AVENUE ROADWAY IMPROVEMENTS AND UTILITY WORK BY HIGHWAY CONTRACTOR (PAGE 00310-11)",{"$nulls":4},{"v":1500000,"d":"$1,500,000.00"}]
[]
[null,"LS=Lump Sum     MH=Man Hour     ED=Each Day     LF=Linear Foot     EA=Each     SY=Square Yard      Cy=Cubic Yard"]
[null,"TN=Ton     LB=Pound     AS=Assembly     GM=Gross Mile     PI=Per Intersection     CF=Cubic Foot"]
[null,"SF=Square Foot     NM=Net Mile"]
[null,"NOTE: IF THERE IS A DISCREPANCY BETWEEN THE PLANS (SUMMARY OF PAY ITEMS)"]
[null,"AND THE ITEMIZED BID SCHEDULE, THE BID SCHEDULE WILL BE UTILIZED FOR BIDDING PURPOSES."]
[null,"TOTAL PROJECT BID AMOUNT IN WORDS: "]
[null,"  _______________________________________________________________________________________________________________________________________________________________"]