{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Bid Tabulation Sheet"],"not_rendered":{"defined_names":2},"read":"whole","date_system":"1900"}

{"sheet":"Bid Tabulation Sheet","index":0,"n_rows":45,"n_cols":6,"rows_kept":45,"merged":[[0,0,0,5],[44,0,44,4]]}
["Bid Tabulation Sheet"]
["Item\nNumber","Item\nDescription","Qty","Units","Unit Cost","Item Cost"]
["101-1","MOBILIZATION, SURVEY \nAND PRE-CONSTRUCTION VIDEO","LS",{"v":1,"d":"1 "},"$","$"]
["102-1","MAINTENANCE  OF  TRAFFIC","LS",{"v":1,"d":"1 "},"$","$"]
["104-10-3","SEDIMENT  BARRIER  (SILT  FENCE)","LF",{"v":4807,"d":"4,807 "},"$","$"]
["104-11","FLOATING  TURBIDITY  BARRIER","LF",{"v":100,"d":"100 "},"$","$"]
["110-1-1","CLEARING  AND  GRUBBING  (ABOUT 2 AC)","LS",{"v":2,"d":"2 "},"$","$"]
["120-1","REGULAR EXCAVATION","CY",{"v":2724,"d":"2,724 "},"$","$"]
["120-6","EMBANKMENT","CY",{"v":3325,"d":"3,325 "},"$","$"]
["160-4","TYPE B STABILIZATION 12\"","SY",{"v":4667,"d":"4,667 "},"$","$"]
["285-706","OPTIONAL BASE, 8\" LIMEROCK","SY",{"v":380,"d":"380 "},"$","$"]
["285-709","FULL  PAVEMENT  RESTORATION (FULL DEPTH \nBADE REPAIR, OPTIONAL  BASE TYPE B  12.5, 6\")","SY",{"v":875,"d":"875 "},"$","$"]
["327-70-16","MILLING  EXIST.  ASPH.  PAVT., 1/2\" (TURNOUTS)","SY",{"v":1285,"d":"1,285 "},"$","$"]
["327-70-5","MILLING  EXIST.  ASPH.  PAVT., 2\"","SY",{"v":12169.888888888889,"d":"12,170 "},"$","$"]
["334-1-13-1","SUPERPAVE  AC TRAFFIC  C  SP  9.5, \n(LEVELING AND/OR REPAIR)","TN",{"v":113,"d":"113 "},"$","$"]
["334-1-13-1","SUPERPAVE  AC TRAFFIC  C  SP  9.5,  1.5\"  -  \nSURFACE  (TURNOUTS)","TN",{"v":138,"d":"138 "},"$","$"]
["334-1-13-1","SUPERPAVE  AC TRAFFIC  C  SP  9.5, 1\"  -  \nSURFACE","TN",{"v":1130,"d":"1,130 "},"$","$"]
["334-1-13-3","SUPERPAVE  AC TRAFFIC  C  SP  12.5,   2\" -  STRUCTURAL","TN",{"v":2259,"d":"2,259 "},"$","$"]
["334-1-13-4","SUPERPAVE  AC TRAFFIC  C  SP  12.5 - \nOVERBUILD","TN",{"v":823,"d":"823 "},"$","$"]
["430-94-1","DESILTING  PIPE   0-24\"","LF",{"v":563,"d":"563 "},"$","$"]
["430-94-2","DESILTING  PIPE   25-36\"","LF",{"v":75,"d":"75 "},"$","$"]
["430-174-215","PIPE  CULVERT  OPTIONAL  MATERIAL,  \nOTHER, 15\",  SD ","LF",{"v":72,"d":"72 "},"$","$"]
["430-175-130","PIPE  CULVERT  OPTIONAL  MATERIAL,  \nOTHER, 30\",  CD ","LF",{"v":8,"d":"8 "},"$","$"]
["430-982-133","MITERED END SECTION, 30\", 1:2 SLOPE \n(INCLUDES 8 LF OF PIPE)","EA",{"v":1,"d":"1 "},"$","$"]
["522-2-129","CONCRETE DRIVEWAYS,  6\"","SY",{"v":333,"d":"333 "},"$","$"]
["530-3","RIPRAP  (RUBBLE)","TN",{"v":10,"d":"10 "},"$","$"]
["570-1-2","PERFORMANCE  TURF, SOD","SY",{"v":24744.444444444445,"d":"24,744 "},"$","$"]
["700-1-11","SINGLE POST SIGN, F & I GROUND MOUNT, \nUP TO 12 SF","AS",{"v":2,"d":"2 "},"$","$"]
["700-1-11-1","SINGLE POST SIGN, F & I GROUND MOUNT, UP TO \n12 SF (45 MPH SIGN MOUNTED ON EXISTING POLE)","AS",{"v":2,"d":"2 "},"$","$"]
["706-3","RETRO  REFLECTIVE  PAVEMENT  MARKERS","EA",{"v":400,"d":"400 "},"$","$"]
["710-11-101","PAINT  PAVE.  MARKING,  STD. \nWHITE,  SOLID  6\"","GM",{"v":2.85,"d":"2.850"},"$","$"]
["710-11-170","PAINT PAVEMENT MARKING, STD. \nWHITE, ARROWS","EA",{"v":2,"d":"2 "},"$","$"]
["710-11-224","PAINT  PAVE.  MARKING,  STD. \nYELLOW, SOLID/DIAG./CHEVRON,  18\"","LF",{"v":29,"d":"29 "},"$","$"]
["710-11-125","PAINT  PAVE.  MARKING,  STD. \nWHITE,  SOLID  24\"","LF",{"v":160,"d":"160 "},"$","$"]
["710-11-201","PAINT  PAVE.  MARKING,  STD. \nYELLOW,  SOLID  6\"","GM",{"v":2,"d":"2 "},"$","$"]
["710-11-231","PAINT  PAVE.  MARKING,  STD. \nYELLOW,  SKIP  6\"  (10/30)","GM",0.714,"$","$"]
["711-11-224","THERMO,  STD. YELLOW,  SOLID, 18\"  \nFOR   DIAG./  CHEVRON","LF",{"v":29,"d":"29 "},"$","$"]
["711-11-125","THERMO,  STD. WHITE,  SOLID, 24\"  \nFOR   STOP  LINE","LF",{"v":160,"d":"160 "},"$","$"]
["711-11-170","THERMO, STD. WHITE, ARROWS","EA",{"v":2,"d":"2 "},"$","$"]
["711-16-101","THERMO,  STD.,  OTHER  SURFACES, \nWHITE, SOLID  6\"","GM",{"v":2.85,"d":"2.850"},"$","$"]
["711-16-201","THERMO,  STD.,  OTHER  SURFACES, \nYELLOW, SOLID  6\"","GM",{"v":2,"d":"2.000"},"$","$"]
["711-16-231","THERMO,  STD.,  OTHER  SURFACES, \nYELLOW,  SKIP,  6\" (10/30)","GM",0.714,"$","$"]
["915-332-2","FULL DEPTH RECLAMATION (9\")","SY",{"v":8361.444444444445,"d":"8,361 "},"$","$"]
["R-1","GEOTEXTILE PAVEMENT FABRIC \n(PETROMAT OR APPROVED EQUAL)","SY",{"v":6800,"d":"6,800 "},"$","$"]
["Opinion of Probable Construction Cost Total: ",{"$nulls":4},"$"]