ADVERTISEMENT FOR BIDS

  City of Carlsbad	
  101 N. Halagueño Street	
  Carlsbad, New Mexico 88220	

PROJECT NAME:                    Double Eagle Phase 3 Water System Improvements	
CITY’S BID NO.:	  	     2018-15							

Pursuant to the provisions of the New Mexico State Purchasing Act, competitive sealed Bid Proposals for construction will be received for:

A.	Base Bid:
1. Construct approximately  21,160  feet of 24-inch, and  630  feet of 12-inch waterlines with associated shutoff valves, air release/vacuum valve stations, and appurtenances.
2. Construct one (1) jack and bore / trench casing crossing under State Road NM200 for 24-inch waterline.
3. Construct one (1) jack and bore crossing under Railroad for 24-inch waterline.
4. Construct eleven (11) jack and bore / auger and bore crossings under numerous existing utilities for 24-inch waterline.
5. Construct one (1) jack and bore / auger and bore crossing under numerous existing utilities for 12-inch waterline. 
6. Construct the water transmission line facilities within State Land easements, Federal Land (Bureau of Land Management) easements, and private land easements.
7. Construct all work with full compliance of Permit Requirements from the New Mexico Department of Transportation, the United States Department of Interior – Bureau of Land Management, and BNSF Railroad Company.
8. Construct Chlorination Building (approximately  1,040  square feet) including building, chlorine loading and feed system, chlorination system, electrical, and instrumentation with SCADA system.
9. Construct 5-million gallon ground storage reservoir (prestressed concrete) including site development, piping, and flow meter structures.
10. Construct Water Booster Pump Station (approximately  168  square feet) including building, booster pumps, piping, electrical, and instrumentation with SCADA system, and site work.

B.	Additive Alternate “A”:
1. Construct approximately  9,650  feet of 16-inch waterline with associated shutoff valves, air release / vacuum valve stations, and appurtenances.
2. Construct two (2) jack and bore / auger and bore crossings under numerous existing utilities for 16-inch water line.
3. Construct one (1) trench casing crossing over existing utility for 16-inch waterline.


4. Construct the water transmission line facilities within State land easements, Federal land (Bureau of Land Management) easements, and private land easements. 
5. Construct all work with full compliance of Permit Requirements from the United States Department of Interior – Bureau of Land Management.

C.	Additive Alternate “B”:
1.	Construct  20  feet of 16-inch waterline extension with shutoff valve, fittings, and thrust block at end of pipe.

Bid Proposal

Bid Proposal consists of the Bidder’s Qualifications Package (Technical Proposal) and Bidder’s Bid (Price Proposal).  Both must be submitted with the Bid Proposal.  Bidder’s Bid and Bidder’s Qualifications Package must be enclosed in separate sealed envelopes with both sealed envelopes enclosed in one sealed envelope.  Bidder must demonstrate the required qualifications and capabilities, both within its organization and within its subcontractors for this project.  Refer to Qualifications Package section of the Project Manual for qualifications submittal requirements and method for scoring qualifications and Bidder’s price.

Bid Proposals will be received by  the City of Carlsbad, City Hall, 101 North Halagueño Street, Carlsbad, NM 88220 , at the office of  the Purchasing Manager  until  11:00 a.m.  (local time) 
on  November 14, 2018 .  City will complete Evaluation of Bids and Bidder’s Qualifications within ten (10) business days.

Pre-Bid Conference.  A non-mandatory Pre-Bid Conference meeting will be held on 
 October 17, 2018  at  8:30 a.m.  (local time) at:  Water Department, 1502 West Stevens Street, Carlsbad, NM 88220 .  A detailed summary of the scope of work, project limits, and requirements will be presented at the Pre-Bid Meeting.  A limited tour of the project site will be provided by the City.  Schedule for Pre‑Bid Conference:
· Pre-Bid Meeting:	 8:30 a.m.  to  10:00 a.m.  at	Carlsbad Water Department
	1502 West Stevens Street
	Carlsbad, NM 88220
· Site Tour:	 Following Pre-Bid Meeting.	

The CONTRACT DOCUMENTS may be examined at the following locations:
 ARI Graphix (www.arigraphix.com), 4716 McLeod, NE, Albuquerque, NM 87109			
 Construction Reporter, 1607 2nd Street, Albuquerque, NM  87107					
 Dodge Data & Analytics, www.construction.com	



Copies of the CONTRACT DOCUMENTS may be obtained at ARI Graphix (www.ariplans.com), 4716 McLeod, NE, Albuquerque, NM 87109.  Contact ARI Graphix for costs of printing CONTRACT DOCUMENTS (non-refundable) at (505) 884-0862.

TO BE PUBLISHED:   September 30, 2018		 in the Carlsbad Current – Argus
[bookmark: _GoBack]TO BE PUBLISHED:   September 30, 2018	  in the Albuquerque Journal


	Matt Fletcher		Date:   September 27, 2018	
	Chief Procurement Officer
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