{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["Summary","Bid Sheet"],"not_rendered":{"defined_names":2},"read":"whole","date_system":"1900"}

{"sheet":"Summary","index":0,"n_rows":22,"n_cols":6,"rows_kept":22,"merged":[[5,2,5,4],[6,2,6,4],[7,2,7,4],[8,2,8,4],[9,0,10,5]]}
["Department of Environmental Services"]
["Engineering Bureau "]
[]
["2100 Clarendon Boulevard   Suite 813   Arlington, VA 22201"]
["TEL 703.228.3721   FAX 703.228.3606  ",{"$nulls":4},"Version:09/2017"]
[null,null,"PROJECT:",null,null,"P31D"]
[null,null,"DATE:",null,null,{"$f":"TODAY()","v":"2023-05-08"}]
[null,null,"PREPARED BY:",null,null,"K. PATEL"]
[null,null,"REVIEWED BY:",null,null,"ZORAN "]
["Rosslyn - Ballston Corridor ADA Improvements Poject - Phase 2 "]
[]
["SITE","PROJECT NAME",{"$nulls":3},"SITE TOTAL"]
["SITE A-2","Fairfax Dr. & N. Utah St.",{"$nulls":3},{"$f":"E13*1.15","v":0}]
["SITE B-4","Fairfax Dr. & N. Lynn St.",{"$nulls":3},0]
["SITE B-5","N Glebe Rd. & 11th St. N",{"$nulls":3},0]
["SITE C-2","N 14th St. & N Uhle St.",{"$nulls":3},0]
["SITE C-3","N Glebe Rd. & Washington Blvd.",{"$nulls":3},0]
["SITE S-4","10th St. & N Barton St.    ",{"$nulls":3},0]
["SITE S-5","14th St. N. & N. Veitch St. ",{"$nulls":3},0]
["SITE S-8","Clarendon Blvd. & Cleveland St. ",{"$nulls":3},0]
[]
[null,"GRAND TOTAL",null,null,{"$f":"SUM(E13:E21)","v":0},{"$f":"SUM(F13:F21)","v":0}]

{"sheet":"Bid Sheet","index":1,"n_rows":244,"n_cols":8,"rows_kept":244,"merged":[[5,0,6,7],[7,0,8,0],[7,1,8,1],[7,2,8,2],[7,3,8,3],[7,4,8,4],[7,5,8,5],[7,6,8,6],[7,7,8,7],[41,0,42,0],[41,1,42,1],[41,2,42,2],[41,3,42,3],[41,4,42,4],[41,5,42,5],[41,6,42,6],[41,7,42,7],[68,0,69,0],[68,1,69,1],[68,2,69,2],[68,3,69,3],[68,4,69,4],[68,5,69,5],[68,6,69,6],[68,7,69,7],[100,0,101,0],[100,1,101,1],[100,2,101,2],[100,3,101,3],[100,4,101,4],[100,5,101,5],[100,6,101,6],[100,7,101,7],[130,0,131,0],[130,1,131,1],[130,2,131,2],[130,3,131,3],[130,4,131,4],[130,5,131,5],[130,6,131,6],[130,7,131,7],[160,0,161,0],[160,1,161,1],[160,2,161,2],[160,3,161,3],[160,4,161,4],[160,5,161,5],[160,6,161,6],[160,7,161,7],[184,0,185,0],[184,1,185,1],[184,2,185,2],[184,3,185,3],[184,4,185,4],[184,5,185,5],[184,6,185,6],[184,7,185,7],[214,0,215,0],[214,1,215,1],[214,2,215,2],[214,3,215,3],[214,4,215,4],[214,5,215,5],[214,6,215,6],[214,7,215,7]]}
["P31D - Rosslyn - Ballston Corridor ADA Improvements Poject - Phase 2 ",{"$nulls":6},"May 2023"]
["Department of Environmental Services"]
[]
["BID TABULATION"]
[]
["Rosslyn - Ballston Corridor ADA Improvements Poject - Phase 2 "]
[]
["Item Number","Item Code","Arlington County Construction Standards and Specifications Item","Pay Item","Quantity","Unit","Unit Price","Subtotal"]
[]
[null,"A-2, Fairfax Dr. & N. Utah St."]
[1,"01400-C1-00030",{"v":1400,"d":"01400"},"Test Pits (or Test Bores), Up to 6' Deep (with restoration)",3,"EA"]
[2,"02200-C1-00050",{"v":2200,"d":"02200"},"Select Borrow (VDOT Section 207 - Select Material, Type I)",4,"CY"]
[3,"02200-C1-00130",{"v":2200,"d":"02200"},"Aggregate, VDOT #21-A  (Compacted in Place per VDOT standards & Specs)",21,"CY"]
[4,"02750-C2-00040",{"v":2750,"d":"02750"},"Concrete Curb, Standard 6\" (VDOT CG-2), includes curb for aprons, ramps, etc.",70,"LF"]
[5,"02750-C2-00060",{"v":2750,"d":"02750"},"Concrete Curb & Gutter, Standard C-2 and C-2R (Arlington County Detail R-2.0), includes curb & gutter for aprons, ramps, etc.",82,"LF"]
[6,"02750-C2-00070",{"v":2750,"d":"02750"},"Concrete Curb & Gutter, Combination 6\" (VDOT CG-6), includes curb & gutter for aprons, ramps, etc.",25,"LF"]
[7,"02611-C2-00120",{"v":2611,"d":"02611"},"Concrete Sidewalk, 4\" Thickness (Arlington County Detail R-2.0)",125,"SY"]
[8,"02611-C2-00190",{"v":2611,"d":"02611"},"CG-12 Detectable Warning Surface - Truncated Domes",11,"SY"]
[9,"03100-C2-00270",{"v":3100,"d":"03100"},"Provide vent cover as per WMATA Plat L-1, and provide finish transition to impacted exposed wall, includes all labour and materials and obtain nacessary WMATA permits.",1,"LS"]
[10,"02600-C3-00010",{"v":2600,"d":"02600"},"Asphalt Concrete, Planing or Milling (1/2\" to 3\" Depth)",188,"SY"]
[11,"02600-C3-00030",{"v":2600,"d":"02600"},"Asphalt Concrete, Base Course (VDOT BM-25.0A)",7,"TON"]
[12,"02600-C3-00070",{"v":2600,"d":"02600"},"Asphalt Concrete, Surface Course (VDOT SM-9.5D)",25,"TON"]
[13,"13160-C8-03000","Arlington County Traffic Signal Standards","Furnish and install solar powered road side flashing beacon, (RRFB) (includes concrete pole foundation, labour and material ) as shown in drawings.",3,"EA"]
[14,"02900-C10-00010",{"v":2900,"d":"02900"},"Four (4) Inch Transverse Markings",42,"LF"]
[15,"02900-C10-00020",{"v":2900,"d":"02900"},"Six (6) Inch Transverse Markings",170,"LF"]
[16,"02900-C10-00050",{"v":2900,"d":"02900"},"Twenty Four (24) Inch Transverse Markings, Note: Used For Continental (Ladder) Crosswalk",160,"LF"]
[17,"02900-C10-00060",{"v":2900,"d":"02900"},"Yield Line Markings (Twenty Four (24) Inch Triangle/Twelve (12) Inch Spacing), Note: LF is Width of Lane for Units",40,"LF"]
[18,"02900-C10-00080",{"v":2900,"d":"02900"},"Four (4) Inch Longitudinal Skip Line (Ten (10) Foot Line/Thirty (30) Foot Spacing), Note: Forty (40) LF Consists of Ten (10) LF of Marking and Thirty (30) LF of Space",100,"LF"]
[19,"02900-C10-00160",{"v":2900,"d":"02900"},"Six (6) Inch Longitudinal Skip Line (Two (2) Foot Line/ Four (4) Foot Spacing), Note: Twelve (12) LF Consists of Two (2) LF of Marking and Four (4) LF of Space",187,"LF"]
[20,"02900-C10-00170",{"v":2900,"d":"02900"},"Twelve (12) Inch Yellow Longitudinal Centerline, Two - Four (4) Inch Yellow Lines with Four (4) Inch Separation",108,"LF"]
[21,"02900-C10-00320",{"v":2900,"d":"02900"},"Six (6) Foot Bicycle Lane Arrow (Only for Multi-Use or Bikes Opposing Traffic)",1,"EA"]
[22,"02619-C10-00410",{"v":2619,"d":"02619"},"Traffic Control Sign (Typical Stop, Yield, No Parking, Speed Limit, or Similar)",3,"EA"]
[23,"02619-C10-00430",{"v":2619,"d":"02619"},"Traffic Control Sign (Typical Stop, Yield, No Parking, Speed Limit, or Similar), Relocate with New Post",2,"EA"]
[24,"02801-C11-00040",329100,"Shredded hardwood mulch; Aged 6 months minimum - Free of Trash & Debris",1,"CY"]
[25,"02800-C11-00110",{"v":2612,"d":"02612"},"Brick Pavers, Remove and Reset (Arlington County Detail R-2.1)",52,"SY"]
[26,"01500-C13-10000",{"v":1500,"d":"01500"},"Temporary Erosion and Sediment Controls",1,"LS"]
[27,"01000-C16-00010",{"v":1000,"d":"01000"},"Maintenance of Traffic (MOT)",1,"LS"]
[28,"01000-C16-00030",{"v":1000,"d":"01000"},"Mobilization and De-Mobilization",1,"LS"]
[29,"01500-SA-00200",{"v":1500,"d":"01500"},"SWPPP Administration",1,"LS"]
[{"$nulls":6},"TOTAL A-2 ="]
[null,"B-4, Fairfax Dr. & N. Lynn St."]
["Item Number","Item Code","Arlington County Construction Standards and Specifications Item","Pay Item","Quantity","Unit","Unit Price","Subtotal"]
[]
[1,"01400-C1-00030",{"v":1400,"d":"01400"},"Test Pits (or Test Bores), Up to 6' Deep (with restoration)",3,"EA"]
[2,"02200-C1-00050",{"v":2200,"d":"02200"},"Select Borrow (VDOT Section 207 - Select Material, Type I)",12,"CY"]
[3,"02200-C1-00130",{"v":2200,"d":"02200"},"Aggregate, VDOT #21-A  (Compacted in Place per VDOT standards & Specs)",24,"CY"]
[4,"02750-C2-00020",{"v":2750,"d":"02750"},"Concrete Curb, Standard Header Curb C-3 (Arlington County Detail R-2.0), includes curb for aprons, ramps, etc.",47,"LF"]
[5,"02750-C2-00040",{"v":2750,"d":"02750"},"Concrete Curb, Standard 6\" (VDOT CG-2), includes curb for aprons, ramps, etc.",84,"LF"]
[6,"02750-C2-00070",{"v":2750,"d":"02750"},"Concrete Curb & Gutter, Combination 6\" (VDOT CG-6), includes curb & gutter for aprons, ramps, etc.",113,"LF"]
[7,"02611-C2-00120",{"v":2611,"d":"02611"},"Concrete Sidewalk, 4\" Thickness (Arlington County Detail R-2.0)",147,"SY"]
[8,"02611-C2-00190",{"v":2611,"d":"02611"},"CG-12 Detectable Warning Surface - Truncated Domes",7,"SY"]
[9,"02600-C3-00010",{"v":2600,"d":"02600"},"Asphalt Concrete, Planing or Milling (1/2\" to 3\" Depth)",401,"SY"]
[10,"02600-C3-00030",{"v":2600,"d":"02600"},"Asphalt Concrete, Base Course (VDOT BM-25.0A)",5,"TON"]
[11,"02600-C3-00070",{"v":2600,"d":"02600"},"Asphalt Concrete, Surface Course (VDOT SM-9.5D)",50,"TON"]
[12,"02505-C4-01440",{"v":2505,"d":"02505"},"Underdrain, Standard VDOT UD-4",80,"LF"]
[13,"13160-C8-03000","Arlington County Traffic Signal Standards","Furnish and install pedestrian pole, signal head, push button, loop detector (includes concrete pole foundation, labour and material ) as per plan. (per latest Arlington County traffic signal & street light specifications)",1,"LS"]
[14,"02900-C10-00010",{"v":2900,"d":"02900"},"Four (4) Inch Transverse Markings",100,"LF"]
[15,"02900-C10-00050",{"v":2900,"d":"02900"},"Twenty Four (24) Inch Transverse Markings, Note: Used For Continental (Ladder) Crosswalk",260,"LF"]
[16,"02900-C10-00170",{"v":2900,"d":"02900"},"Twelve (12) Inch Yellow Longitudinal Centerline, Two - Four (4) Inch Yellow Lines with Four (4) Inch Separation",115,"LF"]
[17,"02619-C10-00430",{"v":2619,"d":"02619"},"Traffic Control Sign (Typical Stop, Yield, No Parking, Speed Limit, or Similar), Relocate with New Post",1,"EA"]
[18,"02801-C11-00060",329200,"Sod, Tall Fescue/Bluegrass Mixture",24,"SY"]
[19,"02801-C11-00080",329100,"Hedge Row - Remove, Reset, and Mulch (Includes All Labor and Materials)",60,"LF"]
[20,"01500-C13-10000",{"v":1500,"d":"01500"},"Temporary Erosion and Sediment Controls",1,"LS"]
[21,"01000-C16-00010",{"v":1000,"d":"01000"},"Maintenance of Traffic (MOT)",1,"LS"]
[22,"01000-C16-00030",{"v":1000,"d":"01000"},"Mobilization and De-Mobilization",1,"LS"]
[23,"01500-SA-00200",{"v":1500,"d":"01500"},"SWPPP Administration",1,"LS"]
[{"$nulls":6},"TOTAL B -4 ="]
[null,"B-5, N Glebe Rd. & 11th Street N  "]
["Item Number","Item Code","Arlington County Construction Standards and Specifications Item","Pay Item","Quantity","Unit","Unit Price","Subtotal"]
[]
[1,"01400-C1-00030",{"v":1400,"d":"01400"},"Test Pits (or Test Bores), Up to 6' Deep (with restoration)",3,"EA"]
[2,"02200-C1-00050",{"v":2200,"d":"02200"},"Select Borrow (VDOT Section 207 - Select Material, Type I)",5,"CY"]
[3,"02200-C1-00130",{"v":2200,"d":"02200"},"Aggregate, VDOT #21-A  (Compacted in Place per VDOT standards & Specs)",14,"CY"]
[4,"02750-C2-00020",{"v":2750,"d":"02750"},"Concrete Curb, Standard Header Curb C-3 (Arlington County Detail R-2.0), includes curb for aprons, ramps, etc.",32,"LF"]
[5,"02750-C2-00070",{"v":2750,"d":"02750"},"Concrete Curb & Gutter, Combination 6\" (VDOT CG-6), includes curb & gutter for aprons, ramps, etc.",97,"LF"]
[6,"02611-C2-00120",{"v":2611,"d":"02611"},"Concrete Sidewalk, 4\" Thickness (Arlington County Detail R-2.0)",74,"SY"]
[7,"02611-C2-00190",{"v":2611,"d":"02611"},"CG-12 Detectable Warning Surface - Truncated Domes",6,"SY"]
[8,"02613-C2-00150",{"v":2613,"d":"02613"},"Concrete Paver Crosswalk (Arlington County Detail R-2.6, including all materials as shown in detail)",14,"SY"]
[9,"02600-C3-00010",{"v":2600,"d":"02600"},"Asphalt Concrete, Planing or Milling (1/2\" to 3\" Depth)",177,"SY"]
[10,"02600-C3-00030",{"v":2600,"d":"02600"},"Asphalt Concrete, Base Course (VDOT BM-25.0A)",4,"TON"]
[11,"02600-C3-00070",{"v":2600,"d":"02600"},"Asphalt Concrete, Surface Course (VDOT SM-9.5D)",23,"TON"]
[12,"02505-C4-01440",{"v":2505,"d":"02505"},"Underdrain, Standard VDOT UD-4",100,"LF"]
[13,"02505-C4-00470",{"v":2505,"d":"02505"},"Catch Basin Structure Top, Remove & Replace",1,"EA"]
[14,"13160-C8-03000","Arlington County Traffic Signal Standards","Furnish and install loop detector stub-out(includes loop wires in saw cut and installing sealant, labour and material ) as per latest Arlington County traffic signal & street light specifications.",1,"LS"]
[15,"02900-C10-00010",{"v":2900,"d":"02900"},"Four (4) Inch Transverse Markings",50,"LF"]
[16,"02900-C10-00020",{"v":2900,"d":"02900"},"Six (6) Inch Transverse Markings",306,"LF"]
[17,"02900-C10-00050",{"v":2900,"d":"02900"},"Twenty Four (24) Inch Transverse Markings, Note: Used For Continental (Ladder) Crosswalk",116,"LF"]
[18,"02900-C10-00070",{"v":2900,"d":"02900"},"Four (4) Inch Longitudinal Solid Line",115,"LF"]
[19,"02900-C10-00170",{"v":2900,"d":"02900"},"Twelve (12) Inch Yellow Longitudinal Centerline, Two - Four (4) Inch Yellow Lines with Four (4) Inch Separation",115,"LF"]
[20,"02900-C10-00240",{"v":2900,"d":"02900"},"Single Arrows",1,"EA"]
[21,"02619-C10-00430",{"v":2619,"d":"02619"},"Traffic Control Sign (Typical Stop, Yield, No Parking, Speed Limit, or Similar), Relocate with New Post",1,"EA"]
[22,"02801-C11-00040",329100,"Shredded hardwood mulch; Aged 6 months minimum - Free of Trash & Debris",2,"CY"]
[23,"02800-C11-00110",{"v":2612,"d":"02612"},"Brick Pavers, Remove and Reset (Arlington County Detail R-2.1)",16,"SY"]
[24,"02800-C11-SP121",{"v":1500,"d":"01500"},"Decorative Stone, Remove & Reset or Replace to Match Existing",8,"SY"]
[25,"01500-C13-10000",{"v":1500,"d":"01500"},"Temporary Erosion and Sediment Controls",1,"LS"]
[26,"01000-C16-00010",{"v":1000,"d":"01000"},"Maintenance of Traffic (MOT)",1,"LS"]
[27,"01000-C16-00030",{"v":1000,"d":"01000"},"Mobilization and De-Mobilization",1,"LS"]
[28,"01500-SA-00200",{"v":1500,"d":"01500"},"SWPPP Administration",1,"LS"]
[{"$nulls":6},"TOTAL B -5 ="]
[null,"C-2,  N 14th St. & N Uhle St."]
["Item Number","Item Code","Arlington County Construction Standards and Specifications Item","Pay Item","Quantity","Unit","Unit Price","Subtotal"]
[]
[1,"01400-C1-00030",{"v":1400,"d":"01400"},"Test Pits (or Test Bores), Up to 6' Deep (with restoration)",3,"EA"]
[2,"02200-C1-00050",{"v":2200,"d":"02200"},"Select Borrow (VDOT Section 207 - Select Material, Type I)",22,"CY"]
[3,"02200-C1-00130",{"v":2200,"d":"02200"},"Aggregate, VDOT #21-A  (Compacted in Place per VDOT standards & Specs)",26,"CY"]
[4,"02750-C2-00020",{"v":2750,"d":"02750"},"Concrete Curb, Standard Header Curb C-3 (Arlington County Detail R-2.0), includes curb for aprons, ramps, etc.",48,"LF"]
[5,"02750-C2-00060",{"v":2750,"d":"02750"},"Concrete Curb & Gutter, Standard C-2 and C-2R (Arlington County Detail R-2.0), includes curb & gutter for aprons, ramps, etc.",184,"LF"]
[6,"02611-C2-00110",{"v":2611,"d":"02611"},"Concrete Sidewalk, 4\" Thickness (Arlington County Detail R-2.0)",117,"SY"]
[7,"02611-C2-00190",{"v":2611,"d":"02611"},"CG-12 Detectable Warning Surface - Truncated Domes",6,"SY"]
[8,"02611-C2-00180",{"v":2611,"d":"02611"},"Concrete Driveway Entrance, 9\" Thick Commercial (Arlington County Details R-2.4A, R-2.4B, R-2.4C, R-2.4D)",9,"SY"]
[9,"02600-C3-00010",{"v":2600,"d":"02600"},"Asphalt Concrete, Planing or Milling (1/2\" to 3\" Depth)",357,"SY"]
[10,"02600-C3-00030",{"v":2600,"d":"02600"},"Asphalt Concrete, Base Course (VDOT BM-25.0A)",7,"TON"]
[11,"02600-C3-00070",{"v":2600,"d":"02600"},"Asphalt Concrete, Surface Course (VDOT SM-9.5D)",45,"TON"]
[12,"02500-C4-00620",{"v":2500,"d":"02500"},"15\" Pipe, RCP Class III, In Place Up to 6' Deep",8,"LF"]
[13,"02505-C4-00100",{"v":2505,"d":"02505"},"CB-2A or CB-2B (throat lengths from 8'-6\" up to 16'-0\"),  In Place Up to 6' Deep, Arlington County Standards.",1,"EA"]
[14,"02505-C4-00520",{"v":2505,"d":"02505"},"Convert Catch Basin to Manhole",1,"EA"]
[15,"02900-C10-00010",{"v":2900,"d":"02900"},"Four (4) Inch Transverse Markings",112,"LF"]
[16,"02900-C10-00020",{"v":2900,"d":"02900"},"Six (6) Inch Transverse Markings",55,"LF"]
[17,"02900-C10-00040",{"v":2900,"d":"02900"},"Eighteen (18) Inch Transverse Markings",13,"LF"]
[18,"02900-C10-00050",{"v":2900,"d":"02900"},"Twenty Four (24) Inch Transverse Markings, Note: Used For Continental (Ladder) Crosswalk",45,"LF"]
[19,"02900-C10-00170",{"v":2900,"d":"02900"},"Twelve (12) Inch Yellow Longitudinal Centerline, Two - Four (4) Inch Yellow Lines with Four (4) Inch Separation",110,"LF"]
[20,"02619-C10-00430",{"v":2619,"d":"02619"},"Traffic Control Sign (Typical Stop, Yield, No Parking, Speed Limit, or Similar), Relocate with New Post",5,"EA"]
[21,"02801-C11-00060",329200,"Sod, Tall Fescue/Bluegrass Mixture",30,"SY"]
[22,"02800-C11-SP121",{"v":1500,"d":"01500"},"Decorative Stone, Remove & Reset or Replace to Match Existing",25,"SY"]
[23,"01500-C13-10000",{"v":1500,"d":"01500"},"Temporary Erosion and Sediment Controls",1,"LS"]
[24,"01000-C16-00010",{"v":1000,"d":"01000"},"Maintenance of Traffic (MOT)",1,"LS"]
[25,"01000-C16-00030",{"v":1000,"d":"01000"},"Mobilization and De-Mobilization",1,"LS"]
[26,"01500-SA-00200",{"v":1500,"d":"01500"},"SWPPP Administration",1,"LS"]
[{"$nulls":6},"TOTAL C -2 ="]
[null,"C-3, N Glebe Rd. & Washington Blvd."]
["Item Number","Item Code","Arlington County Construction Standards and Specifications Item","Pay Item","Quantity","Unit","Unit Price","Subtotal"]
[]
[1,"01400-C1-00030",{"v":1400,"d":"01400"},"Test Pits (or Test Bores), Up to 6' Deep (with restoration)",2,"EA"]
[2,"02200-C1-00050",{"v":2200,"d":"02200"},"Select Borrow (VDOT Section 207 - Select Material, Type I)",3,"CY"]
[3,"02200-C1-00130",{"v":2200,"d":"02200"},"Aggregate, VDOT #21-A  (Compacted in Place per VDOT standards & Specs)",7,"CY"]
[4,"02750-C2-00020",{"v":2750,"d":"02750"},"Concrete Curb, Standard Header Curb C-3 (Arlington County Detail R-2.0), includes curb for aprons, ramps, etc.",10,"LF"]
[5,"02750-C2-00070",{"v":2750,"d":"02750"},"Concrete Curb & Gutter, Combination 6\" (VDOT CG-6), includes curb & gutter for aprons, ramps, etc.",50,"LF"]
[6,"02611-C2-00120",{"v":2611,"d":"02611"},"Concrete Sidewalk, 4\" Thickness (Arlington County Detail R-2.0)",31,"SY"]
[7,"02611-C2-00190",{"v":2611,"d":"02611"},"CG-12 Detectable Warning Surface - Truncated Domes",2,"SY"]
[8,"02600-C3-00010",{"v":2600,"d":"02600"},"Asphalt Concrete, Planing or Milling (1/2\" to 3\" Depth)",57,"SY"]
[9,"02600-C3-00030",{"v":2600,"d":"02600"},"Asphalt Concrete, Base Course (VDOT BM-25.0A)",3,"TON"]
[10,"02600-C3-00070",{"v":2600,"d":"02600"},"Asphalt Concrete, Surface Course (VDOT SM-9.5D)",8,"TON"]
[11,"02505-C4-01440",{"v":2505,"d":"02505"},"Underdrain, Standard VDOT UD-4",51,"LF"]
[12,"13160-C8-03000","Arlington County Traffic Signal Standards","Furnish and install loop detector stub-out(includes loop wires in saw cut and installing sealant, labour and material ) as per latest Arlington County traffic signal & street light specifications.",1,"LS"]
[13,"02900-C10-00050",{"v":2900,"d":"02900"},"Twenty Four (24) Inch Transverse Markings, Note: Used For Continental (Ladder) Crosswalk",475,"LF"]
[14,"02900-C10-00070",{"v":2900,"d":"02900"},"Four (4) Inch Longitudinal Solid Line",210,"LF"]
[15,"02900-C10-00080",{"v":2900,"d":"02900"},"Four (4) Inch Longitudinal Skip Line (Ten (10) Foot Line/Thirty (30) Foot Spacing), Note: Forty (40) LF Consists of Ten (10) LF of Marking and Thirty (30) LF of Space",75,"LF"]
[16,"02900-C10-00100",{"v":2900,"d":"02900"},"Four (4) Inch Longitudinal Skip Line (Two (2) Foot Line/Ten (10) Foot Spacing), Note: Twelve (12) LF Consists of Two (2) LF of Marking and Ten (10) LF of Space, **Turn Lane Skips**",60,"LF"]
[17,"02900-C10-00120",{"v":2900,"d":"02900"},"Six (6) Inch Longitudinal Solid Line",130,"LF"]
[18,"02900-C10-00170",{"v":2900,"d":"02900"},"Twelve (12) Inch Yellow Longitudinal Centerline, Two - Four (4) Inch Yellow Lines with Four (4) Inch Separation",75,"LF"]
[19,"02900-C10-00240",{"v":2900,"d":"02900"},"Single Arrows",3,"EA"]
[20,"02619-C10-00430",{"v":2619,"d":"02619"},"Traffic Control Sign (Typical Stop, Yield, No Parking, Speed Limit, or Similar), Relocate with New Post",2,"EA"]
[21,"02801-C11-00040",329100,"Shredded hardwood mulch; Aged 6 months minimum - Free of Trash & Debris",1,"CY"]
[22,"02800-C11-00110",{"v":2612,"d":"02612"},"Brick Pavers, Remove and Reset (Arlington County Detail R-2.1)",7,"SY"]
[23,"01500-C13-10000",{"v":1500,"d":"01500"},"Temporary Erosion and Sediment Controls",1,"LS"]
[24,"01000-C16-00010",{"v":1000,"d":"01000"},"Maintenance of Traffic (MOT)",1,"LS"]
[25,"01000-C16-00030",{"v":1000,"d":"01000"},"Mobilization and De-Mobilization",1,"LS"]
[26,"01500-SA-00200",{"v":1500,"d":"01500"},"SWPPP Administration",1,"LS"]
[{"$nulls":6},"TOTAL C -3 ="]
[null,"S-4, 10th St. & N Barton St.    "]
["Item Number","Item Code","Arlington County Construction Standards and Specifications Item","Pay Item","Quantity","Unit","Unit Price","Subtotal"]
[]
[1,"01400-C1-00030",{"v":1400,"d":"01400"},"Test Pits (or Test Bores), Up to 6' Deep (with restoration)",2,"EA"]
[2,"02200-C1-00050",{"v":2200,"d":"02200"},"Select Borrow (VDOT Section 207 - Select Material, Type I)",4,"CY"]
[3,"02200-C1-00130",{"v":2200,"d":"02200"},"Aggregate, VDOT #21-A  (Compacted in Place per VDOT standards & Specs)",7,"CY"]
[4,"02750-C2-00020",{"v":2750,"d":"02750"},"Concrete Curb, Standard Header Curb C-3 (Arlington County Detail R-2.0), includes curb for aprons, ramps, etc.",30,"LF"]
[5,"02750-C2-00060",{"v":2750,"d":"02750"},"Concrete Curb & Gutter, Standard C-2 and C-2R (Arlington County Detail R-2.0), includes curb & gutter for aprons, ramps, etc.",10,"LF"]
[6,"02750-C2-00070",{"v":2750,"d":"02750"},"Concrete Curb & Gutter, Combination 6\" (VDOT CG-6), includes curb & gutter for aprons, ramps, etc.",50,"LF"]
[7,"02611-C2-00110",{"v":2611,"d":"02611"},"Concrete Sidewalk, 4\" Thickness (Arlington County Detail R-2.0)",27,"SY"]
[8,"02611-C2-00190",{"v":2611,"d":"02611"},"CG-12 Detectable Warning Surface - Truncated Domes",2,"SY"]
[9,"02600-C3-00010",{"v":2600,"d":"02600"},"Asphalt Concrete, Planing or Milling (1/2\" to 3\" Depth)",157,"SY"]
[10,"02600-C3-00030",{"v":2600,"d":"02600"},"Asphalt Concrete, Base Course (VDOT BM-25.0A)",2,"TON"]
[11,"02600-C3-00060",{"v":2600,"d":"02600"},"Asphalt Concrete, Surface Course (VDOT SM-9.5A)",20,"TON"]
[12,"02900-C10-00040",{"v":2900,"d":"02900"},"Eighteen (18) Inch Transverse Markings",22,"LF"]
[13,"02900-C10-00050",{"v":2900,"d":"02900"},"Twenty Four (24) Inch Transverse Markings, Note: Used For Continental (Ladder) Crosswalk",250,"LF"]
[14,"02900-C10-00070",{"v":2900,"d":"02900"},"Four (4) Inch Longitudinal Solid Line",220,"LF"]
[15,"02900-C10-00170",{"v":2900,"d":"02900"},"Twelve (12) Inch Yellow Longitudinal Centerline, Two - Four (4) Inch Yellow Lines with Four (4) Inch Separation",40,"LF"]
[16,"02801-C11-00070",329200,"Sod, Zoysia",4,"SY"]
[17,"01500-C13-10000",{"v":1500,"d":"01500"},"Temporary Erosion and Sediment Controls",1,"LS"]
[18,"01000-C16-00010",{"v":1000,"d":"01000"},"Maintenance of Traffic (MOT)",1,"LS"]
[19,"01000-C16-00030",{"v":1000,"d":"01000"},"Mobilization and De-Mobilization",1,"LS"]
[20,"01500-SA-00200",{"v":1500,"d":"01500"},"SWPPP Administration",1,"LS"]
[{"$nulls":6},"TOTAL S -4 ="]
[null,"S-5, 14th St. N. & N. Veitch St. "]
["Item Number","Item Code","Arlington County Construction Standards and Specifications Item","Pay Item","Quantity","Unit","Unit Price","Subtotal"]
[]
[1,"02200-C1-00010",{"v":2200,"d":"02200"},"General excavation, only when not included in other pay items.",60,"CY"]
[2,"01400-C1-00030",{"v":1400,"d":"01400"},"Test Pits (or Test Bores), Up to 6' Deep (with restoration)",3,"EA"]
[3,"02200-C1-00050",{"v":2200,"d":"02200"},"Select Borrow (VDOT Section 207 - Select Material, Type I)",29,"CY"]
[4,"02200-C1-00130",{"v":2200,"d":"02200"},"Aggregate, VDOT #21-A  (Compacted in Place per VDOT standards & Specs)",85,"CY"]
[5,"02750-C2-00020",{"v":2750,"d":"02750"},"Concrete Curb, Standard Header Curb C-3 (Arlington County Detail R-2.0), includes curb for aprons, ramps, etc.",36,"LF"]
[6,"02750-C2-00060",{"v":2750,"d":"02750"},"Concrete Curb & Gutter, Standard C-2 and C-2R (Arlington County Detail R-2.0), includes curb & gutter for aprons, ramps, etc.",335,"LF"]
[7,"02611-C2-00110",{"v":2611,"d":"02611"},"Concrete Sidewalk, 4\" Thickness (Arlington County Detail R-2.0)",322,"SY"]
[8,"02611-C2-00190",{"v":2611,"d":"02611"},"CG-12 Detectable Warning Surface - Truncated Domes",12,"SY"]
[9,"02600-C3-00010",{"v":2600,"d":"02600"},"Asphalt Concrete, Planing or Milling (1/2\" to 3\" Depth)",992,"SY"]
[10,"02600-C3-00030",{"v":2600,"d":"02600"},"Asphalt Concrete, Base Course (VDOT BM-25.0A)",133,"TON"]
[11,"02600-C3-00060",{"v":2600,"d":"02600"},"Asphalt Concrete, Surface Course (VDOT SM-9.5A)",123,"TON"]
[12,"02900-C10-00040",{"v":2900,"d":"02900"},"Eighteen (18) Inch Transverse Markings",72,"LF"]
[13,"02900-C10-00050",{"v":2900,"d":"02900"},"Twenty Four (24) Inch Transverse Markings, Note: Used For Continental (Ladder) Crosswalk",400,"LF"]
[14,"02900-C10-00070",{"v":2900,"d":"02900"},"Four (4) Inch Longitudinal Solid Line",180,"LF"]
[15,"02900-C10-00170",{"v":2900,"d":"02900"},"Twelve (12) Inch Yellow Longitudinal Centerline, Two - Four (4) Inch Yellow Lines with Four (4) Inch Separation",160,"LF"]
[16,"02619-C10-00420",{"v":2619,"d":"02619"},"Traffic Control Sign (Typical Stop, Yield, No Parking, Speed Limit, or Similar), Relocate with Existing Post",2,"EA"]
[17,"02619-C10-00430",{"v":2619,"d":"02619"},"Traffic Control Sign (Typical Stop, Yield, No Parking, Speed Limit, or Similar), Relocate with New Post",4,"EA"]
[18,"02800-C11-00030",329100,"Topsoil for Street Trees, Purchased Mixture (per Arlington County DPR Specification)",2,"CY"]
[19,"02801-C11-00040",329100,"Shredded hardwood mulch; Aged 6 months minimum - Free of Trash & Debris",24,"CY"]
[20,"02801-C11-00070",329200,"Sod, Zoysia",39,"SY"]
[21,"02800-C11-00110",{"v":2612,"d":"02612"},"Brick Pavers, Remove and Reset (Arlington County Detail R-2.1)",79,"SY"]
[22,"02800-C11-SP121",{"v":1500,"d":"01500"},"Decorative Stone, Remove & Reset or Replace to Match Existing",10,"SY"]
[23,"01500-C13-10000",{"v":1500,"d":"01500"},"Temporary Erosion and Sediment Controls",1,"LS"]
[24,"01000-C16-00010",{"v":1000,"d":"01000"},"Maintenance of Traffic (MOT)",1,"LS"]
[25,"01000-C16-00030",{"v":1000,"d":"01000"},"Mobilization and De-Mobilization",1,"LS"]
[26,"01500-SA-00200",{"v":1500,"d":"01500"},"SWPPP Administration",1,"LS"]
[{"$nulls":6},"TOTAL S -5 ="]
[null,"S-8, Clarendon Blvd. & Cleveland St. "]
["Item Number","Item Code","Arlington County Construction Standards and Specifications Item","Pay Item","Quantity","Unit","Unit Price","Subtotal"]
[]
[1,"02200-C1-00050",{"v":2200,"d":"02200"},"Select Borrow (VDOT Section 207 - Select Material, Type I)",20,"CY"]
[2,"02200-C1-00130",{"v":2200,"d":"02200"},"Aggregate, VDOT #21-A  (Compacted in Place per VDOT standards & Specs)",37,"CY"]
[3,"02750-C2-00020",{"v":2750,"d":"02750"},"Concrete Curb, Standard Header Curb C-3 (Arlington County Detail R-2.0), includes curb for aprons, ramps, etc.",25,"LF"]
[4,"02750-C2-00060",{"v":2750,"d":"02750"},"Concrete Curb & Gutter, Standard C-2 and C-2R (Arlington County Detail R-2.0), includes curb & gutter for aprons, ramps, etc.",215,"LF"]
[5,"02611-C2-00110",{"v":2611,"d":"02611"},"Concrete Sidewalk, 4\" Thickness (Arlington County Detail R-2.0)",249,"SY"]
[6,"02611-C2-00190",{"v":2611,"d":"02611"},"CG-12 Detectable Warning Surface - Truncated Domes",10,"SY"]
[7,"02600-C3-00010",{"v":2600,"d":"02600"},"Asphalt Concrete, Planing or Milling (1/2\" to 3\" Depth)",576,"SY"]
[8,"02600-C3-00030",{"v":2600,"d":"02600"},"Asphalt Concrete, Base Course (VDOT BM-25.0A)",9,"TON"]
[9,"02600-C3-00060",{"v":2600,"d":"02600"},"Asphalt Concrete, Surface Course (VDOT SM-9.5A)",72,"TON"]
[10,"02900-C10-00040",{"v":2900,"d":"02900"},"Eighteen (18) Inch Transverse Markings",35,"LF"]
[11,"02900-C10-00050",{"v":2900,"d":"02900"},"Twenty Four (24) Inch Transverse Markings, Note: Used For Continental (Ladder) Crosswalk",290,"LF"]
[12,"02900-C10-00060",{"v":2900,"d":"02900"},"Yield Line Markings (Twenty Four (24) Inch Triangle/Twelve (12) Inch Spacing), Note: LF is Width of Lane for Units",25,"LF"]
[13,"02900-C10-00070",{"v":2900,"d":"02900"},"Four (4) Inch Longitudinal Solid Line",350,"LF"]
[14,"02900-C10-00080",{"v":2900,"d":"02900"},"Four (4) Inch Longitudinal Skip Line (Ten (10) Foot Line/Thirty (30) Foot Spacing), Note: Forty (40) LF Consists of Ten (10) LF of Marking and Thirty (30) LF of Space",300,"LF"]
[15,"02900-C10-00120",{"v":2900,"d":"02900"},"Six (6) Inch Longitudinal Solid Line",150,"LF"]
[16,"02900-C10-00170",{"v":2900,"d":"02900"},"Twelve (12) Inch Yellow Longitudinal Centerline, Two - Four (4) Inch Yellow Lines with Four (4) Inch Separation",100,"LF"]
[17,"02900-C10-00290",{"v":2900,"d":"02900"},"Standard Bicycle Symbols (MUTCD, Chapter 9C, Figure 9C-3), \"Bike Symbol\", \"Helmeted Bicyclist Symbol\"",2,"EA"]
[18,"02900-C10-00350",{"v":2900,"d":"02900"},"Colorized Bike Lane Coatings (per Specification 02900)",16,"SY"]
[19,"02619-C10-00410",{"v":2619,"d":"02619"},"Traffic Control Sign (Typical Stop, Yield, No Parking, Speed Limit, or Similar)",4,"EA"]
[20,"02619-C10-00430",{"v":2619,"d":"02619"},"Traffic Control Sign (Typical Stop, Yield, No Parking, Speed Limit, or Similar), Relocate with New Post",2,"EA"]
[21,"02800-C11-00030",329100,"Topsoil for Street Trees, Purchased Mixture (per Arlington County DPR Specification)",4,"CY"]
[22,"02801-C11-00040",329100,"Shredded hardwood mulch; Aged 6 months minimum - Free of Trash & Debris",4,"CY"]
[23,"02801-C11-00070",329200,"Sod, Zoysia",36,"SY"]
[24,"01500-C13-10000",{"v":1500,"d":"01500"},"Temporary Erosion and Sediment Controls",1,"LS"]
[25,"01000-C16-00010",{"v":1000,"d":"01000"},"Maintenance of Traffic (MOT)",1,"LS"]
[26,"01000-C16-00030",{"v":1000,"d":"01000"},"Mobilization and De-Mobilization",1,"LS"]
[27,"01500-SA-00200",{"v":1500,"d":"01500"},"SWPPP Administration",1,"LS"]
[{"$nulls":6},"TOTAL S -8 ="]