{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet2"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet2","index":0,"n_rows":23,"n_cols":6,"rows_kept":23,"merged":[[0,0,0,5]]}
["PD 18-19.009 Resurfacing Group 18-19"]
[null,"Districts 1-5 Overall Quantities"]
["Item Number","Discription","Qty","Units","Unit Cost","Ext Cost"]
[1,"Mobilization",1,"LS",null,{"$f":"C4*E4","v":{"v":0,"d":"$0.00"}}]
[{"$f":"A4+1","v":2},"Striping",1,"LS",null,{"v":0,"d":"$0.00"}]
[3,"Remove Sand, Silt, & Vegetation From Existing Curb and Gutter ",{"v":121513.68075000001,"d":"121514"},"LF",null,{"v":0,"d":"$0.00"}]
[{"$f":"A6+1","v":4},"Earthwork Excavation by machine",{"v":12039.720000000001,"d":"12040"},"CY",null,{"v":0,"d":"$0.00"}]
[{"$f":"A7+1","v":5},"Final grading and seal rolling prior to paving",{"v":230407.48500000002,"d":"230407"},"SY",null,{"v":0,"d":"$0.00"}]
[6,"Disk Up Existing Turf and Redress To Grade (Does not include Seed and Mulch) over 1500sy",{"v":31220.805000000004,"d":"31221"},"SY",null,{"v":0,"d":"$0.00"}]
[7,"1 1/2\" County Spec 2500 Type SP 12.5 Asphalt Concrete Surface, over 1500sy",{"v":218274.21000000002,"d":"218274"},"SY",null,{"v":0,"d":"$0.00"}]
[8,"2\" County Spec 2500 Type SP 12.5 Asphalt, less than 1500sy",{"v":12133.275000000003,"d":"12133"},"SY",null,{"v":0,"d":"$0.00"}]
[9,"Mill Existing Asphalt, 1.5\" - 3\" Thickness, over 1500sy ",{"v":230407.48500000002,"d":"230407"},"SY",null,{"v":0,"d":"$0.00"}]
[10,"12\" Stabilized Subgrade, County Spec 2300, over 1000sy",{"v":72328.41000000002,"d":"72328"},"SY",null,{"v":0,"d":"$0.00"}]
[11,"6\" Graded aggregate Base \"Min. LBR 100 at 100% Modified Proctor\", County Spec 2400, over 1000sy",{"v":72328.41000000002,"d":"72328"},"SY",null,{"v":0,"d":"$0.00"}]
[12,"Construct  3 5/8\" Speed Table, includes Street Print, White Temporary, and Thermoplastic Pavement Markings as per County Detail and MUTCD",11,"EA",null,{"v":0,"d":"$0.00"}]
[13,"Remove Existing Speed Hump",11,"EA",null,{"v":0,"d":"$0.00"}]
[14,"Valley Gutter Section, 6\" thick, Per County Detail",84,"SY",null,{"v":0,"d":"$0.00"}]
[15,"Remove Existing Concrete, 6\" thick",{"v":25.200000000000003,"d":"25"},"SY",null,{"v":0,"d":"$0.00"}]
[16,"Remove & Repour by Hand Existing Broken Curb & Gutter",{"v":16170.000000000002,"d":"16170"},"LF",null,{"v":0,"d":"$0.00"}]
[17,"Adjust Existing Manhole Tops (Rings and Boxes To Be Provided By Contractor) includes concrete collar",{"v":137.55,"d":"138"},"EA",null,{"v":0,"d":"$0.00"}]
[18,"Centipede Sod, Staked, less than 1000sy",{"v":30453.885000000002,"d":"30454"},"SY",null,{"v":0,"d":"$0.00"}]
[]
[{"$nulls":4},"Grand Total",{"$f":"SUM(F4:F22)","v":{"v":0,"d":"$0.00"}}]