{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":47,"n_cols":5,"rows_kept":47,"merged":[[0,0,0,4]]}
["EMW 4-Inch Expansion - Bill of Materials"]
["Material Type","Item #","Quantity","Size","Description"]
["Pipe & Tubing",null,20,"2 Inch","Pipe, Bare C.S., 2.375\" O.D. ERW, 0.154\" W.T., Grade X-46 or greater, Single Randon Joints"]
[null,null,3800,"4 Inch","Pipe, C.S., 4.5\" O.D., ERW, 0.156\" W.T., Grade X-46 or greater, Fusion Bonded Epoxy Coated, 12-14 Mils, double random"]
[null,null,20,"4 Inch","Pipe, Bare C.S., 4.5\" O.D., ERW, 0.237\" W.T., Grade X-46 or greater"]
[null,null,400,"4 Inch","Pipe, C.S., 4.5\" O.D., ERW, 0.237\" W.T., Grade X-46 or greater, 12-14 mil initial FBE with Dual Layered Fusion Bonded Epoxy Coated w/ outer ARO Coating, double random"]
[null,null,80,"4 Inch","Pipe, C.S., 4.5\" O.D., ERW, 0.237\" W.T., Grade X-46 or greater, Fusion Bonded Epoxy Coated, 12-14 Mils, double random"]
[null,null,{"$f":"[1]Counts!W13","v":1},"1-1/2 inch  x 1 inch","Pipe, Swage Nipple, TBE, SMLS, 1-1/2\" x 1\", SCH. 40,  Straight"]
[null,null,4,"1 Inch x 4 Inch","Pipe, Nipple, TBE, SMLS, 1\" x 4\",  SCH. 80, Straight"]
[null,null,4,"4 Inch x 1 Inch","Thread-O-Let, 4\" x 1\", CL 3000"]
[null,null,1,"4 Inch x 2 Inch","Weld-O-Let, 4\" x 2\", CL 3000"]
["Valves",null,{"$f":"[1]Counts!B29","v":1},"1/2 Inch ","Valve, Ball, 1/2\" Nominal Size, Full Port, Stainless, Threaded, NPT, 3,000 psi., Balon, LM-05361, w/ locking handle"]
[null,null,4,"1 Inch ","Valve, Ball, 1\" Nominal Size, Full Port, Stainless, Threaded, NPT, 2,000 psi., Balon,  LM-10361, w/ locking handle"]
[null,null,1,"2 Inch","Valve, Ball,  2\" Nominal Size, Floating,  C.S., Thread x Thread, 2500 psi,  Balon, 2F-S93-SE"]
[null,null,{"$f":"[1]Counts!B23","v":1},"2 Inch","Valve, Ball,  2\" Nominal Size, Floating,  C.S., Flange x Flange, ANSI 150,  Balon, 2F-F13-RF"]
[null,null,2,"4 Inch","Valve, Ball,  4\" Nominal Size, Floating, C.S., Weld x Weld, ANSI 150, Balon, 4F-US13-BW"]
[null,null,2,"4 Inch","Valve, Ball,  4\" Nominal Size, Floating,  C.S., Flange x Flange, ANSI 150,  Balon, 4F-F13-RF"]
["Filters & Strainers",null,1,"4 Inch","Strainer, Y-Style, 4\" Nominal Size, C.S., Flange x Flange, ANSI 150, Mueller, Model 781 - Furnished by EMW"]
["Measurment Components",null,{"$f":"[1]Counts!N19","v":1},"2 Inch","Meter, Ultrasonic, 2\" Nominal Size, Flange x Flange, ANSI 150, SICK, FLOWSICFS500 - Furnisher by EMW"]
[null,null,1,"4 Inch","Insulation Kit, 4\" Nominal Size, Flange, ANSI 150, PSI Line-Backer, Type F - Furnished by EMW"]
["Elbows & Field Bends",null,1,"2 Inch","Elbow, 2\", Weld End, C.S., 90 Degree, Long Radius, STND. SCH., WPB"]
[null,null,{"$f":"[1]Counts!N27","v":4},"4 Inch","Elbow, 4\", Weld End, C.S., 90 Degree, Long Radius, STND. SCH., WPB"]
["Flanges, Gaskets & Stud Bolts",null,5,"4 Inch","Flange, Weld Neck, 4\" Nominal Size, RF, STND Bore, WPB, ANSI 150"]
["Flanges, Gaskets & Stud Bolts",null,{"$f":"[1]Counts!T5","v":2},"2 Inch","Flange, Weld Neck, 2\" Nominal Size, RF, STND Bore, WPB, ANSI 150"]
[null,null,{"$f":"[1]Counts!W5","v":2},"2 Inch","Flange, Flat Faced, 2\" Nominal Size, RF, STND Bore, WPB, ANSI 150"]
[null,null,2,"2 Inch","Gasket, 2\" Nominal Size, ANSI 150, Spiral-Wound, Flexitallic, CG"]
[null,null,2,"2 inch","Gasket, 2\" Nominal Size, ANSI 150, Garlock - For SICK Meter - Furnished by EMW"]
[null,null,{"$f":"[1]Counts!Q8","v":5},"4 Inch","Gasket, 4\" Nominal Size, ANSI 150, Spiral-Wound, Flexitallic, CG"]
[null,null,8,"5/8 Inch x 3-1/4 Inch","Stud Bolts, 5/8\" x 3-1/4\" with B7, 2 Hex-Nuts for 2\" ANSI 150 Flanges"]
[null,null,{"$f":"[1]Counts!Q11","v":40},"5/8 Inch x 3-1/2 Inch","Stud Bolts, 5/8\" x 3-1/4\" with B7, 2 Hex-Nuts for 4\" ANSI  150 Flanges"]
[null,null,8,"5/8 Inch x 4-1/2 Inch","Stud Bolts, 5/8\" x 4-1/2\" with B7, 2 Hex-Nuts for 4\" ANSI  150 Flanges with Insulating Kit"]
[null,null,8,"5/8 Inch x 2-1/2 Inch","SICK Machine Bolts, 5/8\" x 2-1/2\" for 2\" SICK FS500 Ultrasonic meter - Furnished by EMW"]
["Reducers",null,4,"4 Inch x 2 Inch","Reducer, Weld End, C.S., 4\" x 2\", Standard SCH, Grade B"]
["Tees & Branch Connections",null,4,"4 Inch x 4 Inch x 4 Inch","Tee, Weld End, C.S., Straight, 4\" x 4\" x 4\", Standard SCH, Grade B"]
[null,null,1,"4 Inch","Cap, Weld End, C.S., Straight, 4\" , Standard SCH, Grade B"]
["Caps & Plugs",null,{"$f":"[1]Counts!T17","v":4},"1 Inch x 1/4 Inch","Bushing,  Forged steel, 1\" x 1/4\", 2000 psi"]
[null,null,{"$f":"[1]Counts!T17","v":4},"1/4 Inch","Plug, 1/4\", Steel Solid steel, 2000 psi"]
[null,null,{"$f":"[1]Counts!T19","v":1},"1/2 Inch","Plug, 1/2\", Steel Solid steel, 2000 psi"]
[null,null,1,"2 Inch","Plug, 2\", Steel Solid steel, 2000 psi"]
["Miscellaneous Components",null,{"$f":"[1]Counts!Q21","v":2},"4 Inch ","Pipe Supports, 2\" to 4\", E-Z Line, Figure A, 204A 4\" PS D=60 inches"]
[null,null,{"$f":"[1]Counts!Q19","v":1},1,"Sleeper Support, 24\" x 48\" x 6\", Concrete Quikrete Bags"]
[null,null,{"$f":"[1]Counts!B17","v":2},"6 Inch Dia.","Valve Box, 4\" Nominal Size, Part #G6HAT3ACD, Handley Industries"]
[null,null,{"$f":"[1]Counts!B17","v":2},"12 Dia. ","Supports, SonaTube, 12\" Diameter  36\" Long."]
[]
[{"$nulls":4},"Polyken primer #1027"]
[{"$nulls":4},"Polyken tape - 930-35"]
[{"$nulls":4},"Dirax shrink sleeves - for bore pipe"]