
Tandem Dump Truck Specifications
ITB #2021-07-014 ROAD DEPARTMENT



	
	MODEL AND YEAR, MINIMUM SPECIFICATIONS

	
Notes to Bidder:
	
Dump trucks are to be used for transporting dirt and gravel for road constructions.

	
	Truck, Conventional Cab and Chassis, Tandem Axle, Manual Transmission, with GVWR 54,320 minimum with dump body for this class truck chassis,

	
	
ALL SPECIFICATION CONSIDRED MINIMUM

	Equipment
	
GENERAL Description

	Year model
	New or Used Model 2012 or Newer

	
Engine
	Diesel 390 Hp Minimum

	
Aspiration
	Turbo Charged with Air-to-Air intercoolers Filter Spin On Type

	
Engine retard
	Not required

	
Transmission
	MAN-8LL

	
Torque
	Minimum 1100 pound

	
Clutch
	Required

	
Front axle
	
14,300 LB

	
Rear axle
	40,000 LB

	Rear axle ratio
	4.11. Required OR Rated for this configuration

	
Rear axle spacing
	Vendor shall work with body builder on mounting distance

	
Front springs
	
Air track system

	
Power Steering
	Power Steering

	
Suspension rear
	40,000 LB

	

Frame
	
Truck Manufacturer and Body Builder Recommendation

	






Dump Truck Body
	
16-yard capacity Steel construction Telescopic Hoist Asphalt lip on back Air latch tailgate Black in color
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Air dryer
	
Heated Air dryer. Unit(s) shall meet requirements of truck manufacturer for
proper operation of air system, brake system, number of axles, and weight rating of truck."

	
Air compressor
	Unit(s) shall meet requirements of truck manufacturer for proper operation of air system, brake system, number of axles, and weight rating of m truck.

	

Air tank
	Unit(s) shall meet requirements of truck manufacturer for proper operation of air system, brake system, number of axles, and weight rating of with manual drain valve truck.

	
Brakes
	Air Cam-Type Abs With Automatic Slack Adjusters

	Parking brake
	
Cab Controlled

	
Cab
	
MFG Standard Conventional

	
Cab to include
	Minimum (1) cup holder, dome light, MFG standard, 1 ea. grab handle on each side, steps - both sides

	

Cab trim
	To include MFG standard cab trim panels, door trim panels required, headliner to be soft padded cloth or vinyl, flooring to be heavy duty vinyl or rubber, sun
visors required driver and passenger padded vinyl

	

Seat driver
	Air suspension, high back with integral headrest with fore, aft and height adjustments and recline. Cloth with dual armrest with 3-point seat belt.

	

Seat passenger
	
Non suspension, high back, with integral headrest, vinyl, fixed back, dual armrest with 3-point seat belt, lap and shoulder belt type.

	

Gauge cluster/ instrument panel/data center
	Gauge cluster includes engine oil pressure (electronic) water temperature (electronic), fuel (electronic), tachometer (electronic), voltmeter, odometer display, miles, trip miles, engine hours, fault code readout: warning system low fuel, low oil pressure, high engine coolant temp, and low battery voltage (visual and audible): fuel economy, trip information, diagnostics, warning alarm will
sound when headlights are left on

	

Mirrors
	
(2) Power Adjustable Rectangular

	
Air conditioning/ heat
	
Factory installed w/ integrated defrost

	
Grill/ hood
	
Conventional tilt

	
Exterior color (WHITE)
	
Fleet White

	
Steering column
	
Tilt

	
Exhaust
	
MFG Standard Vertical Tailpipe To Include Turn Out And Guard

	Electrical
	12-Volt, Standard Equipment
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To include
	Mfg. standard data link connector for vehicle programming and diagnostics in cab, hazard switch push on /push off, head light dimmer switch w/ turn signal lever, horn electric single, starter switch electric key operated, windshield wiper switch 2- speed with wash and intermittent with MFR standard wind shield
wipers

	
Tires
	

11r 24.5 Ply Steer Tires

	Headlights
	
Sealed Beam

	Marker lighting control
	Not required

	Clearance/marker
	
(4) truck lite amber factory installed on cab or sunshade

	Stop, turn, tail & b/u
	
Flange mounted with two backup lights

	Power outlet
	
n/a

	Alternator
	
12 Volt 130 Minimum

	Batteries
	2500cca
2 batteries minimum

	Jump start stud
	
On battery under step

	Battery box
	
MFR standard

	Radio
	
AM/FM with weather band, clock w/ two dual cone speakers in cab.

	Cb
	
Power connections one pair on dash

	
Horn
	Air Solenoid Operated Single or Dual Acceptable Please Consider Location Due To Cab Shield For Dump Body

	Backup alarm
	87-112 decibels, adjusts automatically per OHSA

	Engine block heater
	Not required

	Air cleaner
	
Dry type, single element

	Fuel/water separator
	
Required

	Fuel tank
	
Minimum 70-gallon aluminum tank

	Def tank
	
Factory spec

	Wheel’s front
	
24.5 steel wheel, hub piloted
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