	SPECIFICATIONS FOR Auger Boring Machine & Augers

	

	EXCEPTIONS: The Bidder must list any exceptions (major & minor) to the specifications. The Bidder must prove "an equal" in writing with literature.  This information must be in the bid package and cannot be supplied at a later date. Failure to list all exceptions either in the space provided or on a separate page will be cause for rejection

	

	DETAILS

	Boring Range of 4" to 24" casing 

	Engine - minimum 31 HP Diesel, Air-cooled @ 2800 rpm

	Transmission minimum 3 forward speeds and 1 reverse 

	Clutch - Operator presence clutch 

	Final drive - Dual planatery 2.5" Hex

	Auger torque - minimum 8512 ft/lbs peak 1st gear

	Forward thurst - 115,000 lb @ 3,000 psi

	Dog plate - Hydraulically activated from control console

	Hydraulic perameters - Gear pump max pressure 3000 psi x 14.5 gpm

	Fuel tank capacity - 5.0 gallons minimum

	Carriage 2900 lbs maximum

	Auger flight - 12" x 20 foot on 2.25

	Operator Station opposite side of spoil chute/ejector

	12" Adapter Kit

	Auger 12" OD 2-1/4" Hex W.C

	Head, Rock 12" OD 2-1/4" Hex W.C

	Head, Combo 12" OD 2-1/4" Hex W.C
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