{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":17,"n_cols":6,"rows_kept":17,"merged":[[15,4,15,5],[16,4,16,5]]}
["REVISED SCHEDULE OF UNIT PRICES 06/28/2018"]
["Additions and deletions from the Work shall be paid in accordance with the Unit Prices indicated below."]
["Item No.","Estimated Quantity","Unit","Description","Unit Price","Total Price"]
[1,1,"LS","Televise Well",null,{"$f":"B4*E4","v":{"v":0,"d":"0.00"}}]
[2,1,"LS","Clean and Airlift Debris",null,{"$f":"B5*E5","v":{"v":0,"d":"0.00"}}]
[3,500,"LF","Design and Install 12” Stainless Steel, Schedule 20 Liner",null,{"v":0,"d":"0.00"}]
[4,210,"LF","Design and Install 5” Stainless Steel Liner, Schedule 40",null,{"v":0,"d":"0.00"}]
[5,75,"LF","Design and Install 5” Stainless Steel wire wrap screen",null,{"v":0,"d":"0.00"}]
[6,1,"LS","Install Chlorinated, Washed, and Sized Gravel Pack from Total Depth to Surface",null,{"v":0,"d":"0.00"}]
[7,1,"LS","Install Test Pump and run 12 hour capacity test",null,{"v":0,"d":"0.00"}]
[8,1,"LS","Design and Purchase Line Shaft Turbine Pump (300 GPM @ 500 TDH, Intake Depth 400 feet)",null,{"v":0,"d":"0.00"}]
[9,1,"LS","Televise Well",null,{"v":0,"d":"0.00"}]
[10,1,"LS","Install Turbine Pump",null,{"v":0,"d":"0.00"}]
[11,1,"LS","Chlorinate Well and Sample",null,{"v":0,"d":"0.00"}]
[12,1,"LF","6” Carbon Steel Column Pipe",null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"Total Bid Price",{"$f":"SUM(F4:F15)","v":{"v":0,"d":"0.00"}}]
["DEDUCT",1,"LS","Deduct for Using Existing Discharge Head on New Pump Assembly",null,"$"]