{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Base Bid"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"Base Bid","index":0,"n_rows":29,"n_cols":6,"rows_kept":29,"merged":[[0,0,0,5],[1,0,1,5],[2,0,2,3],[3,0,3,3],[28,0,28,5]]}
["THIS IS A WORKSHEET ONLY - USE BID FORM SECTION 00300 TO PROVIDE SUBMISSION"]
["PLACID LAKE SIDEWALK IMPROVEMENTS"]
["HIGHLANDS COUNTY PROJECT NO. 20004"]
["BASE BID"]
["TASK NO.","ITEM DESCRIPTION","QUANTITY","UNIT","UNIT PRICE","EXTENDED PRICE"]
[1,"MOBILIZATION",1,"LS"]
[2,"INSURANCE",1,"LS"]
[3,"BONDS",1,"LS"]
[4,"CONSTRUCTION SURVEY STAKING INCLUDING AS-BUILT",1,"LS"]
[5,"TESTING ",1,"LS"]
[6,"MAINTENANCE OF TRAFFIC",1,"LS"]
[7,"REMOVAL OF EXISTING CONCRETE SIDEWALK",405,"SY"]
[8,"REMOVAL OF EXISTING ASPHALT PAVEMENT ROADWAY",3,"SY"]
[9,"MILLING EXISTING ASPH PAVT, 1 1/2\" AVG DEPTH",510,"SY"]
[10,"REGULAR EXCAVATION",6,"CY"]
[11,"REGULAR EMBANKMENT",6,"CY"]
[12,"STABILIZATION, TYPE B, LBR 40, 12\" COMPACTED THICKNESS SIDE STREET CONSTRUCTION",6,"SY"]
[13,"OPTIONAL BASE, BASE GROUP 6, 8” COMPACTED THICKNESS",6,"SY"]
[14,"SUPERPAVE ASPHALTIC CONCRETE, 1 1/2” THICK, RAP 30% MAXIMUM (PATCH)",{"v":0.6,"d":"1"},"TN"]
[15,"SUPERPAVE ASPHALTIC CONCRETE, 1 1/2” THICK, RAP 30% MAXIMUM (RESURFACE)",50,"TN"]
[16,"SIDEWALK CONCRETE, 4\" THICK, 2,500 PSI MIN",450,"SY"]
[17,"DETECTABLE WARNING, YELLOW, EMBEDDED",201,"SF"]
[18,"PERFORMANCE TURF (SOD) ",540,"SY"]
[19,"REMOVE AND REINSTALL EXISTING STOP SIGNS",7,"AS"]
[20,"TEMPORARY PAINTED PAVEMENT MARKINGS, STD, WHITE, SOLID, 12”",325,"LF"]
[21,"TEMPORARY PAINTED PAVEMENT MARKINGS, STD, WHITE, SOLID, 24”",125,"LF"]
[22,"THERMOPLASTIC, STANDARD, WHITE, SOLID, 12”",325,"LF"]
[23,"THERMOPLASTIC, STANDARD, WHITE, SOLID, 24”",125,"LF"]
["USE BID FORM SECTION 00300 TO PROVIDE SUBMISSION"]