{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":115,"n_cols":12,"rows_kept":115,"merged":[[1,3,1,7],[2,3,2,7]]}
[{"$nulls":3},"21-31  ERATE CLOSET UPGRADES SPECIFICATIONS:"]
[{"$nulls":3},"JCSS seeks responsible and responsive vendors who will reorganize data cabling in our network closets and provide and install replacement network switches. Reorganizing will consist of relocating and consolidating multiple patch panels, re-terminating drops into new patch panels, relabeling drops at patch panel and client side, and removing unnecessary cabling and panels.  Vendor will install new patch cables of appropriate lengths and will use the following system: Local LAN (Blue), Wireless (Green) and Camera (Red).  Contract for cabling and providing switches may be awarded separately.  Cabling vendor will be responsible for physical installation of new switches purchased through this RFP even if switches are purchased from another vendor."]
[{"$nulls":3},"Please quote the following preferred models of switches and modules OR EQUAL: 48 port PoE+ switch (Aruba 3810m), 24 port PoE+ switch (Aruba 3810m), 16 port SFP+ switch (Aruba 3810m), SFP+ expansion module (Aruba JL083A), SFP+ LRM transceiver (Aruba J9152D), SFP+ SM transceiver (HP Aruba J9151D), PoE+ power supply (Aruba JL086A#ABA), power supply for 16 port SFP+ switch (Aruba JL085A#ABA), and stacking modules (Aruba JL084A).  Proposals for equivalent models will be considered.  We may select separate vendors for switches and cabling."]
[]
[null,"CRMS",null,"Patch Panels",null,"Drops",null,"Patch Cables",null,"Switches",null,"Other"]
[]
[null,"A Hall",null,"Consolidate multiple patch panels to 2 patch panels (one above and one below switch).",null,"Reterminate into new patch panels and relabel drops at panel and client side.",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)"]
[]
[null,"B Hall",null,"Consolidate multiple patch panels to 2 patch panels (one above and one below switch).",null,"Reterminate into new patch panels and relabel drops at panel and client side.",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)"]
[]
[null,"C Hall",null,"Consolidate multiple patch panels to 2 patch panels (one above and one below switch).",null,"Reterminate into new patch panels and relabel drops at panel and client side.",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)"]
[]
[null,"D Hall",null,"Consolidate multiple patch panels to 2 patch panels (one above and one below switch).",null,"Reterminate into new patch panels and relabel drops at panel and client side.",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)"]
[]
[null,"E Hall",null,"Consolidate multiple patch panels to 3 patch panels (between, above, and below each switch.).",null,"Reterminate into new patch panels and relabel drops at panel and client side.",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)"]
[]
[null,"MDF",null,"Consolidate multiple patch panels to 4 patch panels (between, above, and below each switch.).",null,"Reterminate into new patch panels and relabel drops at panel and client side.",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)",null,"Switch Stack ((3) 48 port PoE+ switch, 2 SFP+ expansion modules, 6 SFP+ LRM transceivers, 3 PoE+ power supplies, 3 stacking modules, 3 stacking cables)"]
[]
[null,"DFES",null,"Patch Panels",null,"Drops",null,"Patch Cables",null,"Switches",null,"Other"]
[]
[null,"Blue Hall",null,"Consolidate multiple patch panels to 2 patch panels (one above and one below switch).",null,"Reterminate into new patch panels and relabel drops at panel and client side.",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)"]
[]
[null,"Green Hall",null,"Consolidate multiple patch panels to 4 patch panels (between, above, and below each switch.).",null,"Reterminate into new patch panels and relabel drops at panel and client side.",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)",null,"Switch Stack ((3) 48 port PoE+ switch, 1 SFP+ expansion modules, 1 SFP+ LRM transceivers, 3 PoE+ power supplies, 3 stacking modules, 3 stacking cables)"]
[]
[null,"MDF",null,"Consolidate multiple patch panels to 4 patch panels (between, above, and below each switch.).",null,"Reterminate into new patch panels and relabel drops at panel and client side.",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)",null,"Switch Stack ((2) 48 port PoE+ switch, (1) 24 port PoE+ switch, 2 SFP+ expansion modules, 5 SFP+ LRM transceivers, 3 PoE+ power supplies, 3 stacking modules, 3 stacking cables)"]
[]
[null,"Red Hall",null,"Consolidate multiple patch panels to 2 patch panels (one above and one below switch).",null,"Reterminate into new patch panels and relabel drops at panel and client side.",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)"]
[]
[null,"Yellow Hall",null,"Consolidate multiple patch panels to 2 patch panels (one above and one below switch).",null,"Reterminate into new patch panels and relabel drops at panel and client side.",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)"]
[]
[null,"GES",null,"Patch Panels",null,"Drops",null,"Patch Cables",null,"Switches",null,"Other"]
[]
[null,"Blue Hall",null,"Consolidate multiple patch panels to 2 patch panels (one above and one below switch).",null,"Reterminate into new patch panels and relabel drops at panel and client side.",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)",{"$nulls":3},"Remove point to point copper ethernet cabling from MDF to IDF."]
[]
[null,"Green Hall",null,"Consolidate multiple patch panels to 2 patch panels (one above and one below switch).",null,"Reterminate into new patch panels and relabel drops at panel and client side.",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)",{"$nulls":3},"Remove point to point copper ethernet cabling from MDF to IDF."]
[]
[null,"Gym",null,"Consolidate multiple patch panels to 2 patch panels (one above and one below switch).",null,"Reterminate into new patch panels and relabel drops at panel and client side.",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)",{"$nulls":3},"Remove point to point copper ethernet cabling from MDF to IDF."]
[]
[null,"MDF",{"$nulls":5},"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)",{"$nulls":3},"Remove point to point copper ethernet cabling from MDF to IDF."]
[]
[null,"Red Hall",null,"Consolidate multiple patch panels to 2 patch panels (one above and one below switch).",null,"Reterminate into new patch panels and relabel drops at panel and client side.",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)",{"$nulls":3},"Remove point to point copper ethernet cabling from MDF to IDF."]
[]
[null,"Yellow Hall",null,"Consolidate multiple patch panels to 2 patch panels (one above and one below switch).",null,"Reterminate into new patch panels and relabel drops at panel and client side.",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)",{"$nulls":3},"Remove point to point copper ethernet cabling from MDF to IDF."]
[]
[null,"GSMS",null,"Patch Panels",null,"Drops",null,"Patch Cables",null,"Switches",null,"Other"]
[]
[null,"B Hall",null,"Consolidate multiple patch panels to 2 patch panels (one above and one below switch).",null,"Reterminate into new patch panels and relabel drops at panel and client side.",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)",{"$nulls":3},"Remove old fiber and panel"]
[]
[null,"D Hall",null,"Consolidate multiple patch panels to 2 patch panels (one above and one below switch).",null,"Reterminate into new patch panels and relabel drops at panel and client side.",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)",{"$nulls":3},"Remove old fiber and panel"]
[]
[null,"E Hall",null,"Consolidate multiple patch panels to 5 patch panels (between, above, and below each switch).   Group active drops together, inactive drops together.",null,"Reterminate into new patch panels and relabel drops at panel and client side.",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)",null,"Switch Stack ((4) 48 port PoE+ switch, 1 SFP+ expansion modules, 1 SFP+ LRM transceivers, 4 PoE+ power supplies, 4 stacking modules, 4 stacking cables)",null,"Remove old fiber and panel"]
[]
[null,"MDF",null,"Consolidate multiple patch panels to 5 patch panels (between, above, and below each switch).   Group active drops together, inactive drops together.",null,"Reterminate into new patch panels and relabel drops at panel and client side.",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)",null,"Switch Stack ((4) 48 port PoE+ switch, 1 SFP+ expansion modules, 4 SFP+ LRM transceivers, 4 PoE+ power supplies, 4 stacking modules, 4 stacking cables)",null,"Remove old fiber and panel"]
[]
[null,"JCHS",null,"Patch Panels",null,"Drops",null,"Patch Cables",null,"Switches",null,"Other"]
[]
[null,"AA",{"$nulls":5},"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)"]
[]
[null,"Ag",null,"Consolidate multiple patch panels to 2 patch panels (one above and one below switch).",null,"Reterminate into new patch panels and relabel drops at panel and client side.",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)"]
[]
[null,"A Hall (Math)",null,"Consolidate multiple patch panels to 4 patch panels (between, above, and below each switch).   Group active drops together, inactive drops together.",null,"Reterminate into new patch panels and relabel drops at panel and client side.",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)",null,"Switch Stack ((3) 48 port PoE+ switch, 1 SFP+ expansion modules, 1 SFP+ LRM transceivers, 3 PoE+ power supplies, 3 stacking modules, 3 stacking cables)"]
[]
[null,"B Hall (Science)",null,"Consolidate multiple patch panels to 3 patch panels (between, above, and below each switch).   Group active drops together, inactive drops together.",null,"Reterminate into new patch panels and relabel drops at panel and client side.",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)"]
[]
[null,"CCA Lower",{"$nulls":5},"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)"]
[]
[null,"CCA Upper",{"$nulls":5},"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)"]
[]
[null,"English Wing",{"$nulls":5},"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)"]
[]
[null,"Field House",{"$nulls":5},"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)"]
[]
[null,"Old Field House",{"$nulls":5},"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)"]
[]
[null,"Fine Arts",null,"Consolidate multiple patch panels to 2 patch panels (one above and one below switch).",null,"Reterminate into new patch panels and relabel drops at panel and client side.",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)"]
[]
[null,"G Hall (English)",null,"Consolidate multiple patch panels to 2 patch panels (one above and one below switch).",null,"Reterminate into new patch panels and relabel drops at panel and client side.",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)"]
[]
[null,"Gym",{"$nulls":5},"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)"]
[]
[null,"H Hall (Social Studies)",null,"Consolidate multiple patch panels to 2 patch panels (one above and one below switch).",null,"Reterminate into new patch panels and relabel drops at panel and client side.",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)"]
[]
[null,"MDF",null,"Consolidate multiple patch panels to 3 patch panels (one above and one below switch).   Group active drops together, inactive drops together.",null,"Reterminate into new patch panels and relabel drops at panel and client side.",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)",null,"Switch Stack ((2) 48 port PoE+ switch, (1) 16 port SFP+ switch, 12 SFP+ LRM transceivers, 2 SFP+ SM transceivers, 2 PoE+ power supplies, 1 standard power supply,  3 stacking modules, 3 stacking cables)"]
[]
[null,"ROTC",null,"Consolidate multiple patch panels to 2 patch panels (one above and one below switch).",null,"Reterminate into new patch panels and relabel drops at panel and client side.",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)"]
[]
[null,"TWES",null,"Patch Panels",null,"Drops",null,"Patch Cables",null,"Switches",null,"Other"]
[]
[null,"Blue Hall",null,"Consolidate multiple patch panels to 2 patch panels (one above and one below switch).",null,"Reterminate into new patch panels and relabel drops at panel and client side.",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)"]
[]
[null,"Green Hall",null,"Consolidate multiple patch panels to 2 patch panels (one above and one below switch).",null,"Reterminate into new patch panels and relabel drops at panel and client side.",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)"]
[]
[null,"Gym",null,"Consolidate multiple patch panels to 2 patch panels (one above and one below switch).",null,"Reterminate into new patch panels and relabel drops at panel and client side.",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)"]
[]
[null,"MDF",null,"Consolidate multiple patch panels to 5 patch panels (between, above, and below each switch).   Group active drops together, inactive drops together.",null,"Reterminate into new patch panels and relabel drops at panel and client side.",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)",null,"Switch Stack ((4) 48 port PoE+ switch, 2 SFP+ expansion modules, 6 SFP+ LRM transceivers, 4 PoE+ power supplies, 4 stacking modules, 4 stacking cables)",null,"Remove old fiber and panel"]
[]
[null,"Red Hall",null,"Consolidate multiple patch panels to 2 patch panels (one above and one below switch).",null,"Reterminate into new patch panels and relabel drops at panel and client side.",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)"]
[]
[null,"Yellow Hall",null,"Consolidate multiple patch panels to 2 patch panels (one above and one below switch).",null,"Reterminate into new patch panels and relabel drops at panel and client side.",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)"]
[]
[null,"WES",null,"Patch Panels",null,"Drops",null,"Patch Cables",null,"Switches",null,"Other"]
[]
[null,"600 Hall",null,"Consolidate multiple patch panels to 2 patch panels (one above and one below switch).",null,"Reterminate into new patch panels and relabel drops at panel and client side.",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)",{"$nulls":3},"Remove old fiber"]
[]
[null,"700 Hall",null,"Consolidate multiple patch panels to 2 patch panels (one above and one below switch).",null,"Reterminate into new patch panels and relabel drops at panel and client side.",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)",{"$nulls":3},"Remove old fiber"]
[]
[null,"Blue Hall",null,"Consolidate multiple patch panels to 2 patch panels (one above and one below switch).",null,"Reterminate into new patch panels and relabel drops at panel and client side.",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)"]
[]
[null,"Gym",null,"Consolidate multiple patch panels to 2 patch panels (one above and one below switch).",null,"Reterminate into new patch panels and relabel drops at panel and client side.",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)"]
[]
[null,"MDF",null,"Consolidate multiple patch panels to 3 patch panels (between, above, and below each switch).",null,"Reterminate into new patch panels and relabel drops at panel and client side.",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)",null,"Switch Stack ((2) 48 port PoE+ switch, 2 SFP+ expansion modules, 7 SFP+ LRM transceivers, 2 PoE+ power supplies, 2 stacking modules, 1 stacking cables)",null,"Remove old fiber and panel"]
[]
[null,"Red Hall",null,"Consolidate multiple patch panels to 2 patch panels (one above and one below switch).",null,"Reterminate into new patch panels and relabel drops at panel and client side.",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)"]
[]
[null,"Yellow Hall",null,"Consolidate multiple patch panels to 2 patch panels (one above and one below switch).",null,"Reterminate into new patch panels and relabel drops at panel and client side.",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)"]