{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":10,"n_cols":2,"rows_kept":10}
["PEC48482","48X48 Dual Corner Lift"]
[null,"Steel: Black - Laminate: Folkstone Grey (Grey Trim)"]
[null,"Includes laminate top primary worksurface(no cable ports),  laminate K/B platform, 2 - sets of Linak lifting legs(one set for primary surface and one set for K/B surface)"]
[null,"Includes Core skins behind lift"]
[null,"Load Capacity: 300 lbs per surface, 600lbs total (evenly distributed).   "]
[null,"Travel Range: 23.7\" - 50.3\" (both surfaces)   "]
[null,"Travel Speed: 1.69\" per second.  "]
[null,"Noise Factor: 51 - 53 dB.   "]
[null,"Lift constructed of high-strength steel, three part telescoping columns  "]
[null,"Has three user defined preset height positions. "]