{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["UNIT PRICE TAB"],"not_rendered":{"images":1,"external_links":2,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"UNIT PRICE TAB","index":0,"n_rows":108,"n_cols":9,"rows_kept":108,"merged":[[0,0,0,8],[1,0,1,8],[2,0,2,8],[4,3,4,8],[7,3,7,8],[13,3,13,8],[17,3,17,8],[27,3,27,8],[74,3,74,8],[76,3,76,8],[78,3,78,8],[93,3,93,8],[107,3,107,7]],"flags":["formulas_cached_only"]}
["ARLINGTON COUNTY, VIRGINIA\nOFFICE OF THE PURCHASING AGENT\nINVITATION TO BID NO. XXX-XX\nPROJECT NO.:  XX-XXX-XX"]
["SUBMIT AN ORIGINAL SIGNED BID FORM AND ONE COPY"]
["THE UNDERSIGNED CERTIFIES THAT (CONTRACTOR NAME)___________________________\nIS CURRENTLY REGISTERED WITH THE VIRGINIA STATE BOARD OF CONTRACTORS AS REQUIRED BY THE CODE OF VIRGINIA.  CERTIFICATE NUMBER _________________ WAS ISSUED ON THE ________DAY OF _____________, 20XX.  THE UNDERSIGNED FURTHER CERTIFIES THAT THE REGISTRATION FEE AND ALL RENEWAL FEES REQUIRED UNDER LAW HAVE BEEN PAID.  THE CONTRACTOR AGREES TO FURNISH ALL NECESSARY LABOR, EQUIPMENT, MATERIALS, AND ALL THINGS NECESSARY TO PERFORM THE WORK AS SET FORTH IN ACCORDANCE WITH THE PLANS AND SPECIFICATIONS. THE CONTRACTOR AGREES TO PERFORM RELATED WORK FOR THE FOLLOWING ITEMS AT THE FOLLOWING STIPULATED PRICES: (ALL PRICES INCLUDE PROVISION AND INSTALLATION).\n"]
[{"$nulls":3},"Bid Item Number","Description","Qty","Unit","Unit Price","Total Price"]
[{"$nulls":3},"EXCAVATION & SITE WORK"]
["02200","C1","1",1,"General Excavation, only when not included in other pay items",610,"CY",null,0]
["02200","C1","14",2,"Aggregate, VDOT #21-B  (Compacted in Place per VDOT standards & Specs)",225,"CY",null,0]
[{"$nulls":3},"CONCRETE WORK"]
["02750","C2","4",3,"Concrete Curb, Standard 6\" (VDOT CG-2), includes curb for aprons, ramps, etc. ",20,"LF",null,0]
[{"$nulls":3},4,"Concrete Curb, Standard 6\" (VDOT MC-1), includes curb for aprons, ramps, etc. ",12,"LF",null,0]
["02750","C2","7",5,"Concrete Curb & Gutter, Combination 6\" (VDOT CG-6), includes curb & gutter for aprons, ramps, etc.",725,"LF",null,0]
["02611","C2","11",6,"Concrete Sidewalk, 4\" Thickness (Arlington County Detail R-2.0)",285,"SY",null,0]
["02611","C2","19",7,"CG-12 Detectable Warning Surface - Truncated Domes",8,"SY",null,0]
[{"$nulls":3},"ASPHALT PAVEMENT WORK"]
["02600","C3","1",8,"Asphalt Concrete, Planing or Milling (1/2\" to 3\" Depth)",4830,"SY",null,0]
["02600","C3","3",9,"Asphalt Concrete, Base Course (VDOT BM-25.0A)",445,"TON",null,0]
["02600","C3","7",10,"Asphalt Concrete, Surface Course (VDOT SM-9.5D)",635,"TON",null,0]
[{"$nulls":3},"STORM SEWER WORK"]
["02550","C4","3",11,"Storm Manhole MH-2 (VDOT MH-2), In Place, DEPTH 8'",1,"EA",null,0]
["02550","C4","25",12,"Curb Drop Inlet, Standard VDOT DI-3B (12\" to 30\" Pipe), In Place Up to 8' Deep, Inlet Throat Length 4' to 20'",1,"EA",null,0]
["02550","C4","50",13,"Adjust Storm Manhole to New Grade (Arlington County Detail S-2.5), Type A",1,"EA",null,0]
["02550","C4","53",14,"Convert Catch Basin to Manhole",1,"EA",null,0]
["02550","C4","61",15,"Storm Manhole, Catch Basin, Drop Inlet, Yard Inlet, or Grate Inlet, Remove",1,"EA",null,0]
["02550","C4","63",16,"15\" Pipe, RCP Class III, In Place Up to 6' Deep",5,"LF",null,0]
["02550","C4","79",17,"42\" Pipe, RCP Class III, In Place Up to 6' Deep",28,"LF",null,0]
["02550","C4","145",18,"Underdrain, Standard VDOT UD-4",350,"LF",null,0]
[{"$nulls":3},19,"Remove storm pipe (42\" RCP)",28,"LF",null,0]
[{"$nulls":3},"WATERMAIN & UTILITY WORK"]
["02550","C6","58",20,"Water Valve Box vertical Adjustment to New Grade",8,"EA",null,0]
["02550","C6","59",21,"Gas Valve Box vertical Adjustment to New Grade",4,"EA",null,0]
[{"$nulls":3},22,"Electric Manhole vertical Adjustment to New Grade",2,"EA",null,0]
["02550","C6","60","02550-C6-00590","Non-Freeze Boxed Ground Hydrant (with Locking Cover and Keys), Jay R. Smith or County approved equivalent (Excavation, Install Copper Tubing, Connect to County Water Meter, Install Ground Hydrant w/Compacted Pea Gravel, Backfill, and Surface Grade Restora",null,"EA",null,0]
["02550","C6","61","02550-C6-00600","PVC Pipe (4\"or 6\"), SDR 35 (less than 14' of cover), only when not included in other pay items",null,"LF",null,0]
["02550","C6","62","02550-C6-00610","PVC Pipe (4\" or 6\"), SDR 26 or stronger (14' to 20' of cover), only when not included in other pay items",null,"LF",null,0]
["02550","C6","63","02550-C6-00620","Abandon Existing Corporation Stop (TO BE PERFORMED AS DIRECTED BY THE COUNTY PROJECT OFFICER)",null,"EA",null,0]
["02550","C6","64","02550-C6-00630","Service Taps (TAP MAIN, INSTALL COPPER TUBING, INSTALL ANGLE VALVES, CORPORATION COCK, METER BOX AND METER YOKE/METER, CONNECT TO EXISTING PRIVATE SERVICE LINE, BACKFILL AND EXCAVATION)--UP TO 1O FT.",null,"EA",null,0]
["02550","C6","65","02550-C6-00640","Service Taps PER ADDITIONAL LINEAR FOOT OVER 10 FT.",null,"LF",null,0]
["02550","C6","66","02550-C6-00650","Service Re-Taps (TAP MAIN, INSTALL COPPER TUBING, CONNECT TO EXISTING SERVICE LINE, ABANDON CORPORATION COCK FROM EXISTING SERVICE LINE, BACKFILL AND EXCAVATION)-UP TO 10 FT.",null,"EA",null,0]
["02550","C6","67","02550-C6-00660","Service Re-Taps PER ADDITIONAL LINEAR FT. OVER 10 FT.",null,"LF",null,0]
["02550","C6","68","02550-C6-00670","Water Meter Relocations (INSTALL COPPER TUBING, CONNECT TO EXISTING COUNTY AND PRIVATE SERVICE LINES, PROVIDE NEW ANGLE VALVES, RELOCATE METER HOUSING AND METER YOKE, BACKFILL AND EXCAVATION)--UP TO 10 FT.",null,"EA",null,0]
["02550","C6","69","02550-C6-00680","Service Relocations PER ADDITIONAL LINEAR FOOT OVER 10 FT.",null,"LF",null,0]
["02550","C6","70","02550-C6-00690","Service Taps (TAP MAIN, INSTALL COPPER TUBING, INSTALL GATE VALVES, CORPORATION COCK, METER BOX AND METER, CONNECT TO EXISTING PRIVATE SERVICE LINE, BACKFILL AND EXCAVATION)--UP TO 1O FT.",null,"EA",null,0]
["02550","C6","71","02550-C6-00700","Service Taps PER ADDITIONAL LINEAR FOOT OVER 10 FT.",null,"LF",null,0]
["02550","C6","72","02550-C6-00710","Service Re-Taps (TAP MAIN, INSTALL COPPER TUBING, CONNECT TO EXISTING SERVICE LINE, ABANDON CORPORATION COCK FROM EXISTING SERVICE LINE, BACKFILL AND EXCAVATION)--UP TO 10 FT.",null,"EA",null,0]
["02550","C6","73","02550-C6-00720","Service Re-Taps PER ADDITIONAL LINEAR FOOT OVER 10 FT.",null,"LF",null,0]
["02550","C6","74","02550-C6-00730","Water Meter Relocations (INSTALL COPPER TUBING, CONNECT TO EXISTING COUNTY AND PRIVATE SERVICE LINES, PROVIDE NEW GATE VALVES, RELOCATE METER HOUSING AND METER, BACKFILL AND EXCAVATION)--UP TO 10 FT.",null,"EA",null,0]
["02510","C7","1","02550-C6-00740","Service Relocations PER ADDITIONAL LINEAR FOOT OVER 10 FT.",null,"LF",null,0]
["02510","C7","2","02510-C7-00010","Sanitary Sewer - 8\" PVC, SDR 35, DEPTH< 8’",null,"LF",null,0]
["02510","C7","3","02510-C7-00020","Sanitary Sewer - 8\" PVC, SDR 35, 8’ ≤ DEPTH < 14’",null,"LF",null,0]
["02510","C7","4","02510-C7-00030","Sanitary Sewer - 8\" PVC, SDR 26, DEPTH ≥ 14'",null,"LF",null,0]
["02510","C7","5","02510-C7-00040","Sanitary Sewer- 8\"DIP CLASS 52, DEPTH < 8'",null,"LF",null,0]
["02510","C7","6","02510-C7-00050","Sanitary Sewer- 8\"DIP CLASS 52, 8'≤ DEPTH <15'",null,"LF",null,0]
["02510","C7","7","02510-C7-00060","Sanitary Sewer- 8\"DIP CLASS 52, DEPTH >15'",null,"LF",null,0]
["02510","C7","8","02510-C7-00070","Sanitary Sewer - 10\" PVC, SDR 35, DEPTH< 8’",null,"LF",null,0]
["02510","C7","9","02510-C7-00080","Sanitary Sewer - 10\" PVC, SDR 35,  8’ ≤ DEPTH < 14'",null,"LF",null,0]
["02510","C7","10","02510-C7-00090","Sanitary Sewer - 10\" PVC, SDR 26, DEPTH ≥ 14'",null,"LF",null,0]
["02510","C7","11","02510-C7-00100","Sanitary Sewer- 10\"DIP CLASS 52, DEPTH < 8'",null,"LF",null,0]
["02510","C7","12","02510-C7-00110","Sanitary Sewer- 10\"DIP CLASS 52, 8'≤ DEPTH <15'",null,"LF",null,0]
["02510","C7","13","02510-C7-00120","Sanitary Sewer- 10\"DIP CLASS 52, DEPTH >15'",null,"LF",null,0]
["02510","C7","14","02510-C7-00130","Sanitary Sewer - 12\" PVC, SDR 35, DEPTH< 8’",null,"LF",null,0]
["02510","C7","15","02510-C7-00140","Sanitary Sewer - 12\" PVC, SDR 35, 8’ ≤ DEPTH < 14'",null,"LF",null,0]
["02510","C7","16","02510-C7-00150","Sanitary Sewer - 12\" PVC, SDR 26,  DEPTH ≥ 14'",null,"LF",null,0]
["02510","C7","17","02510-C7-00160","Sanitary Sewer- 12\"DIP CLASS 52, DEPTH < 8'",null,"LF",null,0]
["02510","C7","18","02510-C7-00170","Sanitary Sewer- 12\"DIP CLASS 52, 8'≤ DEPTH <15'",null,"LF",null,0]
["02510","C7","19","02510-C7-00180","Sanitary Sewer- 12\"DIP CLASS 52, DEPTH >15'",null,"LF",null,0]
["02510","C7","20","02510-C7-00190","Boring And Jacking 18\" TO 24\" Casing Pipe With 8\" TO 12\" Carrier Pipe PER Arlington County SPECIFICATION SECTION 02951 AND DETAIL M-4.0",null,"LF",null,0]
["02510","C7","21","02510-C7-00200","Manhole - Precast Concrete, 4' ID, DEPTH <  8'",null,"VF",null,0]
["02510","C7","22","02510-C7-00210","Manhole-Precast Concrete 4' I.D. DEPTH > 8', PER ADDITIONAL VF OVER 8' ",null,"VF",null,0]
["02510","C7","23","02510-C7-00220","Manhole-Precast Concrete 5' I.D. DEPTH < 8' ",null,"VF",null,0]
["02510","C7","24","02510-C7-00230","Manhole-Precast Concrete 5' I.D. DEPTH > 8', PER ADDITIONAL VF OVER 8' ",null,"VF",null,0]
["02510","C7","25","02510-C7-00240","Manhole-Construct Over Existing Sewer, Arlington County DRAWING S-2.2 (PAYMENT SHALL BE FOR DOGHOUSE BASE AND REMAINDER OF MANHOLE SHALL BE PAID UNDER VF PRICES FOR MANHOLES PER ITEM 20 TO 23 ABOVE)",null,"EA",null,0]
["02510","C7","26","02510-C7-00250","Abandon Existing Manhole",null,"EA",null,0]
["02510","C7","27","02510-C7-00260","Connect To Existing Sanitary Manhole",null,"EA",null,0]
["02510","C7","28","02510-C7-00270","Sanitary Sewer House Laterals(IN ACCORDANCE WITH Arlington County CONSTRUCTION STANDARDS AND SPECIFICATIONS SECTION 02510, PART 3, ITEM 3.5) ",null,"LF",null,0]
[{"$nulls":3},"SANITARY SEWER WORK"]
["02510","C7","29",23,"Adjust Sanitary Manhole to New Grade (Arlington County Detail S-2.5), Type A",7,"EA",null,0]
[{"$nulls":3},"TRAFFIC SIGNAL WORK"]
[{"$nulls":3},24,"Traffic Signal Upgrade (As outlined in the construction planset)",1,"LS",null,0]
[{"$nulls":3},"SIGNING AND PAVEMENT MARKING WORK"]
["02900","C10","5",25,"Twenty Four (24) Inch Transverse Markings, Note: Used For Continental (Ladder) Crosswalk",600,"LF",null,0]
["02900","C10","5",26,"Twenty Four (24) Inch Markings, Yellow, 12 Foot Spacing @ 45 Degree Angle, Note: Used For Left Turn Lane Taper",30,"LF",null,0]
["02900","C10","7",27,"Four (4) Inch Longitudinal Solid Line (White)",680,"LF",null,0]
["02900","C10","7",28,"Four (4) Inch Longitudinal Solid Line (Yellow)",330,"LF",null,0]
["02900","C10","8",29,"Four (4) Inch Longitudinal Skip Line (Ten (10) Foot Line/Thirty (30) Foot Spacing)",340,"LF",null,0]
["02900","C10","10",30,"Four (4) Inch Longitudinal Skip Line (Two (2) Foot Line/Four (4) Foot Spacing) **Turn Lane Skips**",90,"LF",null,0]
["02900","C10","7",31,"Six (6) Inch Longitudinal Solid Line (White)",235,"LF",null,0]
["02900","C10","17",32,"Twelve (12) Inch Yellow Longitudinal Centerline, Two - Four (4) Inch Yellow Lines with Four (4) Inch Separation",900,"LF",null,0]
["02900","C10","24",33,"Single Arrows",3,"EA",null,0]
["02900","C10","26",34,"Lane Reduction Arrows",2,"EA",null,0]
[{"$nulls":3},35,"Removal of Existing Longitudinal Lines (Four (4) Inch Width)",140,"EA",null,0]
["02900","C10","41",36,"Traffic Control Sign (Typical Stop, Yield, No Parking, Speed Limit, or Similar), Install per Detail SG-1.0",2,"EA",null,0]
["02900","C10","41",37,"Traffic Control Sign (Typical Stop, Yield, No Parking, Speed Limit, or Similar), Remove and Dispose",2,"EA",null,0]
["02900","C10","43",38,"Traffic Control Sign (Typical Stop, Yield, No Parking, Speed Limit, or Similar), Relocate with New Post",7,"EA",null,0]
[{"$nulls":3},"LANDSCAPING & EROSION & SEDIMENT CONTROL WORK"]
[{"$nulls":3},39,"Landscape/Retaining Wall (Block, Brick, Segmental, or Similar), Height Greater Than 3' Exposed Face, Remove and Dispose (including Foundation Removal)",100,"SF",null,0]
["02801","C11","6",40,"Sod, Tall Fescue/Bluegrass Mixture, 2\" topsoil + lime and fertilizer (Arlington County spec #329200)",440,"SY",null,0]
[{"$nulls":3},41,"Tree and Shrub - Remove and Dispose, 18\" to 24\" DBH (Diameter at Breast Height)",1,"EA",null,0]
["02800","C11","9",42,"Tree and Shrub - Remove and Dispose, 24\" to 36\" DBH (Diameter at Breast Height)",1,"EA",null,0]
[{"$nulls":3},43,"Tree and Shrub - Deciduous Tree, 2\" to 3\" Caliper",3,"EA",null,0]
[{"$nulls":3},44,"Soil Restoration For Removed Asphalt Trail Area",215,"SY",null,0]
["01500","C13","1",45,"Silt Fence, with Wire Support (Virginia Erosion & Sediment Control Handbook Standard & Specification 3.05)",365,"LF",null,0]
["01500","C13","5",46,"Storm Drain Inlet Protection, Block & Gravel Drop Inlet Application (per Virginia Erosion & Sediment Control Handbook Standard & Specification 3.07)",1,"EA",null,0]
["01500","C13","7",47,"Storm Drain Inlet Protection, Block & Gravel Curb Inlet Application (per Virginia Erosion & Sediment Control Handbook Standard & Specification 3.07)",14,"EA",null,0]
["01500","C13","12",48,"Dewatering Structure (per Virginia Erosion & Sediment Control Handbook Standard & Specification 3.26) (for use with installation of 1 proposed pipe run + unexpected ground water ($1000))",2,"EA",null,0]
["01500","C13","13",49,"6' Chain Link Tree Protection Fence (per Arlington County DPR Standard 02231.1)",630,"LF",null,0]
["01000","M2","1",50,"Maintenance of Traffic (MOT)",1,"LS",null,0]
[{"$nulls":3},51,"Mobilization",1,"LS",null,0]
[{"$nulls":3},"CONTRACT TOTAL",{"$nulls":4},0]