{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Pricing Sheet"],"read":"whole","date_system":"1900"}

{"sheet":"Pricing Sheet","index":0,"n_rows":26,"n_cols":7,"rows_kept":26,"merged":[[0,0,0,6],[2,0,2,6],[3,0,3,6],[5,0,5,6],[7,0,7,6],[11,0,11,6],[18,0,18,6],[22,0,22,5]]}
["ATTACHMENT A - PRICING SHEET"]
[]
["FURNISHING ALL LABOR, MATERIALS, AND EQUIPMENT FOR THE"]
["ETHAN ALLEN GENERATOR REPLACEMENT"]
[]
["PLEASE PROVIDE PRICES IN ALL CELLS HIGHLIGHTED IN BLUE. BIDDERS SHALL PROVIDE THEIR BID PRICES IN THE CELLS HIGHLIGHTED IN BLUE BELOW.  BIDDERS SHALL INCLUDE A BID PRICE FOR ALL ITEMS. FAILURE TO PROVIDE A PRICE FOR ALL ITEMS, OR ANY MODIFICATIONS OR ADDITIONS TO THE BID FORM MAY RESULT IN BID REJECTION."]
[]
["PROJECT COST BREAKDOWNS"]
["ITEM","DESCRIPTION","MANUFACTURER","QTY","UNIT","UNIT PRICE","TOTAL"]
[1,"MOBILIZATION/DE-MOBILIZATION (NOT TO EXCEED 5% OF THE TOTAL BID AMOUNT) - LABOR, MATERIALS, EQUIPMENT, ETC.",null,1,"LS"]
[2,"DEMOLITION - LABOR, MATERIALS, EQUIPMENT, TEMPORARY CONSTRUCTION, ETC.",null,1,"LS"]
["Major Work"]
["ITEM","DESCRIPTION",null,"QTY","UNIT","UNIT PRICE","TOTAL"]
[3,"GENERATOR PAD - LABOR & MATERIALS",null,1,"LS"]
[4,"450kW 480/277V GENERATOR WITH 250 GAL DOUBLE WALL DIESEL BELLY FUEL TANK - LABOR & MATERIALS",null,1,"LS"]
[5,"400A 480V, 3-PHASE 4W PIN AND SLEEVE TYPE TEMPOARY GENERATOR PLUG WITH DISCONNECT SWITCH - LABOR & MATERIALS",null,1,"LS"]
[6,"REMOVING OLD FEEDERS AND INSTALLING NEW FEEDER AND OTHER BRANCH CIRCUIT WIRING - LABOR & MATERIALS",null,1,"LS"]
[7,"DEMOLISHING OLD FAN AND INSTALLING NEW WITH NEW CIRCUITING - LABOR & MATERIALS",null,1,"LS"]
["Miscellaneous"]
["ITEM","DESCRIPTION",null,"QTY","UNIT","UNIT PRICE","TOTAL"]
[8,"WIRING, CONDUIT, FITTINGS, MISC. ELECTRICAL - LABOR & MATERIALS",null,1,"LS"]
[9,"OVERHEAD, PROFIT, TAXES, ETC.",null,1,"LS"]
["LUMP SUM TOTAL BID PRICE",{"$nulls":5},{"$f":"SUM(G10:G22)","v":{"v":0,"d":"$0.00"}}]
[]
[]
["Bidder Name: ________________________________________"]