{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":24,"n_cols":6,"rows_kept":24,"merged":[[0,0,0,5]]}
["PD 18-19.002 Southwest Greenway 1st Extension - Base Bid"]
["Item No.","Description","Quantity","Unit","Unit Price","Amount"]
[1,"Mobilization",1,"LS",null,{"$f":"+C3*E3","v":0}]
[2,"Bonds and Insurance",1,"LS",null,{"$f":"+C4*E4","v":0}]
[3,"Prepare & Implement Maintenance of Traffic Plan",1,"LS",null,0]
[4,"General Building Permit",1,"LS",null,0]
[5,"Deck demolition and removal",1,"LS",null,0]
[6,"Joist and stringer inspection, demolition and removal",1,"LS",null,0]
[7,"Install ADA accessible ramps from gravel path to observation deck and walking trail",2,"LS",null,0]
[8,"Coordination of “switchback” connection with South Old Corry Field Road project",1,"LS",null,0]
[9,"2x12 stringers #2 prime or equivalent",150,"EA",null,0]
[10,"2x10x10 ft. joists #2 prime or equivalent",800,"EA",null,0]
[11,"2x6x8 ft. #2 prime or equivalent",1770,"EA",null,0]
[12,"2x6x10 ft. #2 prime or equivalent",49,"EA",null,0]
[13,"2x4x10 ft. #2 prime or equivalent",784,"EA",null,0]
[14,"2x6x20 ft. composite top rail",49,"EA",null,0]
[15,"2000lf 4 ft. high 14GA galvanized welded wire fence (2x4 mesh)",2000,"LF",null,0]
[16,"Boardwalk installation includes but not limited to; stringers, joists, railing, boardwalk deck",1,"LS",null,0]
[]
[]
[]
[]
[]
[{"$nulls":4},"Total ",{"$f":"SUM(F3:F23)","v":0}]