{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"defined_names":2},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"merged":[[2,0,2,5],[17,0,17,5],[24,4,24,5]]}
["Bidder Name:"]
["TASK NO.","DESCRIPTION","QUANTITY","UNIT","UNIT    PRICE","Extended Price (Qty*Unit)"]
["BAFFEL/FILTER BOX"]
[1,"MOBILIZATION & DEMOBILIZATION",1,"LS"]
[2,"MAINTENACE OF TRAFFIC",1,"LS"]
[3,"EROSION CONTROL, SILT FENCE",164,"LF"]
[4,"EROSION CONTROL, FLOATING TURBIDITY BARRIER",120,"LF"]
[5,"GENERAL REQUIREMENTS (INCLUDING PROJECT INFORMATIONAL SIGN)",1,"LS"]
[6,"CLEARING AND DEMOLITION (PARTIOAL REMOVAL OF FABRIFORM FOR PIPE INSTALLATION)",1,"LS"]
[7,"EARTHWORK",1,"LS"]
[8,"OLDCASTLE NRFS 6’X12’ FILTER BOX WITH BOLD & GOLD ECT3 FILTER MEDIA (OR APPROVED EQUAL)",1,"EA"]
[9,"PIPE CULVERT (PVC), 8” ROUND",32,"LF"]
[10,"EXISTING INLET MODIFICATION (TO TIE-IN PROPOSED 8” PVC PIPE)",1,"LS"]
[11,"CONCRETE PIPE BLOCK, 0.5’ X 2’",1,"LS"]
[12,"CONCRETE SLOPE PAVEMENT, 6” THICK (REPLACING SLOPE PROTECTION WHERE CONCRETE FABRIFORM WAS REMOVED)",1,"LS"]
[13,"RIPRAP RUBBLE, DITCH LINING (SUMP AT 8” PVC PIPE INFLOW)","10 ","TN"]
[14,"RESTORATION SODDING (APPLIED TO ALL DISTURBED AREAS)",800,"SY"]
["FLOATING ISLANDS"]
[1,"MOBILIZATION & DEMOBILIZATION",1,"LF"]
[2,"GENERAL REQUIREMENTS (INCLUDING PROJECT INFORMATIONAL SIGN)",1,"LS"]
[3,"BIOHAVEN 6.5’ X 6’ FLOATING TREATMENT WETLAND MATS WITH BOTTOM-MOUNTED ANCHOR POINTS (OR APPROVED EQUAL)",5,"EA"]
[4,"CONCRETE ANCHOR (FORMED FROM 12” HIGH, 12” DIAMETER CYLINDRICAL FORM) AND SYNTHETIC BRAIDED TETHERING ROPES",5,"EA"]
[5,"PLANTINGS: PICKERELWEED (MINIMUM 2” CONTRAINER AND 12” HIGH)",100,"EA"]
[6,"PLANTINGS: SOFTRUSH (MINIMUM 2” CONTAINER AND 12” HIGH)",85,"EA"]
[null,"TOTAL LUMP SUM BID AMOUNT [numeric]    ",null,null,"$"]
["TOTAL LUMP SUM BID AMOUNT [in words]"]
[]
["LS = Lump Sum, SY = Square Yard, TN = Ton, LF = Linear Foot, and EA = Each"]
[]
["The total of the items listed above must total the lump sum amount below.  "]