{"text_format":"3","workbook":"xls","n_sheets":8,"sheets":["All Rooms","CRMS","DFES","GES","GSMS","JCHS","TWES","WES"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"All Rooms","index":0,"n_rows":43,"n_cols":10,"rows_kept":43,"flags":["formulas_cached_only"]}
["School","Room","Teacher","Ceiling Height","HDMI/VGA/Ethernet Cable Length","3.5mm Audio Cable Length","Top of panel to be at","Dry Erase Board Needs","Power for Panel","Additional Notes"]
[]
["CRMS","A7",null,"10ft","60ft+","30ft+","80\"","Remove existing, replace with 2 smaller boards","Needed above","Relocate A/V hookups by network drops at teacher desk location "]
["CRMS","A8",null,"10ft","60ft+","30ft+","80\"","Remove existing, replace with 2 smaller boards","Needed above"]
["CRMS","B6",null,"10ft","30ft+","40ft+","80\"","Relocate bulletin board","Needed above","Install IFP on hall wall centered between door and teacher desk"]
["CRMS","C2",null,"10ft","60ft+","35ft+","80\"","Remove existing, replace with 2 smaller boards","Needed above"]
["CRMS","C3",null,"10ft","60ft+","35ft+","80\"","Remove existing, replace with 2 smaller boards","Needed above","Install IFP on wall opposite of current SB location, move A/V hookups closer to corner"]
[]
["DFES","Yellow 9","Gifted","10ft","40ft+","35ft+","Adjustable Stand","None","Needed above","install at far left end of dry erase board"]
["DFES","Orange 3","PEC","10ft","35ft+","35ft+","Adjustable Stand","None","Present above","center on wall"]
["DFES","Orange 4","PEC","10ft","30ft+","30ft+","Adjustable Stand","None","Present above","same location as SB"]
["DFES","Purple 6","Art","10ft","65ft+","35ft+","Adjustable Stand","Remove existing, replace with 2 6ft boards","Present below","Needs dry erase board space"]
[]
["GES","Yellow 604",null,"10ft","35ft+","35ft+","72\"","None","Present above"]
["GES","Yellow 605",null,"10ft","35ft+","35ft+","72\"","None","Present above"]
["GES","Yellow 606",null,"10ft","35ft+","35ft+","72\"","None","Present above"]
["GES","Yellow 607",null,"10ft","35ft+","35ft+","72\"","None","Present above"]
[]
["GSMS","A3",null,"10ft","35ft+","35ft+","80\"","None","Needed above","Move AV closer to teacher desk location "]
["GSMS","A4",null,"10ft","35ft+","35ft+","80\"","None","Needed above","Move AV hookups closer to exterior wall corner"]
["GSMS","B10",null,"10ft","30ft+","35ft+","80\"","None","Present below","Install IFP on opposite wall from current SB location. Move AV hookup closer to outer wall corner by network drops."]
["GSMS","B4",null,"10ft","35ft+","35ft+","80\"","None","Needed above","Move AV hookups to front wall closer to outer wall corner"]
["GSMS","C1",null,"10ft","30ft+","35ft+","80\"","None","Present below","Install IFP on opposite wall from current SB location."]
["GSMS","D1",null,"10ft","60ft+","35ft+","80\"","None","Present below"]
["GSMS","E5","Ag","10ft","30ft+","35ft+","80\"","Remove existing, replace with 2 smaller boards","Needed above","Relocate AV hookup to wall with network drop"]
["GSMS","E6","Art","10ft","45ft+","35ft+","80\"","Remove existing, replace with 2 smaller boards","Needed above"]
[]
["JCHS","AG2","Lankford","9ft","60ft+","35ft+","80\"","Add one small dry erase board to right of IFP","Needed above","Wall is sheet metal."]
["JCHS","AG4","Martin","9ft","35ft+","35ft+","80\"","Remove existing bulletin board, replace with 2 smaller dry erase boards","Present below","Install IFP on opposite wall of current SB location.  Move AV hookups and network drop to wall where IFP will be, near corner. Wall is sheetrock."]
["JCHS","F601",null,"9ft","35ft+","35ft+","80\"","Remove existing board, replace with 2 smaller dry erase boards","Present below"]
["JCHS","G180",null,"9ft","50ft+","35ft+","80\"","None","Present below"]
["JCHS","V102",null,"9ft","35ft+","40ft+","80\"","None","Present above"]
[]
["TWES",206,"Art","10ft","55ft+","40ft+","75\"","Remove existing, replace with 2 smaller boards","Needed above"]
[]
["WES","Blue 104",null,"9ft","35ft+","25ft+","72\"","none","present below"]
["WES","Blue 108","Sanders","9ft","35ft+","35ft+","72\"","none","needed above","Install IFP on wall by exterior door"]
["WES","Red 303",null,"9ft","50ft+","30ft+","72\"","Remove existing, replace with 2 smaller boards","present below","Relocate A/V hookups to opposite side of air return "]
["WES","Red 304",null,"9ft","50ft+","30ft+","72\"","Remove existing, replace with 2 smaller boards","present below","Relocate A/V hookups to opposite side of air return "]
["WES","Red 310",null,"9ft","50ft+","25ft+","72\"","Remove existing, replace with 2 smaller boards","present below"]
["WES","Yellow 207",null,"9ft","60ft+","35ft+","72\"","Remove existing, replace with 2 smaller boards","present below"]
["WES","Yellow 208",null,"9ft","60ft+","35ft+","72\"","Remove existing, replace with 2 smaller boards","present below","Center IFP on front wall"]
["WES","Yellow 210",null,"9ft","60ft+","30ft+","72\"","Remove existing, replace with 2 smaller boards","present below","Center IFP on front wall"]

{"sheet":"CRMS","index":1,"n_rows":6,"n_cols":10,"rows_kept":6,"flags":["formulas_cached_only"]}
["School","Room","Teacher","Ceiling Height","HDMI/VGA/Ethernet Cable Length","3.5mm Audio Cable Length","Top of panel to be at","Dry Erase Board Needs","Power for Panel","Additional Notes"]
["CRMS","A7",null,"10ft","60ft+","30ft+","80\"","Remove existing, replace with 2 smaller boards","Needed above","Relocate A/V hookups by network drops at teacher desk location "]
["CRMS","A8",null,"10ft","60ft+","30ft+","80\"","Remove existing, replace with 2 smaller boards","Needed above"]
["CRMS","B6",null,"10ft","30ft+","40ft+","80\"","Relocate bulletin board","Needed above","Install IFP on hall wall centered between door and teacher desk"]
["CRMS","C2",null,"10ft","60ft+","35ft+","80\"","Remove existing, replace with 2 smaller boards","Needed above"]
["CRMS","C3",null,"10ft","60ft+","35ft+","80\"","Remove existing, replace with 2 smaller boards","Needed above","Install IFP on wall opposite of current SB location, move A/V hookups closer to corner"]

{"sheet":"DFES","index":2,"n_rows":6,"n_cols":10,"rows_kept":6,"flags":["formulas_cached_only"]}
["School","Room","Teacher","Ceiling Height","HDMI/VGA/Ethernet Cable Length","3.5mm Audio Cable Length","Top of panel to be at","Dry Erase Board Needs","Power for Panel","Additional Notes"]
["DFES","Yellow 9","Gifted","10ft","40ft+","35ft+","Adjustable Stand","None","Needed above","install at far left end of dry erase board"]
["DFES","Orange 3","PEC","10ft","35ft+","35ft+","Adjustable Stand","None","Present above","center on wall"]
["DFES","Orange 4","PEC","10ft","30ft+","30ft+","Adjustable Stand","None","Present above","same location as SB"]
["DFES","Purple 6","Art","10ft","65ft+","35ft+","Adjustable Stand","Remove existing, replace with 2 6ft boards","Present below","Needs dry erase board space"]
["DFES","Yellow 6 ",{"$nulls":4},"Adjustable Stand","None"]

{"sheet":"GES","index":3,"n_rows":6,"n_cols":10,"rows_kept":6,"flags":["formulas_cached_only"]}
["School","Room","Teacher","Ceiling Height","HDMI/VGA/Ethernet Cable Length","3.5mm Audio Cable Length","Top of panel to be at","Dry Erase Board Needs","Power for Panel","Additional Notes"]
["GES",407,{"$nulls":4},"72\"","None","Present above"]
["GES",604,null,"10ft","35ft+","35ft+","72\"","None","Present above"]
["GES",605,null,"10ft","35ft+","35ft+","72\"","None","Present above"]
["GES",606,null,"10ft","35ft+","35ft+","72\"","None","Present above"]
["GES",607,null,"10ft","35ft+","35ft+","72\"","None","Present above"]

{"sheet":"GSMS","index":4,"n_rows":9,"n_cols":10,"rows_kept":9,"flags":["formulas_cached_only"]}
["School","Room","Teacher","Ceiling Height","HDMI/VGA/Ethernet Cable Length","3.5mm Audio Cable Length","Top of panel to be at","Dry Erase Board Needs","Power for Panel","Additional Notes"]
["GSMS","A3",null,"10ft","35ft+","35ft+","80\"","None","Needed above","Move AV closer to teacher desk location "]
["GSMS","A4",null,"10ft","35ft+","35ft+","80\"","None","Needed above","Move AV hookups closer to exterior wall corner"]
["GSMS","B10",null,"10ft","30ft+","35ft+","80\"","None","Present below","Install IFP on opposite wall from current SB location. Move AV hookup closer to outer wall corner by network drops."]
["GSMS","B4",null,"10ft","35ft+","35ft+","80\"","None","Needed above","Move AV hookups to front wall closer to outer wall corner"]
["GSMS","C1",null,"10ft","30ft+","35ft+","80\"","None","Present below","Install IFP on opposite wall from current SB location."]
["GSMS","D1",null,"10ft","60ft+","35ft+","80\"","None","Present below"]
["GSMS","E5","Ag","10ft","30ft+","35ft+","80\"","Remove existing, replace with 2 smaller boards","Needed above","Relocate AV hookup to wall with network drop"]
["GSMS","E6","Art","10ft","45ft+","35ft+","80\"","Remove existing, replace with 2 smaller boards","Needed above"]

{"sheet":"JCHS","index":5,"n_rows":6,"n_cols":10,"rows_kept":6,"flags":["formulas_cached_only"]}
["School","Room","Teacher","Ceiling Height","HDMI/VGA/Ethernet Cable Length","3.5mm Audio Cable Length","Top of panel to be at","Dry Erase Board Needs","Power for Panel","Additional Notes"]
["JCHS","AG2","Lankford","9ft","60ft+","35ft+","80\"","Add one small dry erase board to right of IFP","Needed above","Wall is sheet metal."]
["JCHS","AG4","Martin","9ft","35ft+","35ft+","80\"","Remove existing bulletin board, replace with 2 smaller dry erase boards","Present below","Install IFP on opposite wall of current SB location.  Move AV hookups and network drop to wall where IFP will be, near corner. Wall is sheetrock."]
["JCHS","F601",null,"9ft","35ft+","35ft+","80\"","Remove existing board, replace with 2 smaller dry erase boards","Present below"]
["JCHS","G180",null,"9ft","50ft+","35ft+","80\"","None","Present below"]
["JCHS","V102",null,"9ft","35ft+","40ft+","80\"","None","Present above"]

{"sheet":"TWES","index":6,"n_rows":6,"n_cols":10,"rows_kept":6,"flags":["formulas_cached_only"]}
["School","Room","Teacher","Ceiling Height","HDMI/VGA/Ethernet Cable Length","3.5mm Audio Cable Length","Top of panel to be at","Dry Erase Board Needs","Power for Panel","Additional Notes"]
["TWES",206,"Art","10ft","55ft+","40ft+","75\"","Remove existing, replace with 2 smaller boards","Needed above"]
["TWES",513,{"$nulls":4},"72\""]
["TWES",602,{"$nulls":4},"72\""]
["TWES",{"$nulls":5},"72\""]
["TWES",{"$nulls":5},"72\""]

{"sheet":"WES","index":7,"n_rows":9,"n_cols":10,"rows_kept":9,"flags":["formulas_cached_only"]}
["School","Room","Teacher","Ceiling Height","HDMI/VGA/Ethernet Cable Length","3.5mm Audio Cable Length","Top of panel to be at","Dry Erase Board Needs","Power for Panel","Additional Notes"]
["WES","Blue 104",null,"9ft","35ft+","25ft+","72\"","none","present below"]
["WES","Blue 108","Sanders","9ft","35ft+","35ft+","72\"","none","needed above","Install IFP on wall by exterior door"]
["WES","Red 303",null,"9ft","50ft+","30ft+","72\"","Remove existing, replace with 2 smaller boards","present below","Relocate A/V hookups to opposite side of air return "]
["WES","Red 304",null,"9ft","50ft+","30ft+","72\"","Remove existing, replace with 2 smaller boards","present below","Relocate A/V hookups to opposite side of air return "]
["WES","Red 310",null,"9ft","50ft+","25ft+","72\"","Remove existing, replace with 2 smaller boards","present below"]
["WES","Yellow 207",null,"9ft","60ft+","35ft+","72\"","Remove existing, replace with 2 smaller boards","present below"]
["WES","Yellow 208",null,"9ft","60ft+","35ft+","72\"","Remove existing, replace with 2 smaller boards","present below","Center IFP on front wall"]
["WES","Yellow 210",null,"9ft","60ft+","30ft+","72\"","Remove existing, replace with 2 smaller boards","present below","Center IFP on front wall"]