Attachment D

Provide a detailed quote per school (below) using the prices/rates shown in Attachment A – Coil Cleaning for the following scenario:

The District’s maintenance department has decided to pursue coil cleaning at three (3) high schools during the 2023 – 2024 school year.  

High School “A” has the following HVAC equipment with coils:
· 108 Package water-source units above ceiling
· 7 Package rooftop units with evaporating coil and condenser
· 4 Split systems with air handlers above the ceiling that can be accessed with a step ladder and a condenser on the roof
· 2 Package DOAS units on roof or above ceiling in the mezzanine

High School “B” has the following HVAC equipment with coils:  
· 132 Split units for air handlers mounted in ceiling that can be accessed with a step ladder & condensing unit on ground level
· 28 Split system with air handler which requires lift; condensers on roof or ground
· 43 Package rooftop units with evaporating coil and condenser
· 3 Package DOAS units on roof or above ceiling in mezzanine
· 3 Package DOAS units on ground
· 1 Mini-split head location inside of building with condenser on roof or ground level

High School “C” has the following HVAC equipment with coils:
· 9 Split systems with air handlers above ceiling that can be accessed with step ladder and condenser on roof
· 5 Package rooftop units with evaporating coil and condenser
· 13 Air handlers for chilled water in penthouse and on mezzanine
· 4 Mini-split head location inside of building with condensers on roofs or ground level

