{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["FY17 Chemicals to be Bid"],"not_rendered":{"defined_names":4},"read":"whole","date_system":"1900"}

{"sheet":"FY17 Chemicals to be Bid","index":0,"n_rows":65,"n_cols":7,"rows_kept":65,"merged":[[0,0,0,6],[1,0,1,6],[2,0,2,6],[3,0,3,6],[4,0,4,6],[5,0,5,6],[6,0,6,6],[7,2,7,5],[8,2,8,5],[9,2,9,5],[10,2,10,5],[11,2,11,5],[12,2,12,5],[13,0,13,6],[14,0,14,6],[15,0,15,6],[17,0,17,6],[19,0,20,0],[20,3,20,4],[20,5,20,6],[21,0,22,0],[22,3,22,4],[22,5,22,6],[23,0,24,0],[24,3,24,4],[24,5,24,6],[25,0,26,0],[26,3,26,4],[26,5,26,6],[27,0,28,0],[28,3,28,4],[28,5,28,6],[29,0,30,0],[30,3,30,4],[30,5,30,6],[31,0,32,0],[32,3,32,4],[32,5,32,6],[33,0,34,0],[34,3,34,4],[34,5,34,6],[35,0,36,0],[36,3,36,4],[36,5,36,6],[37,0,38,0],[38,3,38,4],[38,5,38,6],[39,0,40,0],[40,3,40,4],[40,5,40,6],[41,0,42,0],[42,3,42,4],[42,5,42,6],[43,0,44,0],[44,3,44,4],[44,5,44,6],[45,0,47,0],[46,3,46,4],[46,5,46,6],[47,2,47,6],[48,0,48,6],[49,4,49,6],[54,0,54,6],[55,0,55,6],[56,0,56,6],[57,0,57,6],[58,2,58,6],[59,2,59,6],[60,2,60,6],[61,2,61,6],[62,2,62,6],[63,2,63,6],[64,2,64,6]]}
[]
["BID #16-021"]
["FY16 WATER TREATMENT CHEMICALS"]
["PRICING SUBMITTALS"]
[]
[]
["Submitted by: "]
[null,"Name of Company:"]
[null,"Mailing Address:"]
[null,"City/State/Zip: "]
[null,"Phone (including area code):"]
[null,"Name & e-mail if respondent: "]
[null,"Ordering contact if same for all orders (name/phone/email): "]
[]
["Submittal Deadline: "]
["Wednesday, May 18, 2016   at 2:00 P.M. "]
[]
[]
[null,"CITY OF GRIFFIN\nCHEMICAL/Plant Notes","DESCRIPTION","Apprx Annual Qty","UOM for price","UNIT PRICE (0.000000)","TOTAL"]
["1)","Aqua Pak Nuchar Carbon","dry weight; 45-lb bags; pallets must fit electric pallet jack with 3¾ clearance. Price in dry lbs.",{"v":10500,"d":"10,500"},"dry lbs",".",{"$f":"IF(F20=\".\",0,IF(F20=0,\"No Bid\",IF(F20>0,SUM(D20*F20))))","v":0}]
[null,"Delivers to plants 1,2","See notes for plants 1, 2","Contact phone & email:"]
["2)"," Caustic Soda (50%)","delivered 55 gallon drums @ 700 lbs ea. Price in gallons.",200,"drum",".",{"$f":"IF(F22=\".\",0,IF(F22=0,\"No Bid\",IF(F22>0,SUM(D22*F22))))","v":0}]
[null,"Delivers to plant 3","See notes for plant 3","Contact phone & email:"]
["3)"," Caustic Soda (25%)","delivered 55 gallon drums @ 700 lbs ea. Price in gallons.",30,"drum",".",{"$f":"IF(F24=\".\",0,IF(F24=0,\"No Bid\",IF(F24>0,SUM(D24*F24))))","v":0}]
[null,"Delivers to plant 3","See notes for plant 3","Contact phone & email:"]
["4)","Chemical Hydrated Lime 400  ","HI CAL NSF/ANSI 60; dry weight; 50-lb bags   (Note: Pallets to fit electric pallet jack 3-3/4 clearance). Price in dry lbs.",{"v":350000,"d":"350,000"},"dry lbs",".",{"$f":"IF(F26=\".\",0,IF(F26=0,\"No Bid\",IF(F26>0,SUM(D26*F26))))","v":0}]
[null,"Delivers to plant 1","See notes for plant 1","Contact phone & email:"]
["5)","Liquid Chlorine (150-lb cyl) ","150 lb cylinders. Price in cylinders.",54,"cyl",".",{"$f":"IF(F28=\".\",0,IF(F28=0,\"No Bid\",IF(F28>0,SUM(D28*F28))))","v":0}]
[null,"Delivers to plant 1,3,7","See notes for plant 1,3,7","Contact phone & email:"]
["6)","Liquid Chlorine (1-ton cyl)","1 ton cylinders. Price in cylinders.",69,"cyl",".",{"$f":"IF(F30=\".\",0,IF(F30=0,\"No Bid\",IF(F30>0,SUM(D30*F30))))","v":0}]
[null,"Delivers to plants 1,2,4","See notes for plants 1, 2,4","Contact phone & email:"]
["7)","Liquid Phosphate -Aquadene SK7870","275 gallons per tote; (Valve has to accept 2” Cam Lock Connector; has to fit electric pallet jack with 3 ¾ clearance). Price in wet lbs.",{"v":71880,"d":"71,880"},"wet lbs",".",{"$f":"IF(F32=\".\",0,IF(F32=0,\"No Bid\",IF(F32>0,SUM(D32*F32))))","v":0}]
[null,"Delivers to plants 1,2","See notes for plants 1,2","Contact phone & email:"]
["8)","Magnifloc LT7989 Flocculent ","liquid polymer; NO substitutions; delivered in 55 gal drums. Price in wet lbs.",{"v":25000,"d":"25,000"},"wet lbs",".",{"$f":"IF(F34=\".\",0,IF(F34=0,\"No Bid\",IF(F34>0,SUM(D34*F34))))","v":0}]
[null,"Delivers to plant 1 ","See notes for plant 1","Contact phone & email:"]
["9)","Potassium Permanganate","dry weight; 55-lb containers (ordered by pallets); delivered in 5-gal, 55 lb containers. Price in lbs.",{"v":7500,"d":"7,500"},"dry lbs",".",{"$f":"IF(F36=\".\",0,IF(F36=0,\"No Bid\",IF(F36>0,SUM(D36*F36))))","v":0}]
[null,"Delivers to plants 2,4,5*","See notes for plants 2,4,5","Contact phone & email:"]
["10)"," Soda Ash (50lb bags)","delivered in 275 gallon totes. Price in gallons.",{"v":22500,"d":"22,500"},"lbs",".",{"$f":"IF(F38=\".\",0,IF(F38=0,\"No Bid\",IF(F38>0,SUM(D38*F38))))","v":0}]
[null,"Delivers to plant 1","See notes for plant 1","Contact phone & email:"]
["11)"," Sodium Chlorite – 25% ","BULK - domestic liquid; delivered in 4500 gal loads . Price in wet lbs.",{"v":310000,"d":"310,000"},"wet lbs",".",{"$f":"IF(F40=\".\",0,IF(F40=0,\"No Bid\",IF(F40>0,SUM(D40*F40))))","v":0}]
[null,"Delivers to plants 1,2","See notes for plants 1, 2","Contact phone & email:"]
["12)"," Sodium Hypochlorite (10-15% solution)","delivered in 275 gallon totes. Price in gallons.    POSSIBLE ",{"v":15000,"d":"15,000"},"gal",".",{"$f":"IF(F42=\".\",0,IF(F42=0,\"No Bid\",IF(F42>0,SUM(D42*F42))))","v":0}]
[null,"Delivers to plant 1","See notes for plant 1","Contact phone & email:"]
["13)"," Sodium Permanganate 20%","delivered in 275 gallon totes. Price in gallons.",{"v":1100,"d":"1,100"},"gal",".",{"$f":"IF(F44=\".\",0,IF(F44=0,\"No Bid\",IF(F44>0,SUM(D44*F44))))","v":0}]
[null,"Delivers to plant 1","See notes for plant 1","Contact phone & email:"]
["14)"," Sodium Silico Fluoride ","Manufactured in USA preferred; delivered in 50-lb bags. Price in dry lbs.",{"v":44000,"d":"44,000"},"dry lbs",".",{"$f":"IF(F46=\".\",0,IF(F46=0,\"No Bid\",IF(F46>0,SUM(D46*F46))))","v":0}]
[null,"Delivers to plants 1,2","See notes for plants 1, 2","Contact phone & email:"]
[null,"State Orgin of Manufacture:"]
["All Chemicals are to be FOB Griffin, GA with NO fuel adjustment cost. All Chemicals are to be NF 60 Approved and the CAS Registry Number must be provided.   "]
[null,"Prices submitted (#)",null,"Order contact (email & phone)"]
[]
[null,"Company Name:",{"$nulls":3},"Date Price Submitted: "]
[]
[]
["City of Griffin - Delivery Location addresses and delivery times: "]
["         1                                2                               3                             4                               5                             6                                     7"]
["Harry Simmons            Still Branch Reservoir            Cabin Creek                     Potato Creek                       Shoal Creek               Flint River Pump Station            Sun City Chlorine Booster           \n229 N. Expressway        2045 Flat Shoals Rd            1140 N Hill Street           1150 County Line Rd           2940 W Ellis Rd                1010 Salem Road                        1196 Jordan Hill Road\nGriffin, GA  30223          Concord, GA  30206           Griffin, GA  30224             Griffin, GA  30224            Griffin, GA  30224              Griffin, GA  30224                       Griffin, GA  30223"]
["8A - 2P deliveries     |     8A - 2P deliveries       |     10A- 2P deliveries      |    8A - 2P deliveries       |      8A - 2P deliveries     |  Contact 24hr in adv to schedule    |      8A - 2P deliveries       "]
["*","  GENERAL  Considerations: ","-  Make sure you meet the plant specific delivery considerations for the chemicals singled out below.\n-  Any specific questions are to be submitted; they will be answered by the specific plant and you will receive an \n   email response.  Any questions of significance will be compiled into an addendum.\n-  Invoices are to be sent to the ordering plant."]
[null,"Special Considerations for\n Plant 1: ","-  Chlorine, 1-ton cyl:  must be delivered by short (≤ 30 feet) flat bed trailer with fifth wheel and lift gate. (no B-frames).\n-  Chlorite:  must be delivered by tanker pumper with rear discharge able to pump 25 ft.\n-  All pallet deliveries must fit existing pallet jack with 3 3/4 clearance."]
[null,"Special Considerations for\n Plant 2: ","-  General:  lift arm cross bar on boom raises to height of 10'10\" from ground (7' from dock)\n-  General:  All pallet deliveries must fit existing pallet jack with 3 3/4 clearance. \n-  Chlorine: 1-ton cyl:  must be delivered by short (≤ 30 feet) flat bed trailer with fifth wheel and lift gate. (no B-frames).\n-  Sodium Hypochlorite: Facility will only provide outside hookup - vendor is responsible for providing means of off loading chemical."]
[null,"Special Considerations for\n Plants 3, 4 and 5: ","-  General:  low boom; very sharp turn to dock\n-  General: deliveries need to be by vehicles ≤ 40 feet. This may be by enclosed truck, standard box trailer with lift gate or by flatbeds."]
[null,"Special Considerations for\n Plant 6: ","- Must be delivered by short (≤ 30 feet) flat bed trailer with fifth wheel and lift gate. (no B-frames). \n-  All pallet deliveries must fit existing pallet jack with 3 3/4 clearance. "]
[null,"Special Considerations for\n Plant 7: ","- Chlorine, 150-lb cylinders:  delivery of these cylinders will be coordinated through the Harry Simmons WTP but be delivered to the Sun City Chlorine Booster Pump Station.  We try to schedule the delivery of the tanks with the delivery for Plant 3 (Cabin Creek).  Lift gate is needed for delivery."]
["*","  Special Note: ","-  Sodium Hypochlorite (10-15% solution) is currently under consideration and there is no guarantee that it will be used. The quantity listed is an estimated quantity that may be needed if the City convert to a bleach system for disinfection purposes.\n"]