{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["BidItems"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"BidItems","index":0,"n_rows":116,"n_cols":18,"rows_kept":116,"merged":[[1,3,1,5],[2,3,2,5],[3,3,3,5],[4,3,4,5],[5,3,5,5],[6,3,6,5],[7,3,7,5],[8,3,8,5],[9,3,9,5],[10,3,10,5],[11,3,11,5],[12,3,12,5],[13,3,13,5],[14,3,14,5],[15,3,15,5],[16,3,16,5],[17,3,17,5],[18,3,18,5],[19,3,19,5],[52,2,52,7],[87,2,87,7],[92,2,92,7],[98,2,98,7],[104,2,104,7],[109,2,109,7],[115,1,115,9]],"flags":["formulas_cached_only"]}
[null,"***Bidder shall enter all positions, and their hourly rates below, for any prevailing wage hourly workers that will be working on this contract.  Prevailing wage rates must be taken into account in Bidder’s unit prices submitted below.***"]
[null,null,"PREVAILING WAGE POSITIONS UTILIZED","PREVAILING WAGE HOURLY RATE "]
{"$rows_empty":19}
[null,"***Bidder Please Note:  To be responsive you MUST enter a Unit Price for each line item below.***"]
["Callout","ItemNumber","ItemDescription","Class","Color","Est Quant","Act Quant","Unit","UnitPrice","MarkingType","Amount"]
[null,"ITEM","DESCRIPTION","CLASS","COLOR","QTY","Qty","UNIT","TOTAL",null,"TOTAL"]
[null,null,"GROUP I- MARKINGS (VDOT TYPE A- PAINT)",{"$nulls":6},"`",{"$nulls":7},"White"]
["A",1,"PROVIDE AND INSTALL 4 INCH TRANSVERSE MARKINGS","N/A","white or yellow",50,null,"LF",null,"GROUP I MARKINGS (VDOT TYPE A - PAINT)",0,{"$nulls":6},"Yellow"]
["F",2,"PROVIDE AND INSTALL 6 INCH TRANSVERSE MARKINGS","N/A","white or yellow",50,null,"LF",null,"GROUP I MARKINGS (VDOT TYPE A - PAINT)",0,{"$nulls":6},"Black"]
[null,3,"PROVIDE AND INSTALL 8 INCH TRANSVERSE MARKINGS","N/A","white or yellow",50,null,"LF",null,"GROUP I MARKINGS (VDOT TYPE A - PAINT)",0]
[null,4,"PROVIDE AND INSTALL 12 INCH TRANSVERSE MARKINGS","N/A","white or yellow",50,null,"LF",null,"GROUP I MARKINGS (VDOT TYPE A - PAINT)",0,{"$nulls":6},"Paving N-1"]
["D",5,"PROVIDE AND INSTALL 18 INCH TRANSVERSE MARKINGS","N/A","white or yellow",50,null,"LF",null,"GROUP I MARKINGS (VDOT TYPE A - PAINT)",0,{"$nulls":6},"Paving N-2"]
["E",6,"PROVIDE AND INSTALL 24 INCH TRANSVERSE MARKINGS","N/A","white or yellow",100,null,"LF",null,"GROUP I MARKINGS (VDOT TYPE A - PAINT)",0,{"$nulls":6},"Paving N-3"]
[null,7,"PROVIDE AND INSTALL YIELD LINE MARKINGS (24 INCH TRIANGLE/12 INCH SPACING) - NOTE: LF IS WIDTH OF LANE","N/A","White",50,null,"LF",null,"GROUP I MARKINGS (VDOT TYPE A - PAINT)",0,{"$nulls":6},"Paving N-4"]
["A",8,"PROVIDE AND INSTALL 4 INCH LONGITUDINAL SOLID LINE","N/A","white or yellow",500,null,"LF",null,"GROUP I MARKINGS (VDOT TYPE A - PAINT)",0,{"$nulls":6},"Paving N-5"]
["F",9,"PROVIDE AND INSTALL 6 INCH LONGITUDINAL SOLID LINE","N/A","white or yellow",100,null,"LF",null,"GROUP I MARKINGS (VDOT TYPE A - PAINT)",0,{"$nulls":6},"Paving N-10"]
[null,10,"PROVIDE AND INSTALL 8 INCH LONGITUDINAL SOLID LINE","N/A","white or yellow",50,null,"LF",null,"GROUP I MARKINGS (VDOT TYPE A - PAINT)",0,{"$nulls":6},"Paving S-2"]
[null,11,"PROVIDE AND INSTALL 12 INCH LONGITUDINAL SOLID LINE","N/A","white or yellow",50,null,"LF",null,"GROUP I MARKINGS (VDOT TYPE A - PAINT)",0,{"$nulls":6},"Paving S-6"]
["I",12,"PROVIDE AND INSTALL LONGITUDINAL  SOLID 4 INCH DOUBLE LINE (TWO 4 INCH SOLID LINES WITH 4 INCH SPACING)",1,"White OR Yellow",100,null,"LF",null,"GROUP I MARKINGS (VDOT TYPE A - PAINT)",0,{"$nulls":6},"Paving S-7"]
["I",13,"PROVIDE AND INSTALL 12 INCH YELLOW LONGITUDINAL CENTERLINE (TWO 4 INCH YELLOW LINES WITH 4 INCH SEPARATION)","N/A","Yellow",100,null,"LF",null,"GROUP I MARKINGS (VDOT TYPE A - PAINT)",0,{"$nulls":6},"Paving S-8"]
[null,14,"PROVIDE AND INSTALL 12 INCH YELLOW TWO WAY LEFT TURN LANE MARKING (ONE 4 INCH SOLID YELLOW LINE AND ONE 4 INCH YELLOW SKIP LINE) ","N/A","Yellow",50,null,"LF",null,"GROUP I MARKINGS (VDOT TYPE A - PAINT)",0]
[null,15,"PROVIDE AND INSTALL 6 FOOT PEDESTRIAN SYMBOL","N/A","White",25,null,"EA",null,"GROUP I MARKINGS (VDOT TYPE A - PAINT)",0]
["M",16,"PROVIDE AND INSTALL 8 FOOT  LETTERS","N/A","White",7,null,"EA",null,"GROUP I MARKINGS (VDOT TYPE A - PAINT)",0]
["K",17,"PROVIDE AND INSTALL SINGLE ARROWS","N/A","White",7,null,"EA",null,"GROUP I MARKINGS (VDOT TYPE A - PAINT)",0]
["L",18,"PROVIDE AND INSTALL COMBINATION ARROWS","N/A","White",5,null,"EA",null,"GROUP I MARKINGS (VDOT TYPE A - PAINT)",0]
["K",19,"PROVIDE AND INSTALL LANE REDUCTION ARROWS","N/A","White",5,null,"EA",null,"GROUP I MARKINGS (VDOT TYPE A - PAINT)",0]
[null,20,"PROVIDE AND INSTALL 13 FOOT YIELD AHEAD SYMBOL","N/A","White",5,null,"EA",null,"GROUP I MARKINGS (VDOT TYPE A - PAINT)",0]
[null,21,"PROVIDE AND INSTALL SPEED HUMP MARKINGS - NOTE: MUTCD FIG. 3B-29 OPTION A OR FIG. 3B-30 OPTION A AS APPROPRIATE, 2 EACH PER HUMP ","N/A","White",5,null,"EA",null,"GROUP I MARKINGS (VDOT TYPE A - PAINT)",0]
[null,22,"PROVIDE AND INSTALL  STANDARD BICYCLE SYMBOLS - NOTE: STANDARD HIGHWAY SIGNS PAGE 10-16 \"SKINNY BIKE\", SEE ATTACHED ","N/A","White",2,null,"EA",null,"GROUP I MARKINGS (VDOT TYPE A - PAINT)",0]
[null,23,"PROVIDE AND INSTALL SHARED LANE SYMBOLS - NOTE: SEE ATTACHED ","N/A","White",25,null,"EA",null,"GROUP I MARKINGS (VDOT TYPE A - PAINT)",0]
[null,24,"PROVIDE AND INSTALL  BICYCLE DETECTOR SYMBOL - NOTE: STANDARD HIGHWAY SIGNS PAGE 10-17 ","N/A","White",5,null,"EA",null,"GROUP I MARKINGS (VDOT TYPE A - PAINT)",0]
[null,25,"PROVIDE AND INSTALL 6 FOOT BICYCLE LANE ARROW","N/A","White",5,null,"EA",null,"GROUP I MARKINGS (VDOT TYPE A - PAINT)",0]
[null,26,"PROVIDE AND INSTALL PREFERENTIAL LANE SYMBOL","N/A","White",10,null,"EA",null,"GROUP I MARKINGS (VDOT TYPE A - PAINT)",0]
[null,27,"PROVIDE AND INSTALL HANDICAP SYMBOL","N/A","White",2,null,"EA",null,"GROUP I MARKINGS (VDOT TYPE A - PAINT)",0]
[null,null,"GROUP II- MARKINGS \n(VDOT TYPE B\n CLASS I, II,III & IV THERMO/EPOXY)"]
["A",28,"PROVIDE AND INSTALL 4 INCH TRANSVERSE MARKINGS",1,"White OR Yellow",{"v":2000,"d":"2,000"},null,"LF",null,"GROUP II MARKINGS (VDOT TYPE B CLASS I, II, III, & VI - THERMO/EPOXY)",0]
["F",29,"PROVIDE AND INSTALL 6 INCH TRANSVERSE MARKINGS",1,"White OR Yellow",{"v":12000,"d":"12,000"},null,"LF",null,"GROUP II MARKINGS (VDOT TYPE B CLASS I, II, III, & VI - THERMO/EPOXY)",0]
[null,30,"PROVIDE AND INSTALL 8 INCH TRANSVERSE MARKINGS",1,"White OR Yellow",250,null,"LF",null,"GROUP II MARKINGS (VDOT TYPE B CLASS I, II, III, & VI - THERMO/EPOXY)",0]
[null,31,"PROVIDE AND INSTALL 12 INCH TRANSVERSE MARKINGS",1,"White OR Yellow",{"v":1000,"d":"1,000"},null,"LF",null,"GROUP II MARKINGS (VDOT TYPE B CLASS I, II, III, & VI - THERMO/EPOXY)",0]
["D",32,"PROVDE AND INSTALL 18 INCH TRANSVERSE MARKINGS",1,"White OR Yellow",{"v":5000,"d":"5,000"},null,"LF",null,"GROUP II MARKINGS (VDOT TYPE B CLASS I, II, III, & VI - THERMO/EPOXY)",0]
["E",33,"PROVIDE AND INSTALL 24 INCH TRANSVERSE MARKINGS",1,"White OR Yellow",{"v":18000,"d":"18,000"},null,"LF",null,"GROUP II MARKINGS (VDOT TYPE B CLASS I, II, III, & VI - THERMO/EPOXY)",0]
[null,34,"PROVIDE AND INSTALL YIELD LINE MARKINGS (24 INCH TRIANGLE/12 INCH SPACING) - NOTE: LF IS WIDTH OF LANE",1,"White",500,null,"LF",null,"GROUP II MARKINGS (VDOT TYPE B CLASS I, II, III, & VI - THERMO/EPOXY)",0]
["A",35,"PROVIDE AND INSTALL 4 INCH LONGITUDINAL SOLID LINE ",1,"White OR Yellow",{"v":25000,"d":"25,000"},null,"LF",null,"GROUP II MARKINGS (VDOT TYPE B CLASS I, II, III, & VI - THERMO/EPOXY)",0]
["B G H",36,"PROVIDE AND INSTALL 4 INCH LONGITUDINAL SKIP LINES",1,"White OR Yellow",{"v":12000,"d":"12,000"},null,"LF",null,"GROUP II MARKINGS (VDOT TYPE B CLASS I, II, III, & VI - THERMO/EPOXY)",0]
["F",37,"PROVIDE AND INSTALL 6 INCH LONGITUDINAL SOLID LINE",1,"White OR Yellow",{"v":20000,"d":"20,000"},null,"LF",null,"GROUP II MARKINGS (VDOT TYPE B CLASS I, II, III, & VI - THERMO/EPOXY)",0]
["N S T",38,"PROVIDE AND INSTALL 6 INCH LONGITUDINAL SKIP LINES",1,"White OR Yellow",{"v":10000,"d":"10,000"},null,"LF",null,"GROUP II MARKINGS (VDOT TYPE B CLASS I, II, III, & VI - THERMO/EPOXY)",0]
[null,39,"PROVIDE AND INSTALL 8 INCH LONGITUDINAL SOLID LINE ",1,"White OR Yellow",200,null,"LF",null,"GROUP II MARKINGS (VDOT TYPE B CLASS I, II, III, & VI - THERMO/EPOXY)",0]
[null,40,"PROVIDE AND INSTALL 8 INCH LONGITUDINAL SKIP LINES ",1,"White OR Yellow",200,null,"LF",null,"GROUP II MARKINGS (VDOT TYPE B CLASS I, II, III, & VI - THERMO/EPOXY)",0]
[null,41,"PROVIDE AND INSTALL 12 INCH LONGITUDINAL SOLID LINE",1,"White OR Yellow",500,null,"LF",null,"GROUP II MARKINGS (VDOT TYPE B CLASS I, II, III, & VI - THERMO/EPOXY)",0]
[null,42,"PROVIDE AND INSTALL 12 INCH LONGITUDINAL SKIP LINES",1,"White OR Yellow",500,null,"LF",null,"GROUP II MARKINGS (VDOT TYPE B CLASS I, II, III, & VI - THERMO/EPOXY)",0]
[null,43,"PROVIDE AND INSTALL SOLID 4 INCH DOUBLE LINE (TWO 4 INCH SOLID LINES WITH 4 INCH SPACING)",1,"White OR Yellow",{"v":1000,"d":"1,000"},null,"LF",null,"GROUP II MARKINGS (VDOT TYPE B CLASS I, II, III, & VI - THERMO/EPOXY)",0]
[null,44,"PROVIDE AND INSTALL LONGITUDINAL  SOLID 6 INCH DOUBLE LINE (TWO 6 INCH SOLID LINES WITH 4 INCH SPACING)",1,"White OR Yellow",100,null,"LF",null,"GROUP II MARKINGS (VDOT TYPE B CLASS I, II, III, & VI - THERMO/EPOXY)",0]
[null,45,"PROVIDE AND INSTALL LONGITUDINAL WIDE SOLID DOUBLE LINE (TWO 8 INCH SOLID LINES WITH 4 INCH SPACING)",1,"white",50,null,"LF",null,"GROUP II MARKINGS (VDOT TYPE B CLASS I, II, III, & VI - THERMO/EPOXY)",0]
[null,46,"PROVIDE AND INSTALL 12 INCH YELLOW LONGITUDINAL CENTERLINE (TWO FOUR (4) INCH YELLOW LINES WITH FOUR (4) INCH SEPARATION)",1,"Yellow",{"v":25000,"d":"25,000"},null,"LF",null,"GROUP II MARKINGS (VDOT TYPE B CLASS I, II, III, & VI - THERMO/EPOXY)",0]
[null,47,"PROVIDE AND INSTALL 12 INCH YELLOW TWO WAY LEFT TURN LANE MARKING (ONE 4 INCH SOLID YELLOW LINE AND ONE 4 INCH YELLOW SKIP LINE (10/30) WITH 4 INCH INCH SPACING)",1,"Yellow",{"v":1000,"d":"1,000"},null,"LF",null,"GROUP II MARKINGS (VDOT TYPE B CLASS I, II, III, & VI - THERMO/EPOXY)",0]
[null,48,"PROVIDE AND INSTALL LONGITUDINAL WIDE DOUBLE SKIP LINE ",1,"Yellow",500,null,"LF",null,"GROUP II MARKINGS (VDOT TYPE B CLASS I, II, III, & VI - THERMO/EPOXY)",0]
[null,49,"PROVIDE AND INSTALL 6 FOOT PEDESTRIAN SYMBOL",1,"White",25,null,"LF",null,"GROUP II MARKINGS (VDOT TYPE B CLASS I, II, III, & VI - THERMO/EPOXY)",0]
[null,50,"PROVIDE AND INSTALL 6 FOOT LETTERS",1,"White",25,null,"LF",null,"GROUP II MARKINGS (VDOT TYPE B CLASS I, II, III, & VI - THERMO/EPOXY)",0]
[null,51,"PROVIDE AND INSTALL 8 FOOT LETTERS",1,"White",125,null,"EA",null,"GROUP II MARKINGS (VDOT TYPE B CLASS I, II, III, & VI - THERMO/EPOXY)",0]
["K",52,"PROVIDE AND INSTALL SINGLE ARROWS",1,"White",125,null,"EA",null,"GROUP II MARKINGS (VDOT TYPE B CLASS I, II, III, & VI - THERMO/EPOXY)",0]
["L",53,"PROVIDE AND INSTALL COMBINATION ARROWS",1,"White",50,null,"EA",null,"GROUP II MARKINGS (VDOT TYPE B CLASS I, II, III, & VI - THERMO/EPOXY)",0]
["K",54,"PROVIDE AND INSTALL LANE REDUCTION ARROWS",1,"White",10,null,"EA",null,"GROUP II MARKINGS (VDOT TYPE B CLASS I, II, III, & VI - THERMO/EPOXY)",0]
[null,55,"PROVIDE AND INSTALL SPEED HUMP MARKINGS - NOTE: MUTCD FIG. 3B-29 OPTION A OR FIG. 3B-30 OPTION A AS APPROPRIATE, 2 EACH PER HUMP ",1,"White",25,null,"EA",null,"GROUP II MARKINGS (VDOT TYPE B CLASS I, II, III, & VI - THERMO/EPOXY)",0]
[null,56,"PROVIDE AND INSTALL  STANDARD \"HELMETED\" BICYCLE SYMBOL",1,"White",125,null,"EA",null,"GROUP II MARKINGS (VDOT TYPE B CLASS I, II, III, & VI - THERMO/EPOXY)",0]
[null,57,"PROVIDE AND INSTALL SHARED LANE SYMBOLS - NOTE: SEE ATTACHED ",1,"White",50,null,"EA",null,"GROUP II MARKINGS (VDOT TYPE B CLASS I, II, III, & VI - THERMO/EPOXY)",0]
[null,58,"PROVIDE AND INSTALL  BICYCLE DETECTOR SYMBOL - NOTE: STANDARD HIGHWAY SIGNS PAGE 10-17 ",1,"White",2,null,"EA",null,"GROUP II MARKINGS (VDOT TYPE B CLASS I, II, III, & VI - THERMO/EPOXY)",0]
[null,59,"PROVIDE AND INSTALL 6 FOOT BICYCLE LANE ARROW",1,"White",10,null,"EA",null,"GROUP II MARKINGS (VDOT TYPE B CLASS I, II, III, & VI - THERMO/EPOXY)",0]
[null,60,"PROVIDE AND INSTALL PREFERENTIAL LANE SYMBOL",1,"White",5,null,"EA",null,"GROUP II MARKINGS (VDOT TYPE B CLASS I, II, III, & VI - THERMO/EPOXY)",0]
[null,61,"PROVIDE AND INSTALL HANDICAP SYMBOL",1,"White",10,null,"EA",null,"GROUP II MARKINGS (VDOT TYPE B CLASS I, II, III, & VI - THERMO/EPOXY)",0]
[null,null,"GROUP III-\nTEMPORARY MARKINGS \n(VDOT TYPE D & E)"]
[null,62,"PROVIDE AND INSTALL REMOVABLE TAPE 4 INCH BY 4 INCH SQUARE OR DOT - NOTE: LF INCLUDES SPACING PER CONTRACT SPECS","N/A","White",1000,null,"LF",null,"GROUP III - TEMPORARY MARKINGS",0]
[null,63,"PROVIDE AND INSTALL REMOVABLE TAPE 4 INCH LINE (BLACK)","N/A","Black",5000,null,"LF",null,"GROUP III - TEMPORARY MARKINGS",0]
[null,64,"PROVIDE AND INSTALL REMOVABLE TAPE 6 INCH LINE (BLACK)","N/A","Black",1000,null,"LF",null,"GROUP III - TEMPORARY MARKINGS",0]
[null,65,"PROVIDE AND INSTALL REMOVABLE TAPE 12 INCH LINE (BLACK)","N/A","Black",500,null,"LF",null,"GROUP III - TEMPORARY MARKINGS",0]
[null,null,"GROUP IV- \nMARKINGS REMOVAL "]
[null,66,"REMOVAL OF EXISTING LONGITUDINAL LINES (UP TO AND INCLUDING 6 INCH WIDTH) - NOTE: BASE UNIT FOR REMOVAL","N/A","N/A",1500,null,"LF",null,"GROUP IV - MARKING REMOVAL",0]
[null,67,"REMOVAL OF EXISTING LONGITUDINAL LINES (EACH ADDITONAL 6 INCH INCREMENT) - NOTE: ADD TO BASE UNIT FOR LINES WIDER THAN 6 INCHES","N/A","N/A",1000,null,"LF",null,"GROUP IV - MARKING REMOVAL",0]
[null,68,"REMOVAL OF EXISTING TRANSVERSE LINES (UP TO AND INCLUDING 6 INCH WITDH) - NOTE: BASE UNIT FOR REMOVAL","N/A","N/A",1000,null,"LF",null,"GROUP IV - MARKING REMOVAL",0]
[null,69,"REMOVAL OF EXISTING TRANSVERSE LINES (EACH ADDITIONAL 6 INCH INCREMENT) - NOTE: ADD TO BASE UNIT FOR LINES WIDER THAN 6 INCHES","N/A","N/A",1000,null,"LF",null,"GROUP IV - MARKING REMOVAL",0]
[null,70,"REMOVAL OF EXISTING SYMBOLS, LETTERS, ARROWS","N/A","N/A",100,null,"EA",null,"GROUP IV - MARKING REMOVAL",0]
[null,null,"GROUP V- PREFORMED/COLORED THERMO"]
[null,71,"Colorized bike lane markings","N/A","GREEN",1000,null,"SF",null,"GROUP V-COLORED THERMO",0]
[null,72,"MMA (FHWA/MUTCD approved Red/Green or other)","N/A","GREEN/RED",6000,null,"SF ",null,"GROUP V-COLORED THERMO",0]
[null,73,"Preformed Thermo (Type B Cl II) Bike Lane Symbol with Green Background 4’x7’; includes epoxy adhesive","N/A","GREEN",50,null,"EA",null,"GROUP V-COLORED THERMO",0]
[null,74,"Preformed Thermo (Type B Cl II) Green 2'x5'; includes epoxy adhesive","N/A","GREEN",5000,null,"SF",null,"GROUP V-COLORED THERMO",0]
[null,75,"Preformed Thermo Letters (Stencils)","N/A","WHITE",100,null,"EA",null,"GROUP V-COLORED THERMO",0]
[null,null,"GROUP VI- CONTRAST"]
[null,76,"Type B Cl VI 4” Contrast","N/A","WHITE/ BLACK",1000,null,"LF",null,"GROUP VI-CONTRAST",0]
[null,77,"Type B Cl VI 6” Contrast","N/A","WHITE/ BLACK",1500,null,"LF",null,"GROUP VI-CONTRAST",0]
[null,78,"Type B Cl VI 8” Contrast","N/A","WHITE/ BLACK",500,null,"LF",null,"GROUP VI-CONTRAST",0]
[null,79,"Type B Cl VI 12” Contrast","N/A","WHITE/ BLACK",500,null,"LF",null,"GROUP VI-CONTRAST",0]
[null,null,"GROUP VII- LANE BARRIERS"]
[null,80,"Flexible Post Delineators- 36\" tall","N/A","White/  Yellow",200,null,"EA",null,"GROUP VII - LANE BARRIERS",0]
[null,81,"\tRubber wheel stops- 72\" long x 6\" wide x 4\" tall","N/A","N/A",100,null,"EA",null,"GROUP VII - LANE BARRIERS",0]
[null,82,"\tLinear bike lane separator- 29.5\" long x 4.75\" wide x 4\" tall","N/A","N/A",20,null,"EA",null,"GROUP VII - LANE BARRIERS",0]
[null,83,"\tPrecast concrete barrier- 96\" long x 18\" wide x 4.5\" tall","N/A","N/A",30,null,"EA",null,"GROUP VII - LANE BARRIERS",0]
[null,84,"\tPrecast concrete barrier- 96\" long x 18\" wide x 6\" tall","N/A","N/A",30,null,"EA",null,"GROUP VII - LANE BARRIERS",0]
[null,"GRAND TOTAL- BID PRICE (Items 1-84):",{"$nulls":8},0]