{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Exhibit A"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Exhibit A","index":0,"n_rows":184,"n_cols":8,"rows_kept":184,"merged":[[0,0,0,7],[1,0,1,7],[2,0,2,7],[5,0,5,1],[161,0,161,1],[162,0,162,1],[163,0,163,1],[164,0,164,1],[165,0,165,1],[166,0,166,1],[167,0,167,1],[168,0,168,1],[173,1,173,7],[175,1,175,7],[176,1,176,7],[177,1,177,7],[178,1,178,7],[179,1,179,7],[180,1,180,7],[182,3,182,5],[183,3,183,5]],"flags":["formulas_cached_only"]}
["Exhibit A - Request for Quote - Musical Instrument Repairs 2021-2026"]
["RFQ0321INSTRP"]
[]
["Vendor:"]
[]
["Instructions: Complete all yellow fields"]
["Instruments","Services","2021-22 Unit Price","2022-23 Unit Price","2023-24 Unit Price","2024-25 Unit Price","2025-26 Unit Price","Turnaround time for repair (pick-up to return)"]
["BAND INSTRUMENTS - BRASS"]
["Trumpet","Playing Condition: The work necessary to restore the instrument's playability and durability for at least one year of service. (Includes: solder work, springs, valve adjustments, accessible dents, corks, lubes)"]
["Trumpet","Chemical flush: treat instrument for lime and scale by disassembling instrument and dipping in a sulfamic solution. Scrub out the horn with soap and water and dry it thoroughly. Horn is reassembled with fresh lubes, new corks and felts."]
["Trumpet","Pull stuck slide"]
["Trumpet","Straighten bent key"]
["Trumpet","Straighten valve stem"]
["French Horn Single","Playing Condition: The work necessary to restore the instrument's playability and durability for at least one year of service. (Includes: solder work, springs, valve adjustments, accessible dents, corks, lubes)"]
["French Horn Single","Chemical flush: treat instrument for lime and scale by disassembling instrument and dipping in a sulfamic solution. Scrub out the horn with soap and water and dry it thoroughly. Horn is reassembled with fresh lubes, new corks and felts."]
["French Horn Single","Pull stuck slide"]
["French Horn Single","Straighten bent key"]
["French Horn Single","Straighten valve stem"]
["French Horn Double","Playing Condition: The work necessary to restore the instrument's playability and durability for at least one year of service. (Includes: solder work, springs, valve adjustments, accessible dents, corks, lubes)"]
["French Horn Double","Chemical flush: treat instrument for lime and scale by disassembling instrument and dipping in a sulfamic solution. Scrub out the horn with soap and water and dry it thoroughly. Horn is reassembled with fresh lubes, new corks and felts."]
["French Horn Double","Pull stuck slide"]
["French Horn Double","Straighten bent key"]
["French Horn Double","Straighten valve stem"]
["Marching Baritone","Playing Condition: The work necessary to restore the instrument's playability and durability for at least one year of service. (Includes: solder work, springs, valve adjustments, accessible dents, corks, lubes)"]
["Marching Baritone","Chemical flush: treat instrument for lime and scale by disassembling instrument and dipping in a sulfamic solution. Scrub out the horn with soap and water and dry it thoroughly. Horn is reassembled with fresh lubes, new corks and felts. "]
["Marching Baritone","Pull stuck slide"]
["Marching Baritone","Straighten bent key"]
["Marching Baritone","Straighten valve stem"]
["Euphonium/Baritone","Replace spit cork"]
["Euphonium/Baritone","Replace spit valve spring"]
["Euphonium/Baritone","Playing condition: The work necessary to restore the instrument's playability and durability for at least one year of service.(includes: solder work, springs, valve adjustments, accessible dents, corks)"]
["Euphonium/Baritone","Pull stuck slide"]
["Euphonium/Baritone","Pull stuck mouthpiece"]
["Euphonium/Baritone","Straighten bent key"]
["Euphonium/Baritone","Straighten valve system"]
["Euphonium/Baritone","Chemical Flush/Cleaning (3 valve)"]
["Euphonium/Baritone","Chemical Flush/Cleaning (4 valve)"]
["Sousaphone","Playing condition: The work necessary to restore the instrument's playability and durability for at least one year of service.(includes: solder work, springs, valve adjustments, accessible dents, corks)"]
["Sousaphone","Pull stuck slide"]
["Sousaphone","Straighten bent key"]
["Sousaphone","Straighten valve system"]
["Sousaphone","Replace valve spring"]
["Sousaphone","Chemical Flush/Cleaning (fiberglass)"]
["Sousaphone","Chemical Flush/Cleaning (lacquer)"]
["Tuba - Specify if bids are different for 4/4 and 3/4. Otherwise, it will be assumed the bid is for both.","Playing condition: The work necessary to restore the instrument's playability and durability for at least one year of service.(includes: solder work, springs, valve adjustments, accessible dents, corks)"]
["Tuba","Pull stuck slide"]
["Tuba","Straighten bent key"]
["Tuba","Straighten valve system"]
["Tuba","Chemical Flush/Cleaning (3 valve)"]
["Tuba","Chemical Flush/Cleaning (4 valve)"]
[null,"Subtotals"," "," "," "," "," "]
["BAND INSTRUMENTS - WOODWIND"]
["Flute ","Complete re-pad of all keys and to include: disassembly, cleaning, correcting all spring and rod problems, replace key corks, clean old glue from pad cups, repair nicked tone holes, leveling and adjusting keys, and parts."]
["Flute ","Replace and seat one pad"]
["Flute ","Playing condition: The work necessary to restore the instrument's playability and durability for at least one year of service.(Includes pads, solder work, springs, key adjustments."]
["Flute ","Straighten a bent key"]
["Oboe ","Complete re-pad of all keys and to include: disassembly, cleaning, correcting all spring and rod problems, replace key corks, clean old glue from pad cups, repair nicked tone holes, leveling and adjusting keys, and parts."]
["Oboe ","Replace and seat one pad"]
["Oboe ","Playing condition: The work necessary to restore the instrument's playability and durability for at least one year of service.(Includes pads, solder work, springs, key adjustments."]
["Oboe ","Repair basic crack"]
["Oboe ","Straighten a bent key"]
["Clarinet","Complete re-pad of all keys and to include: disassembly, cleaning, correcting all spring and rod problems, replace key corks, clean old glue from pad cups, repair nicked tone holes, leveling and adjusting keys, and parts."]
["Clarinet","Replace and seat one pad"]
["Clarinet","Playing condition: The work necessary to restore the instrument's playability and durability for at least one year of service.(Includes pads, solder work, springs, key adjustments."]
["Clarinet","Repair basic crack"]
["Clarinet","Straighten a bent key"]
["Bass Clarinet","Complete re-pad of all keys and to include: disassembly, cleaning, correcting all spring and rod problems, replace key corks, clean old glue from pad cups, repair nicked tone holes, leveling and adjusting keys, and parts."]
["Bass Clarinet","Replace and seat one pad"]
["Bass Clarinet","Playing condition: The work necessary to restore the instrument's playability and durability for at least one year of service.(Includes pads, solder work, springs, key adjustments."]
["Bass Clarinet","Repair basic crack"]
["Bass Clarinet","Straighten a bent key"]
["Bassoon","Complete re-pad of all keys and to include: disassembly, cleaning, correcting all spring and rod problems, replace key corks, clean old glue from pad cups, repair nicked tone holes, leveling and adjusting keys, and parts."]
["Bassoon","Replace and seat one pad"]
["Bassoon","Playing condition: The work necessary to restore the instrument's playability and durability for at least one year of service.(Includes pads, solder work, springs, key adjustments."]
["Bassoon","Repair basic crack"]
["Bassoon","Straighten a bent key"]
["Alto Saxophone","Complete re-pad of all keys and to include: disassembly, cleaning, correcting all spring and rod problems, replace key corks, clean old glue from pad cups, repair nicked tone holes, leveling and adjusting keys, and parts."]
["Alto Saxophone","Replace and seat one pad"]
["Alto Saxophone","Playing condition: The work necessary to restore the instrument's playability and durability for at least one year of service.(Includes pads, solder work, springs, key adjustments)"]
["Alto Saxophone","Repair basic crack"]
["Alto Saxophone","Straighten a bent key"]
["Baritone Saxophone","Complete re-pad of all keys and to include: disassembly, cleaning, correcting all spring and rod problems, replace key corks, clean old glue from pad cups, repair nicked tone holes, leveling and adjusting keys, and parts."]
["Baritone Saxophone","Replace and seat one pad"]
["Baritone Saxophone","Playing condition: The work necessary to restore the instrument's playability and durability for at least one year of service.(Includes pads, solder work, springs, key adjustments)"]
["Baritone Saxophone","Repair basic crack"]
["Baritone Saxophone","Straighten a bent key"]
[null,"Subtotals"," "," "," "," "," "]
["BAND INSTRUMENTS - PERCUSSION"]
["Snare Drum","Repair shell seams"]
["Snare Drum","Replace tension rods and lugs"]
["Bass Drum","Repair shell seams"]
["Bass Drum","Replace lugs"]
["Toms","Repair shell seams"]
["Toms","Replace tension rods and lugs"]
["Timpani","Replace tension rods "]
["Timpani","Repair tin pin pedal"]
["Timpani","Repair tin pin turning gauge"]
["Timpani","Repair spring tension adjustment screw"]
[null,"Subtotals"," "," "," "," "," "]
["ELEMENTARY INSTRUMENTS"]
["Elementary Xylophones/Metallophones","Replace tubing"]
["Elementary Xylophones/Metallophones","Straighten nails"]
["Elementary Xylophones/Metallophones","Replace a nail/rubber sleeve"]
["Elementary Xylophones/Metallophones","Eliminate buzzing (bass xylophone)"]
[null,"Subtotals"," "," "," "," "," "]
["ORCHESTRAL STRINGS INSTRUMENTS"]
["Bass","Reset neck"]
["Bass","Carve and set new bridge"]
["Bass","Bow re-hair"]
["Bass","Glasser fiberglass bow exchange"]
["Bass","Reglue fingerboard"]
["Bass","Repair crack-top, back with removal (include price per inch of the crack)"]
["Bass","Repair crack-top, back without removal (include price per inch of the crack)"]
["Bass","Reset existing sound post"]
["Bass","Re-drill tap screw (endpin assembly)"]
["Bass","Refit pegs (per peg)"]
["Cello","Reset neck"]
["Cello","Carve and set new bridge"]
["Cello","Reglue fingerboard"]
["Cello","Bow re-hair"]
["Cello","Glasser fiberglass bow exchange"]
["Cello","Reglue fingerboard"]
["Cello","Reset existing sound post"]
["Cello","Repair crack-top, back with removal (include price per inch of the crack)"]
["Cello","Repair crack-top, back without removal (include price per inch of the crack)"]
["Cello","Re-drill tap screw (endpin assembly)"]
["Cello","Refit pegs (per peg)"]
["Violin","Reset neck"]
["Violin","Carve and set new bridge"]
["Violin","Bow re-hair"]
["Violin","Glasser fiberglass bow exchange"]
["Violin","Reglue fingerboard"]
["Violin","Reset existing sound post"]
["Violin","Repair crack-top, back with removal (include price per inch of the crack)"]
["Violin","Repair crack-top, back without removal (include price per inch of the crack)"]
["Violin","Refit pegs (per peg)"]
["Viola","Reset neck"]
["Viola","Carve and set new bridge"]
["Viola","Bow re-hair"]
["Viola","Glasser fiberglass bow exchange"]
["Viola","Reglue fingerboard"]
["Viola","Reset existing sound post"]
["Viola","Repair crack-top, back with removal (include price per inch of the crack)"]
["Viola","Repair crack-top, back without removal (include price per inch of the crack)"]
["Viola","Refit pegs"]
[null,"Subtotals"," "," "," "," "," "]
["GUITARS"]
["Guitar","Remove and Replace Bridge"]
["Guitar","Reglue Bridge With Removal"]
["Guitar","Repair and cleat cracked top (per inch)"]
["Guitar","Repair and cleat cracked side (per inch)"]
["Guitar","Repair and cleat cracked back (per inch)"]
["Guitar","Reglue Nut"]
["Guitar","Replace Nut"]
["Guitar","Replace Saddle"]
["Guitar","Full Fret Dress (Level,Recrown,Polish)"]
["Guitar","Reglue Binding per inch"]
[null,"Subtotals"," "," "," "," "," "]
["ACOUSTIC PIANOS"]
["Acoustic Piano","Tuning"]
[null,"Subtotals"," "," "," "," "," "]
["ELECTRONICS"]
["Provide a brief narrative response explaining process for handling electronics repairs, including pricing for repairs and any additional fees associated with Proposer’s services."]
[]
[]
[]
[]
[]
[]
[null,"Subtotals"," "," "," "," "," "]
[]
[null,"Totals"," "," "," "," "," "]
[]
[null,"The Proposer hereby declares understanding, agreement and certification of compliance to provide the items and/or services, at the prices quoted, in accordance with all terms and conditions, requirements and specifications of the original Request for Quote (RFQ) and as modified by any addenda thereto."]
[]
["Company Name:"]
["Address:"]
["Contact:"]
["Title:"]
["Phone:"]
["Email:"]
[]
[]
[null,"Printed Name",null,"Signature of Officer",{"$nulls":3},"Date"]