{"text_format":"3","workbook":"xls","n_sheets":8,"sheets":["All Rooms","CRMS","DFES","GES","GSMS","JCHS","TWES","WES"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"All Rooms","index":0,"n_rows":27,"n_cols":10,"rows_kept":27,"flags":["formulas_cached_only"]}
["School","Room","Teacher","Ceiling Height","HDMI/VGA/Ethernet Cable Length","3.5mm Audio Cable Length","Top of panel to be at","Dry Erase Board Needs","Power for Panel","Additional Notes"]
[]
["CRMS","A-1","PEC","10'","50'+","30'+","80\"","2 - one on each side of IFP","Needed above"]
["CRMS","A-2","PEC","10'","40'+","30'+","80\"","2 - one on each side of IFP","Needed above","Center IFP on wall adjacent to existing SMART board (wall with existing dry erase board)"]
["CRMS","B-1","PEC","10'","50'+","30'+","80\"","2 - one on each side of IFP","Needed above"]
["CRMS","C-1","PEC","10'","50'+","30'+","80\"","2 - one on each side of IFP","Needed above"]
[]
["DFES","B-3","Counselor","10'","35'+","35'+",null,"none","Needed above","center on front wall. install on height adjustable stand provided by school. speaker needed."]
["DFES","B-11","PEC","10'","35'+","35'+",null,"none","Needed above","center on front wall. install on height adjustable stand provided by school."]
["DFES","B-12","PEC","10'","35'+","35'+",null,"none","Needed above","center on front wall. install on height adjustable stand provided by school."]
["DFES","Y-7","EIP","10'","35'+","35'+",null,"none","Needed above","center on front wall. install on height adjustable stand provided by school."]
["DFES","R-3","EIP","10'","35'+","35'+",null,"none","Needed above","center on front wall. install on height adjustable stand provided by school."]
[]
["GES","Red 404","PEC","10'+","35'+","40'+","72\"","none","Present above"]
["GES","Red 406","PEC","10'+","35'+","40'+","72\"","none","Present above"]
[]
["GSMS","E3","IC","10'","6'+ direct connect","30'+","80\"","none","Present below"]
[]
["JCHS"]
[]
["TWES","Yellow 602","PEC","10'","35'+","35'+","72\"","2 - one on each side of IFP","Needed above"]
[]
["WES","Red 302","PEC","10'","35'+","35'+","72\"","2 - one on each side of IFP","Present below"]
["WES","Yellow 209","EIP","10'","25'+","35'+","72\"","2 - one on each side of IFP","Present below"]
["WES","Blue 101","Vaughn","10'","35'+","35'+","72\"","2 - one on each side of IFP","Needed above"]
["WES","Blue 107","Pull out","10'","10'+ direct connect","35'+","72\"","none","Present above"]
["WES","Blue 110","EIP","10'","10'+ direct connect","35'+","72\"","none","Present above"]

{"sheet":"CRMS","index":1,"n_rows":5,"n_cols":10,"rows_kept":5,"flags":["formulas_cached_only"]}
["School","Room","Teacher","Ceiling Height","HDMI/VGA/Ethernet Cable Length","3.5mm Audio Cable Length","Top of panel to be at","Dry Erase Board Needs","Power for Panel","Additional Notes"]
["CRMS","A-1","PEC","10'","50'+","30'+","80\"","2 - one on each side of IFP","Needed above"]
["CRMS","A-2","PEC","10'","40'+","30'+","80\"","2 - one on each side of IFP","Needed above","Center IFP on wall adjacent to existing SMART board (wall with existing dry erase board)"]
["CRMS","B-1","PEC","10'","50'+","30'+","80\"","2 - one on each side of IFP","Needed above"]
["CRMS","C-1","PEC","10'","50'+","30'+","80\"","2 - one on each side of IFP","Needed above"]

{"sheet":"DFES","index":2,"n_rows":6,"n_cols":10,"rows_kept":6,"flags":["formulas_cached_only"]}
["School","Room","Teacher","Ceiling Height","HDMI/VGA/Ethernet Cable Length","3.5mm Audio Cable Length","Top of panel to be at","Dry Erase Board Needs","Power for Panel","Additional Notes"]
["DFES","B-3","Counselor","10'","35'+","35'+",null,"none","Needed above","center on front wall. install on height adjustable stand provided by school. speaker needed."]
["DFES","B-11","PEC","10'","35'+","35'+",null,"none","Needed above","center on front wall. install on height adjustable stand provided by school."]
["DFES","B-12","PEC","10'","35'+","35'+",null,"none","Needed above","center on front wall. install on height adjustable stand provided by school."]
["DFES","Y-7","EIP","10'","35'+","35'+",null,"none","Needed above","center on front wall. install on height adjustable stand provided by school."]
["DFES","R-3","EIP","10'","35'+","35'+",null,"none","Needed above","center on front wall. install on height adjustable stand provided by school."]

{"sheet":"GES","index":3,"n_rows":3,"n_cols":10,"rows_kept":3,"flags":["formulas_cached_only"]}
["School","Room","Teacher","Ceiling Height","HDMI/VGA/Ethernet Cable Length","3.5mm Audio Cable Length","Top of panel to be at","Dry Erase Board Needs","Power for Panel","Additional Notes"]
["GES","Red 404","PEC","10'+","35'+","40'+","72\"","none","Present above"]
["GES","Red 406","PEC","10'+","35'+","40'+","72\"","none","Present above"]

{"sheet":"GSMS","index":4,"n_rows":2,"n_cols":10,"rows_kept":2,"flags":["formulas_cached_only"]}
["School","Room","Teacher","Ceiling Height","HDMI/VGA/Ethernet Cable Length","3.5mm Audio Cable Length","Top of panel to be at","Dry Erase Board Needs","Power for Panel","Additional Notes"]
["GSMS","E3","IC","10'","6'+ direct connect","30'+","80\"","none","Present below"]

{"sheet":"JCHS","index":5,"n_rows":2,"n_cols":10,"rows_kept":2,"flags":["formulas_cached_only"]}
["School","Room","Teacher","Ceiling Height","HDMI/VGA/Ethernet Cable Length","3.5mm Audio Cable Length","Top of panel to be at","Dry Erase Board Needs","Power for Panel","Additional Notes"]
["JCHS"]

{"sheet":"TWES","index":6,"n_rows":2,"n_cols":10,"rows_kept":2,"flags":["formulas_cached_only"]}
["School","Room","Teacher","Ceiling Height","HDMI/VGA/Ethernet Cable Length","3.5mm Audio Cable Length","Top of panel to be at","Dry Erase Board Needs","Power for Panel","Additional Notes"]
["TWES","Yellow 602","PEC","10'","35'+","35'+","72\"","2 - one on each side of IFP","Needed above"]

{"sheet":"WES","index":7,"n_rows":6,"n_cols":10,"rows_kept":6,"flags":["formulas_cached_only"]}
["School","Room","Teacher","Ceiling Height","HDMI/VGA/Ethernet Cable Length","3.5mm Audio Cable Length","Top of panel to be at","Dry Erase Board Needs","Power for Panel","Additional Notes"]
["WES","Red 302","PEC","10'","35'+","35'+","72\"","2 - one on each side of IFP","Present below"]
["WES","Yellow 209","EIP","10'","25'+","35'+","72\"","2 - one on each side of IFP","Present below"]
["WES","Blue 101","Vaughn","10'","35'+","35'+","72\"","2 - one on each side of IFP","Needed above"]
["WES","Blue 107","Pull out","10'","10'+ direct connect","35'+","72\"","none","Present above"]
["WES","Blue 110","EIP","10'","10'+ direct connect","35'+","72\"","none","Present above"]