{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":65,"n_cols":7,"rows_kept":65,"merged":[[0,0,0,6],[1,0,1,6],[2,0,2,6],[3,0,3,6],[5,0,5,1],[6,0,6,1],[7,0,7,1],[8,0,8,1],[9,0,9,1],[10,0,10,1],[11,0,11,1],[12,0,12,1],[13,0,13,1],[14,0,14,1],[15,0,15,1],[16,0,16,1],[17,0,17,1],[18,0,18,1],[19,0,19,1],[20,0,20,1],[21,0,21,1],[22,0,22,1],[23,0,23,1],[24,0,24,1],[25,0,25,1],[26,0,26,1],[27,0,27,1],[28,0,28,1],[29,0,29,1],[30,0,30,1],[31,0,31,1],[32,0,32,1],[33,0,33,1],[34,0,34,1],[40,0,40,1],[41,0,41,1],[42,0,42,1],[43,0,43,1],[44,0,44,1],[45,0,45,1],[46,0,46,1],[47,0,47,1],[48,0,48,1],[49,0,49,1],[50,0,50,1],[51,0,51,1],[52,0,52,1],[53,0,53,1],[54,0,54,1],[55,0,55,1],[56,0,56,1],[57,0,57,1],[58,0,58,1],[59,0,59,1],[60,0,60,1],[61,0,61,1],[62,0,62,1],[63,0,63,1]],"flags":["formulas_cached_only"]}
["Lafayette High School Gym Sound System"]
["RFQ0520LHSGSSREV"]
["Exhibit A"]
[]
["Vendor:"]
[]
["Instructions: Complete all yellow fields"]
[]
["Base Package - Wireless Portable Case"]
["Equipment",null,"Comparable Subsitutions Only","Quantity","Unit Price","Extended Price","Estimated Delivery/\nShipping Timeline"]
["Portable Case"]
["Gator G-TOUR 16 U Cast - Rack Case with Casters, 16U",null,null,1,null," "]
["Lowell SVP-1 - 1RU Steel Vented Panel (flanged)",null,null,5,null," "]
["Lowell SEP-1 - 1RU Steel Blank Panel (flanged)",null,null,3,null," "]
["Lowell SEP-2 - 2RU Steel Blank Panel (flanged)",null,null,1,null," "]
["Lowell SEP-6 - 6RU Steel Blank Panel (flanged)",null,null,2,null," "]
["Lowell UDE-314 - Rack Utility Drawer, 3U",null,null,1,null," "]
["Furman M-8X2 - Power Conditioner, 8 Outlet, 15A",null,null,1,null," "]
["Custom Connection Panel - (4) XLR-F, (1) 3.5mm TRS F, (1) XLR-M, IEC Power",null,null,1,null," "]
["JBL CSM 28 - 8 Ch. Mixer",null,null,1,null," "]
["Denon DN-500CB - CD/Media/Bluetooth Player",null,null,1,null," "]
["Sennheiser EW 100 G4-835-S-A1 (507886) - Wireless Vocal Set with SKM 100 G4-S Handheld Microphone",null,null,2,null," "]
["Sennheiser SR IEM G4-A1 (508181) - Stereo Monitoring Transmitter, including (1) GA3 Rackmount Kit",null,null,1,null," "]
["Miscellaneous Case Assemble Materials and Connection Cables",null,null,1,null," "]
["Electro-Voice EV US690 - Gooseneck Dynamic Cardioid Microphone",null,null,1,null," "]
["Astatic/CAD 40-116 Shock Mount Base with Push-To-Talk or Push-To-Mute Switch, No Phantom Power Required",null,null,1,null," "]
["Switchcraft D3FBX - D Series 3 Pin XLR Female - Silver Pins / Black Finish",null,null,1,null," "]
["Pro Co MM-15 - 15' Mastermike XLRF to XLRM Microphone Cable",null,null,1,null," "]
["Installation Labor - Case Assembly and Testing",null,null,1,null," "]
["Portable Case Receiver (at existing head-end)"]
["Sennheiser EM 100 G4-A1 (507945) Rackmount True Diversity Receiver, including (1) GA3 Rack Kit, Frequency range: A1 (470-516 MHz)",null,null,1,null," "]
["Sennheiser A 1031-U (004645) - Receiving/Transmitting Antenna, Passive, Omnidirectional, BNC Connector, 3/8\" Mounting Thread",null,null,1,null," "]
["C2G 03186 - 15ft RG58 BNC Coax Cable",null,null,1,null," "]
["Miscellaneous Installation Materials",null,null,1,null," "]
["Installation Labor - Wireless Receiver and Antenna",null,null,1,null," "]
[null,null,"Base Package - Total",null,null," "]
[]
["Alternate Add-On Package - Processing Upgrade, Control and Input Panels"]
["Equipment",null,"Comparable Subsitutions Only","Quantity","Unit Price","Extended Price","Estimated Delivery/\nShipping Timeline"]
["Head-End and Control"]
["RF Venue DISTRO4 - 4-Channel RF + DC Antenna Distribution System",null,null,1,null," "]
["Attero Tech unBT2A - Bluetooth Audio Wall Plate - Single Gang Receiver",null,null,1,null," "]
["BSS BSSBLU100M - Soundweb London DSP, 12 Analog Mic/Line Input, 8 Analog Output, Signal Processor with BLU Link",null,null,1,null," "]
["Furman M-8X2 - Power Conditioner, 8 Outlet, 15A",null,null,2,null," "]
["Netgear GS108PE - ProSAFE 8-port Gigabit Plus Switch 4 x 10/100/1000 (PoE) + 4 x 10/100/1000",null,null,1,null," "]
["Lowell RPSW-MP - Switch-Momentary SPST-Rocker Switch, 1 Status LED, 1-Gang, White",null,null,1,null," "]
["BSS EC-8BV-WHT - Soundweb Contrio Controller, Ethernet Controller with 8 Buttons and Volume (White - US)",null,null,1,null," "]
["BSS EC-4B-WHT - Soundweb Contrio Controller, Ethernet Controller with 4 Buttons (White - US)",null,null,1,null," "]
["FSR 16304 (WB-PS5G) - 5 Gang Locking Wall Plate Cover with Window",null,null,1,null," "]
["FSR 94002 (WB-KEY) - Replacement Keys for WB Series Wall Boxes",null,null,2,null," "]
["5 Gang Surface Mount Box",null,null,1,null," "]
["RDL D-CIJ3 - Consumer Input Jacks - Mono",null,null,1,null," "]
["RDL D-XLR3F - XLR 3-pin Female Jack on Decora Wall Plate",null,null,2,null," "]
["3 Gang Surface Mount Box",null,null,1,null," "]
["Liberty 22-2C-PSH-WHT - White Audio and Control 22 AWG 1 Pair Shielded Plenum Reel, As Needed",null,null,1]
["Liberty 24-4P-P-L5-EN-WHT - White Category 5e U/UTP EN Series 24 AWG 4 Pair Unshielded Cable Reel, As Needed",null,null,1]
["Liberty RG58-CMP-WHT - White Microwave and Wireless RF195 RG58 Solid Dual Shield Plenum Cable Reel, 1000', As Needed",null,null,1]
["Miscellaneous Wire, Cables, Connectors and Installation Materials, As Needed",null,null,1]
["Labor - Design, Engineering and Programming",null,null,1,null," "]
["Labor - Wire Run (Control and Connection Boxes)",null,null,1,null," "]
["Labor - Head-End",null,null,1,null," "]
["Labor - Control and Connection Boxes",null,null,1,null," "]
["Labor - EQ and Commissioning",null,null,1,null," "]
["Labor - Training",null,null,1,null," "]
[null,null,"Alternate Add-On Package - Total",null,null," "]