{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet3","index":0,"n_rows":33,"n_cols":4,"rows_kept":33,"merged":[[1,0,1,3],[2,0,2,3],[3,0,3,3],[8,0,9,3],[12,0,12,2],[12,3,12,4],[13,0,16,2],[13,3,16,4],[17,1,17,2],[27,0,28,3],[32,0,33,3]],"flags":["formulas_cached_only"]}
[]
["FRANKLIN COUNTY ROAD DEPARTMENT"]
["100 Lewis Ferry Road"]
["Frankfort, KY  40601"]
[]
["Phone:  502-875-8760",null,null,"FAX:  502-875-8766"]
[]
[]
["40x60x16 Pole Barn with 12x14x60 Open Shed "]
[]
["Please bid your prices for the following:"]
[]
["Specifications:",null,null,"BID PRICE"]
["•\tConstruct a 40x60x16 Pole building with 12x14x60 Open Shed (Roof Only) across back side of building. (constructed on existing concrete foundation)\n•\tThe unit will be constructed on 6x6 treated post anchored to a concrete footer. \n•\tPost will be set on 8ft centers with structurally engineered trusses with a 4/12 roof pitch set on 4ft centers. \n•\tAll side walls and roof purlins will be set on 24\" centers. \n•\tUnit will be wrapped with single bubble insulation and covered with #1 grade metal; color matching exist building.\n•\tUnit will have two 16x14 Insulated Commercial style overhead doors with openers and two walk through doors. \n•\tWill place existing windows where the owner wants them. (Qty: 4- 65”x46”)\n•\tUnit will have 6\" gutters and down spouts installed on side walls."]
[]
[]
[]
[]
["Name of Company:"]
["Address:"]
["City, State, Zip Code:"]
["Phone #:"]
[]
["Authorized Signature:"]
["Printed Name:"]
["Title:"]
["Date:"]
["Bids should include the total for all necessary materials and labor for complete \"turn key\" install.  "]
[]
["Printed Name:"]
["Title:"]
["Date:"]
["Bids should include the total for all necessary materials and labor for complete \"turn key\" install.  "]