{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Bid Schedule 2223-33MJ"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Bid Schedule 2223-33MJ","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"merged":[[1,1,1,4],[2,1,2,4],[14,1,14,4],[16,0,16,4]],"flags":["formulas_cached_only"]}
["VIII.BIDDING SCHEDULE"]
["Name of Offeror as identified on the cover page:"]
["Authorized Signature:"]
[]
["Type","Description","Unit","Quantity","Cost per Unit","Total"]
["Asphalt Patching","Provide all labor, materials, transportation, equipment, services and supervision necessary to perform routine pavement maintenance and resurfacing that will keep the pavement as near to its original condition as possible; this includes all labor involved to perform desired outcome. Patching shall include saw cutting and removing damaged pavement, tacking edges, adding base material as needed and adding 2” hot asphalt mix.","Square Ft.",100,0,0]
["Asphalt Patching - Heavy Traffic","Provide all labor, materials, transportation, equipment, services and supervision necessary to perform routine pavement maintenance and resurfacing that will keep the pavement as near to its original condition as possible; this includes all labor involved to perform desired outcome. Patching shall include saw cutting and removing damaged pavement, tacking edges, adding base material as needed and adding 3.5” hot asphalt mix.","Square Ft.",100,0,0]
["Asphalt Milling","Provide all labor, materials, transportation, equipment, services and supervision necessary to perform asphalt milling to serve as a base for pavement that will restore the pavement as near to its original condition as possible; this includes all labor involved to perform desired outcome. ","Square Yd.",100,0,0]
["Asphalt Paving 2\"","Provide all labor, materials, transportation, equipment, services and supervision necessary to perform routine paveingresurfacing that will keep the pavement as near to its original condition as possible; this includes all labor involved to perform desired outcome. Paving shall include adding 2” hot asphalt mix.","Square Yd.",100,0,0]
["Asphalt Paving 3.5\"","Provide all labor, materials, transportation, equipment, services and supervision necessary to perform routine paveingresurfacing that will keep the pavement as near to its original condition as possible; this includes all labor involved to perform desired outcome. Paving shall include adding 3.5” hot asphalt mix.","Square Yd.",100,0,0]
["Line Striping","Provide all labor, materials, transportation, equipment, services and supervision necessary to perform LINE STRIPING as needed in adherence to specifications.","Linear Ft.",198,0,0]
["Crack Sealing","Provide all labor, materials, transportation, equipment, services and supervision necessary to perform CRACK SEALING as needed in adherence to specifications.","Linear Ft.",100,0,0]
["Asphalt Sealing","Provide all labor, materials, transportation, equipment, services and supervision necessary to perform ASPHALT SEALING as needed in adherence to specifications; price is for 2 coats. ","Square Yd.",{"v":10000,"d":"10,000"},0,0]
["Parking Bumpers","Provide all labor, materials, transportation, equipment, services and supervision necessary to perform PARKING BUMPERS as needed in adherence to specifications.","Each",10,0,0]
[null,"Calculating The Low Bid: Highlighted Colums will be used for evaluation purposes in calculating the lowest bid.",{"$nulls":3},0]
[]
["Whilte the below unit cost will not be considered in the determing the lowest bidder, it must be provided with your response to be considered and will be a part of the resulting contract. "]
[]
["Type","Description","Unit","Quantity","Cost per Unit"]
["Curb and Gutter","Provide all labor, materials, transportation, equipment, services and supervision necessary to perform CURB AND GUTTER services as needed in adherence to specifications; price is for 2 feet.","Linear Ft.",1,0]
["Concrete Sidewalk","Provide all labor, materials, transportation, equipment, services and supervision necessary to perform CONCRETE SIDEWALK services as needed in adherence to specifications; price is for 2 feet.","Each",1,0]
["Speed Bumps","Provide all labor, materials, transportation, equipment, services and supervision necessary to provide SPEED BUMPS as needed in adherence to specifications.","Linear Ft.",1,0]
["Speed Humps","Povide all labor, materials, transportation, equipment, services and supervision necessary to provide SPEED HUMPS as needed in adherence to specifications.","Linear Ft.",1,0]
["Speed Tables","Provide all labor, materials, transportation, equipment, services and supervision necessary to provide SPEED TABLES as needed in adherence to specifications.","Linear Ft.",1,0]
["Base Material","Provide all materials and transportation to provide BASE MATERIAL as requested in adherence to specifications.","Ton",1,0]
["Misc. Labor/Equipment","Miscelleanous Cost per hour","Per Hour",1,0]