{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":142,"n_cols":10,"rows_kept":142,"merged":[[1,1,1,9],[3,1,3,9],[5,1,5,9]],"flags":["formulas_cached_only"]}
[]
[null,"ERATE CLOSET UPGRADES SPECIFICATIONS:"]
[]
[null,"JCSS seeks responsible and responsive vendors who will provide and/or install new network equipment and racks/cabinets throughout the district as well as reorganize data cabling in our admin office and PreK network closets.  Contract for equipment, equipment installation, and cabling reorganization may be awarded separately.  Equipment installation vendor will be responsible for removing old equipment and delivering it to the JCSS Technology office, installing new equipment, and replacing patch cables as needed.  Patch cables of appropriate lengths and colors should be installed when the existing cables do not meet the following criteria : 1 foot cable direct from panel to switch, Local LAN (Blue), Wireless (Green) and Camera (Red).  Reorganizing data cabling will consist of relocating and consolidating multiple patch panels, re-terminating drops into new jacks and patch panels, relabeling drops at patch panel and client side, and removing unnecessary cabling and panels.  Vendor will install new patch cables of appropriate lengths and will use the following system: Local LAN (Blue), Wireless (Green) and Camera (Red)."]
[]
[null,"Please quote the following preferred models of switches and modules OR EQUAL: 48 port PoE+ switch (Aruba 3810m), 24 port PoE+ switch (Aruba 3810m), SFP+ expansion module (Aruba JL083A), SFP+ LRM transceiver (Aruba J9152D), SFP+ SM transceiver (Aruba J9151D), PoE+ power supply (Aruba JL086A#ABA), 1 meter stacking cables (Aruba J9665A), 3 meter stacking cables (Aruba J9579A), stacking modules (Aruba JL084A), cabinets (Hoffman AccessPlus Double-Hinge, Type 1), patch panels (Panduit NetKey Faceplate Modular Patch Panels), UPSs (APC SMT1000RM2UC, APCSMT2200RM2UC). Proposals for equivalent models will be considered.  We may select separate vendors for switches and cabling."]
[]
[null,"CRMS",null,"Drops",null,"Patch Cables",null,"Switches",null,"Other"]
[]
[null,"A Hall",{"$nulls":4},"l","Aruba 3810 Stack ((1) 48 port PoE+, 2 stacking modules, 1 stacking cable)",null,"Move SFP+ module from E hall stack, Move Aruba 3810m 48 port from MDF"]
[]
[null,"B Hall"]
[]
[null,"C Hall"]
[]
[null,"D Hall"]
[]
[null,"E Hall",{"$nulls":7},"Move extra SFP+ module to new switch in A Hall"]
[]
[null,"MDF",{"$nulls":5},"Aruba 3810 24 port PoE+",null,"Move 1 48 port PoE+ to A Hall"]
[]
[null,"DFES",null,"Drops",null,"Patch Cables",null,"Switches",null,"Other"]
[]
[null,"Blue Hall",{"$nulls":5},"1 SFP+ module",null,"Move Aruba 3810m 48 port from Green Hall IDF"]
[]
[null,"Green Hall",{"$nulls":5},"Aruba 3810 24 port PoE+",null,"Move Aruba 3810m 48 port to Blue Hall IDF"]
[]
[null,"MDF"]
[]
[null,"Red Hall",{"$nulls":5},"Aruba 3810 48 port PoE+, 1 SFP+ module",null,"Provide and install new 1000Va UPS."]
[]
[null,"Yellow Hall",{"$nulls":5},"Aruba 3810 48 port PoE+, 1 SFP+ module"]
[]
[null,"GES",null,"Drops",null,"Patch Cables",null,"Switches",null,"Other"]
[]
[null,"Blue Hall",{"$nulls":5},"Aruba 3810 Stack ((1) 48 port PoE+, (1) 24 port PoE+, 1 SFP+ module, 2 stacking modules, 1 stacking cable)"]
[]
[null,"Green Hall",{"$nulls":5},"Aruba 3810 Stack ((2) 48 port PoE+, 1 SFP+ module, 2 stacking modules, 1 stacking cable)"]
[]
[null,"Gym"]
[]
[null,"MDF",{"$nulls":5},"Aruba 3810 Stack ((5) 48 port PoE+, 2 SFP+ modules, 5 stacking modules, (4)1m stacking cables, (1)3m stacking cable)",null,"Provide and install (1/2) 2200Va UPS(s)."]
[]
[null,"Red Hall",{"$nulls":5},"Aruba 3810 Stack ((2) 48 port PoE+, 1 SFP+ module, 2 stacking modules, 1 stacking cable)"]
[]
[null,"Yellow Hall",{"$nulls":5},"Aruba 3810 Stack ((1) 48 port PoE+, (1) 24 port PoE+, 1 SFP+ module, 2 stacking modules, 1 stacking cable)"]
[]
[null,"GSMS",null,"Drops",null,"Patch Cables",null,"Switches",null,"Other"]
[]
[null,"B Hall",{"$nulls":5},"Aruba 3810 48 port PoE+, 1 SFP+ module"]
[]
[null,"D Hall",{"$nulls":5},"Aruba 3810 Stack ((2) 48 port PoE+, 1 SFP+ module, 2 stacking modules, 1 stacking cable)"]
[]
[null,"E Hall",{"$nulls":5},"Aruba 3810 48 port PoE+, 1 stacking module, 1 stacking cable"]
[]
[null,"MDF"]
[]
[null,"JCHS",null,"Drops",null,"Patch Cables",null,"Switches",null,"Other"]
[]
[null,"AA"]
[]
[null,"Ag",{"$nulls":5},"Aruba 3810 Stack ((2) 48 port PoE+, 1 SFP+ modules, 2 stacking modules, 1 stacking cable)"]
[]
[null,"A Hall (Math)"]
[]
[null,"B Hall (Science)",{"$nulls":5},"Aruba 3810 Stack ((2) 48 port PoE+, (1) 24 port PoE+, 1 SFP+ module, 3 stacking modules, 3 stacking cables))"]
[]
[null,"CCA Lower",{"$nulls":5},"Aruba 3810 Stack ((3) 48 port PoE+, 1 SFP+ module, 3 stacking modules, 3 stacking cables)"]
[]
[null,"CCA Upper",{"$nulls":5},"Aruba 3810 Stack ((5) 48 port PoE+, 1 SFP+ module, 5 stacking modules, (4) 1m stacking cables, (1) 3m stacking cable)"]
[]
[null,"English Wing",{"$nulls":5},"Aruba 3810 Stack ((3) 48 port PoE+, 1 SFP+ module, 3 stacking modules, 3 stacking cables)"]
[]
[null,"Field House",{"$nulls":5},"Aruba 3810  (1) 48 port PoE+, 1 SFP+ module",null,"Move 24 port PoE+ switch to G Hall IDF (including stacking module, stacking cable, SFP+ module), Move 24 port non-PoE switch to Old Field House IDF"]
[]
[null,"Old Field House",{"$nulls":7},"Provide and install new 30in+ deep/12u+ height cabinet, provide and install new 1000Va UPS, move 24 port non-PoE switch from Field House IDF."]
[]
[null,"Fine Arts"]
[]
[null,"G Hall (English)",{"$nulls":5},"Aruba 3810 (1) 48 port PoE+,  1 stacking module",null,"Move 24 port PoE switch from Field House IDF with stacking module, stacking cable, and SFP+ module"]
[]
[null,"Gym",{"$nulls":5},"Aruba 3810  (1) 48 port PoE+, 1 SFP+ module"]
[]
[null,"H Hall (Social Studies)",{"$nulls":5},"Aruba 3810  (1) 48 port PoE+, 1 SFP+ module"]
[]
[null,"MDF",{"$nulls":5},"Aruba 3810 48 port PoE+ , 1 stacking module, (1) 3m stacking cable"]
[]
[null,"ROTC"]
[]
[null,"TWES",null,"Drops",null,"Patch Cables",null,"Switches",null,"Other"]
[]
[null,"Blue Hall",{"$nulls":5},"Aruba 3810 Stack ((2) 48 port PoE+, 1 SFP+ module, 2 stacking modules, 1 stacking cable)"]
[]
[null,"Green Hall",{"$nulls":5},"Aruba 3810 Stack ((2) 48 port PoE+, 1 SFP+ module, 2 stacking modules, 1 stacking cable)"]
[]
[null,"Gym"]
[]
[null,"MDF"]
[]
[null,"Red Hall",{"$nulls":5},"Aruba 3810 Stack ((2) 48 port PoE+, 1 SFP+ module, 2 stacking modules, 1 stacking cable)"]
[]
[null,"Yellow Hall",{"$nulls":5},"Aruba 3810 Stack ((2) 48 port PoE+, 1 SFP+ module, 2 stacking modules, 1 stacking cable)"]
[]
[null,"WES",null,"Drops",null,"Patch Cables",null,"Switches",null,"Other"]
[]
[null,"600 Hall",{"$nulls":5},"Aruba 3810 Stack ((1) 48 port PoE+, (1) 24 port PoE+, 1 SFP+ module, 2 stacking modules, 1 stacking cable)"]
[]
[null,"700 Hall",{"$nulls":5},"Aruba 3810 Stack ((1) 48 port PoE+, (1) 24 port PoE+, 1 SFP+ module, 2 stacking modules, 1 stacking cable)"]
[]
[null,"Blue Hall"]
[]
[null,"Gym"]
[]
[null,"MDF"]
[]
[null,"Red Hall",{"$nulls":5},"Aruba 3810 Stack ((2) 48 port PoE+, 1 SFP+ module, 2 stacking modules, 1 stacking cable)"]
[]
[null,"Yellow Hall"]
[]
[null,"PreK",null,"Drops",null,"Patch Cables",null,"Switches",null,"Other"]
[]
[null,"MDF",null,"Reterminate into new jacks of appropriate color into new patch panels and relabel drops at panel and client side. Local LAN (blue), Wireless (green), Camera (Red)",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)",null,"Aruba 3810 Stack ((2) 48 port PoE+, 1 SFP+ module, 2 stacking modules, 1 stacking cable)",null,"Remove old fiber, provide and install new 2200VaUPS"]
[]
[null,"Transportation",null,"Reterminate into new jacks of appropriate color into new patch panels and relabel drops at panel and client side. Local LAN (blue), Wireless (green), Camera (Red)",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)",null,"Aruba 3810 48 port PoE+, 1 SFP+ module"]
[]
[null,"BOE",null,"Drops",null,"Patch Cables",null,"Switches",null,"Other"]
[]
[null,"MDF",null,"Reterminate into new jacks of appropriate color into new patch panels and relabel drops at panel and client side. Local LAN (blue), Wireless (green), Camera (Red)",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)",null,"Aruba 3810 Stack ((1) 48 port PoE+, (1) 24 port PoE+, 1 SFP+ module, 2 stacking modules, 1 stacking cable)"]
[]
[null,"AP",null,"Reterminate into new jacks of appropriate color into new patch panels and relabel drops at panel and client side. Local LAN (blue), Wireless (green), Camera (Red)",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)",null,"Aruba 3810 24 port PoE+, 1 SFP+ module"]
[]
[null,"Nutrition",null,"Reterminate into new jacks of appropriate color into new patch panels and relabel drops at panel and client side. Local LAN (blue), Wireless (green), Camera (Red)",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)",null,"Aruba 3810 24 port PoE+"]
[]
[null,"Facilities",null,"Reterminate into new jacks of appropriate color into new patch panels and relabel drops at panel and client side. Local LAN (blue), Wireless (green), Camera (Red)",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)",null,"Aruba 3810 24 port PoE+, 1 SFP+ module"]
[]
[null,"PL",null,"Reterminate into new jacks of appropriate color into new patch panels and relabel drops at panel and client side. Local LAN (blue), Wireless (green), Camera (Red)",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)",null,"Aruba 3810 24 port PoE+, 1 SFP+ module"]
[]
[null,"PEC",null,"Reterminate into new jacks of appropriate color into new patch panels and relabel drops at panel and client side. Local LAN (blue), Wireless (green), Camera (Red)",null,"New patch cables of appropriate length should be installed for all drops patched into panel.  Local LAN (blue), Wireless (green), Camera (Red)",null,"Aruba 3810 24 port PoE+, 1 SFP+ module"]
[]
[null,"Technology",null,"Drops",null,"Patch Cables",null,"Switches",null,"Other"]
[]
[null,"Data Center"]