{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":18,"n_cols":6,"rows_kept":18,"merged":[[0,0,0,5],[1,0,1,5],[2,0,2,5],[3,4,3,5],[5,0,5,5],[10,0,10,5],[17,0,17,4]]}
["INVITATION TO BID NO. 24-DES-ITBPW-304"]
["TRAFFIC CALMING DEVICES"]
["Attachment 2"]
[]
["Line Item No.","Description","Unit","Yearly Approximate Quantities","Unit Price","Extended Price"]
["Section I_Utility Patch Repair"]
[1,"Edge Milling","L.F.",{"v":1000,"d":"1,000"},null,{"$f":"SUM(D7*E7)","v":{"v":0,"d":"$0.00"}}]
[2,"VDOT 21A Aggregate Mat’l","Ton",300,null,{"$f":"SUM(D8*E8)","v":{"v":0,"d":"$0.00"}}]
[3,"Base Asphalt BM-25.0A","Ton",200,null,{"v":0,"d":"$0.00"}]
[4,"Top Asphalt SM-9.5A","Ton",150,null,{"v":0,"d":"$0.00"}]
["Section II_Traffic Calming Devices"]
[5,"Full Milling (2”)","S.F.",{"v":8500,"d":"8,500"},null,{"v":0,"d":"$0.00"}]
[6,"Provide and Install Raised Asphalt","Ton",250,null,{"v":0,"d":"$0.00"}]
[7,"Provide and Install At-Grade Asphalt","Ton",25,null,{"v":0,"d":"$0.00"}]
[8,"Provide and Install Preformed Thermoplastic Crosswalk","S.F.",{"v":2000,"d":"2,000"},null,{"v":0,"d":"$0.00"}]
[9,"Provide and Install Yellow Centerline Marking on Raise Surfaces ","L.F.",{"v":1000,"d":"1,000"},null,{"v":0,"d":"$0.00"}]
[10,"Speed Table/Cushion Thermoplastic Markings","EA.",50,null,{"v":0,"d":"$0.00"}]
["GRAND TOTAL BID PRICE:",{"$nulls":4},{"$f":"SUM(F7,F8,F9,F10,F12,F13,F14,F15,F16,F17)","v":{"v":0,"d":"$0.00"}}]