{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Bid Form"],"not_rendered":{"defined_names":2},"read":"whole","date_system":"1900"}

{"sheet":"Bid Form","index":0,"n_rows":76,"n_cols":14,"rows_kept":76,"merged":[[0,0,0,13],[1,0,1,13],[2,0,2,13],[3,0,4,0],[3,1,4,1],[3,2,3,4],[3,5,3,9],[21,3,22,3],[21,4,22,4],[21,5,22,5],[21,6,22,6],[21,7,22,7],[21,8,22,8],[21,9,22,9],[21,10,22,10],[21,11,22,11],[21,12,22,12],[21,13,22,13],[70,8,70,10],[71,8,71,10],[72,8,72,10],[73,0,73,12],[74,1,74,12],[75,1,75,12]]}
["Exhibit A"]
["Bid Form"]
["Front St. Underground (UG) Infrastructure Upgrade T3 - Project #1927 Materials RFB \n"]
["Item No. ","Equipment Description ","Specified",null,null,"Quoted",{"$nulls":6},"Total"]
[null,null,"Quantity","Manufacturer","Part Number","Manufacturer","Part Number","Quantity ",null,"Unit Price","Unit",null,"Cost ","Lead Time"]
[1,"Three Phase Junction Cabinet, 25 kV, 600 A, 30\"x67\"x23\", Four Parking Stands, Three Back Plates",1,"APS","APS306723-ACACACA",{"$nulls":3},"x",null,"EA","=",{"$f":"H6*J6","v":{"v":0,"d":"$0.00"}}]
[2,"Polymer Concrete Junction Box, Square Enclosure, 48\"x48\"x48\", Tier 15, Flush mount",2,"Oldcastle",4848,{"$nulls":3},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[3,"Secondary Pedestal, Above Grade, With Penta Bolt and Hasp, 15\" x 15\" x 30\"",1,"Nordic","PSP-151530",{"$nulls":3},"x",null,"EA","=",{"$f":"H8*J8","v":{"v":0,"d":"$0.00"}}]
[4,"15 kV, 200 A Loadbreak Junction, with U-straps, 4 Interfaces",3,"Eaton","LJ215C4U",{"$nulls":3},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[5,"15 kV, 200 A Loadbreak Elbow",19,"Elastimold","161LR-BS240",{"$nulls":3},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[6,"15 kV, 200 A Insulated Shielded Elbow Surge Arrester, 12.7 kV RMS MCOV",4,"Elastimold","167ESA-15",{"$nulls":3},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[7,"15 kV Cable Splice",7,"3M","5411-C1-1/0",{"$nulls":3},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[8,"Flood-Seal Multi-port Bus Connectors, 6 outlets, with rubber insulating sleeve covers",22,"Homac","175 Series\nFXL33-175\nFS1175",{"$nulls":3},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[9,"Flood-Seal Dual Adapter Kit",16,"Homac","175 Series\nFS175DPK",{"$nulls":3},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[10,"Flood-Seal Multi-port Bus Connectors, 3 outlets, Y type, with rubber insulating sleeve covers",9,"Homac","125 Series\nFSY125-21\nCS2011",{"$nulls":3},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[11,"Flood-Seal Multi-port Bus Connectors, 2-bolt, 6 outlets, with rubber insulating sleeve covers",11,"Homac","125 Series\nFSN 6-125-AWR\nCS2011",{"$nulls":3},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[12,"Flood-Seal Multi-port Bus Connectors, 2-bolt, 4 outlets, with rubber insulating sleeve covers",0,"Homac","125 Series\nFSN 4-125-AWR\nCS2011",{"$nulls":3},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[13,"Flood-Seal Multi-port Bus Connectors, 1&2-bolt, 4 outlets",4,"Homac","125 Series\nFS 31-125-AWR",{"$nulls":3},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[14,"Flood-Seal Sealing Sleeve, 2-bolt",4,"Homac","WL 2 P",{"$nulls":3},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[15,"Flood-Seal Sealing Sleeve, 1-bolt",8,"Homac","WS 2 P",{"$nulls":3},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[16,"Flood-Seal Sealing Sleeve, Small Conductor Adapter, #12 & #10",8,"Homac","SC",{"$nulls":3},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[17,"Manhole Wall Support, 316 stainless steel slotted channel, 72\" long, 13/16\" x 1-5/8\", 12 GA (one 10' piece, field cut to length)",7,"Unistrut","P3300T-10ST",{"$nulls":3},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[18,"Pull Box Wall Support, 316 stainless steel slotted channel, 48\" long, 13/16\" x 1-5/8\", 12 GA (leftover from above cut)",0]
[19,"Cable Support Bracket, 316 stainless steel slotted channel, 18\" long, 1-5/8\"x1-5/8\", 12 GA",60,"Unistrut","P2946-ST",{"$nulls":3},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[20,"Cable Clamp, 1-7/8\", polymer, with 316 stainless steel strap",205,"Unistrut","030N034",{"$nulls":3},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[21,"600 V Terminal Lug, 500 kcmil AL, 2-hole NEMA",97,"Blackburn","AL500-NTN",{"$nulls":3},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[22,"600 V Terminal Lug, 350 kcmil AL, 2-hole NEMA",33,"Blackburn","AL350-NTN",{"$nulls":3},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[23,"600 V Terminal Lug, # 4/0 AWG AL, 2-hole NEMA",9,"Blackburn","AL4/0-NTN",{"$nulls":3},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[24,"600 V Terminal Lug, # 2/0 AWG AL, 2-hole NEMA",14,"Blackburn","AL2/0-NTN",{"$nulls":3},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[25,"600 V Terminal Lug, # 1/0 AWG AL, 2-hole NEMA",0,"Blackburn","AL1/0-NTN",{"$nulls":3},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[26,"600 V Terminal Lug, # 10 AWG AL, 2-hole NEMA",8,{"$nulls":5},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[27,"600 V Terminal Lug, # 12 AWG AL, 2-hole NEMA",4,{"$nulls":5},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[28,"600 V Terminal Lug, 500 kcmil AL, 1-hole NEMA",3,"Blackburn","AL500-48",{"$nulls":3},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[29,"600 V Terminal Lug, 350 kcmil AL, 1-hole NEMA",2,"Blackburn","AL350-48",{"$nulls":3},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[30,"600 V Terminal Lug, # 4/0 AWG AL, 1-hole NEMA",3,"Blackburn","AL4/0-48",{"$nulls":3},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[31,"600 V Terminal Lug, # 2/0 AWG AL, 1-hole NEMA",7,"Blackburn","AL2/0-48",{"$nulls":3},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[32,"600 V Terminal Lug, # 1/0 AWG AL, 1-hole NEMA",0,"Blackburn","AL1/0-48",{"$nulls":3},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[33,"600 V Terminal Lug, # 10 AWG AL, 1-hole NEMA",12,"Burndy","YA10A-TN",{"$nulls":3},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[34,"600 V Terminal Lug, # 12 AWG AL, 1-hole NEMA",7,"Burndy","YA12A-TN",{"$nulls":3},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[35,"4-hole NEMA Stud Connectors (ea) for xfmr sized 10-75 kVA",3,"Homac","2042-1",{"$nulls":3},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[36,"4-hole NEMA Stud Connectors (ea) for xfmr sized 100-167 kVA",7,"Homac","2042-2",{"$nulls":3},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[37,"15 kV URD Cable No. 1/0 AWG AL, EPR (ft)",1650,{"$nulls":5},"x",null,"FT","=",{"v":0,"d":"$0.00"}]
[38,"600 V, Single Conductor Secondary UD Cable 500 kcmil AL, Color Coded Yellow",3500,{"$nulls":5},"x",null,"FT","=",{"v":0,"d":"$0.00"}]
[39,"600 V, Single Conductor Secondary UD Cable 500 kcmil AL, Color Coded Blue",1500,{"$nulls":5},"x",null,"FT","=",{"v":0,"d":"$0.00"}]
[40,"600 V, Single Conductor Secondary UD Cable 500 kcmil AL, Color Coded Black",1500,{"$nulls":5},"x",null,"FT","=",{"v":0,"d":"$0.00"}]
[41,"600 V, Single Conductor Secondary UD Cable 500 kcmil AL, Color Coded Red",1500,{"$nulls":5},"x",null,"FT","=",{"v":0,"d":"$0.00"}]
[42,"600 V, Single Conductor Secondary UD Cable 350 kcmil AL, Color Coded White",2350,{"$nulls":5},"x",null,"FT","=",{"v":0,"d":"$0.00"}]
[43,"600 V, Triplex Secondary UD Cable, 500-350 kcmil AL",100,{"$nulls":5},"x",null,"FT","=",{"v":0,"d":"$0.00"}]
[44,"600 V, Triplex Secondary UD Cable, 4/0-2/0 AWG AL",100,{"$nulls":5},"x",null,"FT","=",{"v":0,"d":"$0.00"}]
[45,"600 V, Quadruplex Secondary UD Cable, 4/0-2/0 AWG AL",165,{"$nulls":5},"x",null,"FT","=",{"v":0,"d":"$0.00"}]
[46,"600 V, Single Conductor Secondary UD Cable, #10 AWG AL",400,{"$nulls":5},"x",null,"FT","=",{"v":0,"d":"$0.00"}]
[47,"600 V, Single Conductor Secondary UD Cable, #12 AWG CU",200,{"$nulls":5},"x",null,"FT","=",{"v":0,"d":"$0.00"}]
[48,"600 V, Single Conductor Secondary UD Cable, #2/0 AWG CU",200,{"$nulls":5},"x",null,"FT","=",{"v":0,"d":"$0.00"}]
[49,"#4 AWG Bare Copper, Soft Drawn",90,{"$nulls":5},"x",null,"FT","=",{"v":0,"d":"$0.00"}]
[50,"#2/0 AWG Bare Copper, Soft Drawn",80,{"$nulls":5},"x",null,"FT","=",{"v":0,"d":"$0.00"}]
[51,"5/8\" Copper Ground Rod, 10' long",7,{"$nulls":5},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[52,"Grounding lug, tin-plated copper, for Unistrut Channel",16,"Erico","BCR8T",{"$nulls":3},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[53,"Transformer grounding lug",16,"Erico","TGC2/0",{"$nulls":3},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[54,"Ground Rod Clamp, 5/8\"",10,"Burndy","GCRT1/0",{"$nulls":3},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[55,"Cadweld Handle Clamp for use with C, E, Q and R molds",1,"Erico","CDWL160",{"$nulls":3},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[56,"Ignitor Controller Unit, 6 ft",1,"Erico","PLUSCU",{"$nulls":3},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[57,"Horizontal thru parallel cable mold, #2/0 AWG to #2/0 AWG",1,"Cadweld","PTC2G2G",{"$nulls":3},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[58,"#115 Weld Metal Cartridge",2,"Cadweld","115PLUSF20",{"$nulls":3},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[59,"#2/0 Stranded to Copper Rod Horizontal Through Top mold",1,"Cadweld","GTC-162G",{"$nulls":3},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[60,"Fireproofing tape (20' lengths)",22,"Scotch","77B3X20FT",{"$nulls":3},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[61,"Bolt, 316 stainless steel, 3/8\" x 1-1/4\", Hex head cap screw",150,{"$nulls":5},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[62,"Redhead Trubol, 3/8\" x 3-3/4\", 316 stainless steel",40,{"$nulls":5},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[63,"Channel Washer, 1/2\" ID x 1-1/4\" OD flat washer, stainless steel",40,{"$nulls":5},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[64,"Hex nut, 3/8\" x 1-1/4\", 316 stainless steel",40,{"$nulls":5},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[65,"Channel Nut w/ Regular Spring, for 3/8\" hex head screw and 1-5/8\" channel, 1/2\"-13, 316 stainless steel",150,{"$nulls":5},"x",null,"EA","=",{"v":0,"d":"$0.00"}]
[{"$nulls":8},"SUBTOTAL:"]
[{"$nulls":8},"FREIGHT:"]
[{"$nulls":8},"TOTAL BID AMOUNT:"]
[]
[null,"The above prices include all mobilization, labor, material, and equipment, overhead, profit, taxes, insurance, permit fees, etc. to complete the work."]
[null,"The City of Georgetown reserves the right to add or reduce the scope of work and material quantities as the budget and schedule allows. \n"]