{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Unit_Price_Tab"],"not_rendered":{"external_links":3,"defined_names":8},"read":"whole","date_system":"1900"}

{"sheet":"Unit_Price_Tab","index":0,"n_rows":45,"n_cols":6,"rows_kept":45,"merged":[[1,0,1,5]]}
[]
["THE UNDERSIGNED CERTIFIES THAT (CONTRACTOR NAME)___________________________\nIS CURRENTLY REGISTERED WITH THE VIRGINIA STATE BOARD OF CONTRACTORS AS REQUIRED BY THE CODE OF VIRGINIA.  CERTIFICATE NUMBER _________________ WAS ISSUED ON THE ________DAY OF _____________, 20XX.  THE UNDERSIGNED FURTHER CERTIFIES THAT THE REGISTRATION FEE AND ALL RENEWAL FEES REQUIRED UNDER LAW HAVE BEEN PAID.  THE CONTRACTOR AGREES TO FURNISH ALL NECESSARY LABOR, EQUIPMENT, MATERIALS, AND ALL THINGS NECESSARY TO PERFORM THE WORK AS SET FORTH IN ACCORDANCE WITH THE PLANS AND SPECIFICATIONS. THE CONTRACTOR AGREES TO PERFORM RELATED WORK FOR THE FOLLOWING ITEMS AT THE FOLLOWING STIPULATED PRICES: (ALL PRICES INCLUDE PROVISION AND INSTALLATION)."]
[]
[]
["C2","CONCRETE WORK"]
["MASTER ITEM #","DESCRIPTION","QTY","UNIT","UNIT PRICE","TOTAL"]
["03100-C2-SP003","Concrete Class T3 (VDOT Item 69036)",160,"CY"]
[{"$nulls":4},"SUBTOTAL"]
[]
["C11","LANDSCAPE AND HARDSCAPE RESTORATION WORK"]
["MASTER ITEM #","DESCRIPTION","QTY","UNIT","UNIT\nPRICE","TOTAL"]
["02801-C11-00050","Seed, Mixture of 85% Tall Fescue/Bluegrass and 15% Annual Rye",1100,"SY"]
["02800-C11-00500","Tree/Stump Removal - Class A. Remove and Dispose, Up to 6\" DBH to 12\" DBH (Diameter at Breast Height)",25,"EA"]
["02800-C11-00501","Tree/Stump Removal - Class B. Remove and Dispose, over 12\" DBH to 18\" DBH (Diameter at Breast Height)",5,"EA"]
["02800-C11-00502","Tree/Stump Removal - Class C. Remove and Dispose, over 18\" DBH to 24\" DBH (Diameter at Breast Height)",6,"EA"]
["02800-C11-00503","Tree/Stump Removal - Class D. Remove and Dispose, over 24\" DBH to 30\" DBH (Diameter at Breast Height)",1,"EA"]
["03100-C11-SP002","Furnish and Install Complete Concrete Retaining wall including but not limited to excavation (all depths), aggregate material, porous backfill, geotextile fabric, drain pipes, water stop, and weep holes as per details showns on sheet 007",130,"CY"]
["02800-C11-SP004","Architectural Treatment (VDOT Item 65004) (Per detail on sheet 007 or approved equal)",120,"SY"]
["02800-C11-SP005","HR-1 Type II Pedestrian Railing (VDOT Item 25003)",190,"LF"]
[{"$nulls":4},"SUBTOTAL"]
[]
["C13","EROSION AND SEDIMENT CONTROL WORK"]
["MASTER ITEM #","DESCRIPTION","QTY","UNIT","UNIT\nPRICE","TOTAL"]
["01500-C13-10000","Temporary Erosion and Sediment Controls",1,"LS"]
[{"$nulls":4},"SUBTOTAL"]
[]
[]
["C19","RETAINING WALL"]
["MASTER ITEM #","DESCRIPTION","QTY","UNIT","UNIT\nPRICE","TOTAL"]
["XXXXX-C19-XXXXX","Furnish and Install Complete Concrete Retaining wall including but not limited to aggregate material, porous backfill, geotextile fabric, drain pipes, water stop, and weep holes as per details showns on sheet 007",130,"CY"]
[]
["XXXXX-C19-XXXXX","Architectural Treatment (VDOT Item 65004) (Per detail on sheet 007 or approved equal)",120,"SY"]
["XXXXX-C19-XXXXX","HR-1 Type II Pedestrian Railing (VDOT Item 25003)",190,"LF"]
[{"$nulls":4},"SUBTOTAL"]
[]
[{"$nulls":4}," CONTRACT TOTAL (EXCLUDING PERCENTAGE ITEMS)"]
[]
["PCT",{"$f":"VLOOKUP(A38,[3]!Table_BidItem_CategoryClassification[#All],2,FALSE)","v":{"$error":"#REF!"}}]
["MASTER ITEM #","DESCRIPTION","QTY","UNIT","UNIT\nPRICE","TOTAL"]
["01000-C16-00010","Maintenance of Traffic (MOT)","NA","%"]
["01000-C16-00030","Mobilization and De-Mobilization","NA","%"]
["01500-SA-00200","SWPPP Administration","NA","%"]
[{"$nulls":4},"PERCENTAGE LINE ITEMS SUBTOTAL"]
[]
[{"$nulls":4},"PROJECT TOTAL :"]